(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)

  (general
    (links 0)
    (no_connects 0)
    (area 97.042741 84.924999 167.820859 140.075001)
    (thickness 1.6)
    (drawings 4)
    (tracks 304)
    (zones 0)
    (modules 120)
    (nets 1)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959FC8)
    (at 127.4496 90.5342)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959FBD)
    (at 127.4496 96.5342)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959FB2)
    (at 127.4496 93.5342)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959FA7)
    (at 113.8936 93.7882)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer B.Cu) (tedit 574D9791) (tstamp 59959F86)
    (at 120.6246 100.2792)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference REF** (at 0 5.375) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value SOIC-14_3.9x8.7mm_Pitch1.27mm (at 0 -5.375) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.95 4.35) (end 1.95 4.35) (layer B.Fab) (width 0.15))
    (fp_line (start 1.95 4.35) (end 1.95 -4.35) (layer B.Fab) (width 0.15))
    (fp_line (start 1.95 -4.35) (end -1.95 -4.35) (layer B.Fab) (width 0.15))
    (fp_line (start -1.95 -4.35) (end -1.95 3.35) (layer B.Fab) (width 0.15))
    (fp_line (start -1.95 3.35) (end -0.95 4.35) (layer B.Fab) (width 0.15))
    (fp_line (start -3.7 4.65) (end -3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.7 4.65) (end 3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.7 4.65) (end 3.7 4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end 3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.075 4.45) (end -2.075 4.425) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.075 4.45) (end 2.075 4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.075 -4.45) (end 2.075 -4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end -2.075 -4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end 2.075 4.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end 2.075 -4.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 4.425) (end -3.45 4.425) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959F7B)
    (at 113.8936 90.7882)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959F70)
    (at 151.1986 90.4072)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959F65)
    (at 137.6426 96.6612)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959F5A)
    (at 137.6426 93.6612)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer B.Cu) (tedit 574D9791) (tstamp 59959F39)
    (at 144.3736 100.1522)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference REF** (at 0 5.375) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value SOIC-14_3.9x8.7mm_Pitch1.27mm (at 0 -5.375) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.95 4.35) (end 1.95 4.35) (layer B.Fab) (width 0.15))
    (fp_line (start 1.95 4.35) (end 1.95 -4.35) (layer B.Fab) (width 0.15))
    (fp_line (start 1.95 -4.35) (end -1.95 -4.35) (layer B.Fab) (width 0.15))
    (fp_line (start -1.95 -4.35) (end -1.95 3.35) (layer B.Fab) (width 0.15))
    (fp_line (start -1.95 3.35) (end -0.95 4.35) (layer B.Fab) (width 0.15))
    (fp_line (start -3.7 4.65) (end -3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.7 4.65) (end 3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.7 4.65) (end 3.7 4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end 3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.075 4.45) (end -2.075 4.425) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.075 4.45) (end 2.075 4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.075 -4.45) (end 2.075 -4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end -2.075 -4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end 2.075 4.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end 2.075 -4.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 4.425) (end -3.45 4.425) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959F2E)
    (at 151.1986 93.4072)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959F23)
    (at 137.6426 90.6612)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959F18)
    (at 113.8936 108.7882)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959F0D)
    (at 113.8936 102.7882)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959F02)
    (at 113.8936 105.7882)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959EF7)
    (at 113.8936 96.7882)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959EEC)
    (at 113.8936 99.7882)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959EE1)
    (at 151.1986 108.4072)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959ED6)
    (at 151.1986 105.4072)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959ECB)
    (at 151.1986 102.4072)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959EC0)
    (at 151.1986 96.4072)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959EB5)
    (at 151.1986 99.4072)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959EAA)
    (at 137.6426 105.6612)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E9F)
    (at 127.4496 102.5342)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E94)
    (at 127.4496 108.5342)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E89)
    (at 137.6426 108.6612)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E7E)
    (at 137.6426 99.6612)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E73)
    (at 127.4496 105.5342)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E68)
    (at 137.6426 102.6612)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E5D)
    (at 127.4496 99.5342)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer B.Cu) (tedit 574D9791) (tstamp 59959E3C)
    (at 143.8656 124.4092)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference REF** (at 0 5.375) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value SOIC-14_3.9x8.7mm_Pitch1.27mm (at 0 -5.375) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.95 4.35) (end 1.95 4.35) (layer B.Fab) (width 0.15))
    (fp_line (start 1.95 4.35) (end 1.95 -4.35) (layer B.Fab) (width 0.15))
    (fp_line (start 1.95 -4.35) (end -1.95 -4.35) (layer B.Fab) (width 0.15))
    (fp_line (start -1.95 -4.35) (end -1.95 3.35) (layer B.Fab) (width 0.15))
    (fp_line (start -1.95 3.35) (end -0.95 4.35) (layer B.Fab) (width 0.15))
    (fp_line (start -3.7 4.65) (end -3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.7 4.65) (end 3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.7 4.65) (end 3.7 4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end 3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.075 4.45) (end -2.075 4.425) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.075 4.45) (end 2.075 4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.075 -4.45) (end 2.075 -4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end -2.075 -4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end 2.075 4.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end 2.075 -4.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 4.425) (end -3.45 4.425) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E31)
    (at 137.1346 126.9182)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E26)
    (at 137.1346 117.9182)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E1B)
    (at 137.1346 114.9182)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E10)
    (at 137.1346 120.9182)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959E05)
    (at 137.1346 123.9182)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959DFA)
    (at 137.1346 129.9182)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959DEF)
    (at 137.1346 132.9182)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959DE4)
    (at 126.9416 118.0452)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959DD9)
    (at 126.9416 121.0452)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959DCE)
    (at 126.9416 124.0452)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959DC3)
    (at 126.9416 130.0452)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959DB8)
    (at 126.9416 115.0452)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959DAD)
    (at 126.9416 133.0452)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959DA2)
    (at 126.9416 127.0452)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer B.Cu) (tedit 574D9791) (tstamp 59959D81)
    (at 120.1166 124.7902)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference REF** (at 0 5.375) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value SOIC-14_3.9x8.7mm_Pitch1.27mm (at 0 -5.375) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.95 4.35) (end 1.95 4.35) (layer B.Fab) (width 0.15))
    (fp_line (start 1.95 4.35) (end 1.95 -4.35) (layer B.Fab) (width 0.15))
    (fp_line (start 1.95 -4.35) (end -1.95 -4.35) (layer B.Fab) (width 0.15))
    (fp_line (start -1.95 -4.35) (end -1.95 3.35) (layer B.Fab) (width 0.15))
    (fp_line (start -1.95 3.35) (end -0.95 4.35) (layer B.Fab) (width 0.15))
    (fp_line (start -3.7 4.65) (end -3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.7 4.65) (end 3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.7 4.65) (end 3.7 4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end 3.7 -4.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.075 4.45) (end -2.075 4.425) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.075 4.45) (end 2.075 4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.075 -4.45) (end 2.075 -4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end -2.075 -4.335) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end 2.075 4.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end 2.075 -4.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.075 4.425) (end -3.45 4.425) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D76)
    (at 113.3856 130.2992)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D6B)
    (at 113.3856 124.2992)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D60)
    (at 113.3856 121.2992)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D55)
    (at 113.3856 115.2992)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D4A)
    (at 113.3856 133.2992)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D3F)
    (at 113.3856 118.2992)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D34)
    (at 113.3856 127.2992)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D29)
    (at 150.6906 129.6642)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D1E)
    (at 150.6906 120.6642)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D13)
    (at 150.6906 114.6642)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959D08)
    (at 150.6906 123.6642)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959CFD)
    (at 150.6906 132.6642)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959CF2)
    (at 150.6906 117.6642)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer B.Cu) (tedit 56E5DE14) (tstamp 59959CE7)
    (at 150.6906 126.6642)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0.25) (end 0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end 0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end -0.75 -0.25) (layer B.Fab) (width 0.15))
    (fp_line (start -0.75 -0.25) (end -0.75 0.25) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer B.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer B.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 574D9791) (tstamp 599598A6)
    (at 120.904 123.19)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference REF** (at 0 -5.375) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SOIC-14_3.9x8.7mm_Pitch1.27mm (at 0 5.375) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -4.35) (end 1.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 -4.35) (end 1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 4.35) (end -1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 4.35) (end -1.95 -3.35) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 -3.35) (end -0.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -3.7 -4.65) (end -3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end 3.7 -4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -4.45) (end -2.075 -4.425) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -4.45) (end 2.075 -4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 4.45) (end 2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end -2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end 2.075 -4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end 2.075 4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.425) (end -3.45 -4.425) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995989B)
    (at 127.729 129.935)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959890)
    (at 127.729 126.935)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959885)
    (at 127.729 120.935)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995987A)
    (at 127.729 132.935)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995986F)
    (at 114.173 132.681)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959864)
    (at 127.729 123.935)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959859)
    (at 114.173 126.681)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995984E)
    (at 114.173 129.681)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959843)
    (at 114.173 123.681)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959838)
    (at 114.173 120.681)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995982D)
    (at 114.173 114.681)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959822)
    (at 114.173 117.681)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959817)
    (at 127.729 117.935)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995980C)
    (at 127.729 114.935)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 574D9791) (tstamp 599597C5)
    (at 144.653 123.317)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference REF** (at 0 -5.375) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SOIC-14_3.9x8.7mm_Pitch1.27mm (at 0 5.375) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -4.35) (end 1.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 -4.35) (end 1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 4.35) (end -1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 4.35) (end -1.95 -3.35) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 -3.35) (end -0.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -3.7 -4.65) (end -3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end 3.7 -4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -4.45) (end -2.075 -4.425) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -4.45) (end 2.075 -4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 4.45) (end 2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end -2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end 2.075 -4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end 2.075 4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.425) (end -3.45 -4.425) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599597BA)
    (at 151.478 130.062)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599597AF)
    (at 151.478 127.062)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599597A4)
    (at 151.478 121.062)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959799)
    (at 151.478 133.062)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995978E)
    (at 137.922 132.808)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959783)
    (at 151.478 124.062)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959778)
    (at 137.922 126.808)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995976D)
    (at 137.922 129.808)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959762)
    (at 137.922 123.808)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959757)
    (at 137.922 120.808)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995974C)
    (at 137.922 114.808)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959741)
    (at 137.922 117.808)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959736)
    (at 151.478 118.062)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995972B)
    (at 151.478 115.062)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 574D9791) (tstamp 599596E4)
    (at 144.145 99.06)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference REF** (at 0 -5.375) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SOIC-14_3.9x8.7mm_Pitch1.27mm (at 0 5.375) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -4.35) (end 1.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 -4.35) (end 1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 4.35) (end -1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 4.35) (end -1.95 -3.35) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 -3.35) (end -0.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -3.7 -4.65) (end -3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end 3.7 -4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -4.45) (end -2.075 -4.425) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -4.45) (end 2.075 -4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 4.45) (end 2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end -2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end 2.075 -4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end 2.075 4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.425) (end -3.45 -4.425) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599596D9)
    (at 150.97 105.805)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599596CE)
    (at 150.97 102.805)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599596C3)
    (at 150.97 96.805)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599596B8)
    (at 150.97 108.805)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599596AD)
    (at 137.414 108.551)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599596A2)
    (at 150.97 99.805)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959697)
    (at 137.414 102.551)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995968C)
    (at 137.414 105.551)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959681)
    (at 137.414 99.551)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959676)
    (at 137.414 96.551)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995966B)
    (at 137.414 90.551)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959660)
    (at 137.414 93.551)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959655)
    (at 150.97 93.805)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995964A)
    (at 150.97 90.805)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599595A4)
    (at 127.221 108.424)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959599)
    (at 113.665 108.17)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995958E)
    (at 127.221 105.424)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959583)
    (at 113.665 105.17)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959578)
    (at 127.221 102.424)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995956D)
    (at 113.665 102.17)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959562)
    (at 127.221 99.424)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959557)
    (at 113.665 99.17)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995954C)
    (at 127.221 96.424)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959541)
    (at 113.665 96.17)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959536)
    (at 127.221 93.424)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 5995952B)
    (at 113.665 93.17)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 59959520)
    (at 127.221 90.424)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 574D9791) (tstamp 598B74F6)
    (at 120.396 98.679)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference REF** (at 0 -5.375) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SOIC-14_3.9x8.7mm_Pitch1.27mm (at 0 5.375) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -4.35) (end 1.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 -4.35) (end 1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 4.35) (end -1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 4.35) (end -1.95 -3.35) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 -3.35) (end -0.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -3.7 -4.65) (end -3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end 3.7 -4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -4.45) (end -2.075 -4.425) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -4.45) (end 2.075 -4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 4.45) (end 2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end -2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end 2.075 -4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end 2.075 4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.425) (end -3.45 -4.425) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Measurement_Points:Test_Point_Keystone_5000-5004_Miniature (layer F.Cu) (tedit 56E5DE14) (tstamp 599594EE)
    (at 113.665 90.17)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Test_Point_Keystone_5000-5004_Miniature (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 -0.25) (end 0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 -0.25) (end 0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start 0.75 0.25) (end -0.75 0.25) (layer F.Fab) (width 0.15))
    (fp_line (start -0.75 0.25) (end -0.75 -0.25) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.15))
    (fp_circle (center 0 0) (end 1.4 0) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )

  (gr_line (start 110 140) (end 110 85) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155 140) (end 110 140) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155 85) (end 155 140) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110 85) (end 155 85) (layer Edge.Cuts) (width 0.15))

  (segment (start 124.1976 120.7892) (end 126.9416 118.0452) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CE6))
  (segment (start 124.1976 121.8692) (end 124.1976 120.7892) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CE5))
  (segment (start 122.8166 119.1702) (end 126.9416 115.0452) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CE4))
  (segment (start 122.8166 120.9802) (end 122.8166 119.1702) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CE3))
  (segment (start 123.8166 122.2502) (end 124.1976 121.8692) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CE2))
  (segment (start 117.4166 119.3302) (end 113.3856 115.2992) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CE1))
  (segment (start 114.4806 122.3942) (end 113.3856 121.2992) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CE0))
  (segment (start 115.2906 121.1242) (end 115.2906 120.2042) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CDF))
  (segment (start 117.4166 120.9802) (end 117.4166 119.3302) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CDE))
  (segment (start 117.4166 122.2502) (end 116.4166 122.2502) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CDD))
  (segment (start 116.4166 122.2502) (end 115.2906 121.1242) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CDC))
  (segment (start 115.2906 120.2042) (end 113.3856 118.2992) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CDB))
  (segment (start 116.4166 127.3302) (end 115.6546 128.0922) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CDA))
  (segment (start 117.4166 126.0602) (end 116.4166 126.0602) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD9))
  (segment (start 116.4166 126.0602) (end 115.1776 127.2992) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD8))
  (segment (start 115.6546 128.0922) (end 115.5926 128.0922) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD7))
  (segment (start 117.4166 127.3302) (end 116.4166 127.3302) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD6))
  (segment (start 117.4166 129.2682) (end 113.3856 133.2992) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD5))
  (segment (start 115.1776 127.2992) (end 113.3856 127.2992) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD4))
  (segment (start 115.5926 128.0922) (end 113.3856 130.2992) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD3))
  (segment (start 117.4166 128.6002) (end 117.4166 129.2682) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD2))
  (segment (start 124.2266 127.3302) (end 126.9416 130.0452) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD1))
  (segment (start 122.8166 127.3302) (end 124.2266 127.3302) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CD0))
  (segment (start 122.8166 126.0602) (end 125.9566 126.0602) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CCF))
  (segment (start 122.8166 129.1502) (end 126.7116 133.0452) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CCE))
  (segment (start 126.7116 133.0452) (end 126.9416 133.0452) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CCD))
  (segment (start 125.9566 126.0602) (end 126.9416 127.0452) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CCC))
  (segment (start 122.8166 128.6002) (end 122.8166 129.1502) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CCB))
  (segment (start 122.8166 122.2502) (end 123.8166 122.2502) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CCA))
  (segment (start 126.1966 124.7902) (end 126.9416 124.0452) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC9))
  (segment (start 122.8166 124.7902) (end 126.1966 124.7902) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC8))
  (segment (start 124.4666 123.5202) (end 126.9416 121.0452) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC7))
  (segment (start 122.8166 123.5202) (end 124.4666 123.5202) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC6))
  (segment (start 116.4166 123.5202) (end 115.2906 122.3942) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC5))
  (segment (start 115.2906 122.3942) (end 114.4806 122.3942) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC4))
  (segment (start 117.4166 124.7902) (end 113.8766 124.7902) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC3))
  (segment (start 113.8766 124.7902) (end 113.3856 124.2992) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC2))
  (segment (start 117.4166 123.5202) (end 116.4166 123.5202) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC1))
  (segment (start 141.6736 104.6302) (end 137.6426 108.6612) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CC0))
  (segment (start 139.4346 102.6612) (end 137.6426 102.6612) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CBF))
  (segment (start 139.8496 103.4542) (end 137.6426 105.6612) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CBE))
  (segment (start 141.6736 103.9622) (end 141.6736 104.6302) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CBD))
  (segment (start 147.0736 94.5322) (end 151.1986 90.4072) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CBC))
  (segment (start 147.0736 96.3422) (end 147.0736 94.5322) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CBB))
  (segment (start 148.4546 96.1512) (end 151.1986 93.4072) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CBA))
  (segment (start 148.4546 97.2312) (end 148.4546 96.1512) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB9))
  (segment (start 148.0736 97.6122) (end 148.4546 97.2312) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB8))
  (segment (start 138.1336 100.1522) (end 137.6426 99.6612) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB7))
  (segment (start 139.5476 97.7562) (end 138.7376 97.7562) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB6))
  (segment (start 140.6736 98.8822) (end 139.5476 97.7562) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB5))
  (segment (start 141.6736 98.8822) (end 140.6736 98.8822) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB4))
  (segment (start 141.6736 100.1522) (end 138.1336 100.1522) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB3))
  (segment (start 147.0736 98.8822) (end 148.7236 98.8822) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB2))
  (segment (start 147.0736 100.1522) (end 150.4536 100.1522) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB1))
  (segment (start 150.4536 100.1522) (end 151.1986 99.4072) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CB0))
  (segment (start 148.7236 98.8822) (end 151.1986 96.4072) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CAF))
  (segment (start 147.0736 97.6122) (end 148.0736 97.6122) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CAE))
  (segment (start 147.0736 101.4222) (end 150.2136 101.4222) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CAD))
  (segment (start 147.0736 103.9622) (end 147.0736 104.5122) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CAC))
  (segment (start 150.9686 108.4072) (end 151.1986 108.4072) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CAB))
  (segment (start 147.0736 102.6922) (end 148.4836 102.6922) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CAA))
  (segment (start 150.2136 101.4222) (end 151.1986 102.4072) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA9))
  (segment (start 147.0736 104.5122) (end 150.9686 108.4072) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA8))
  (segment (start 148.4836 102.6922) (end 151.1986 105.4072) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA7))
  (segment (start 141.6736 97.6122) (end 140.6736 97.6122) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA6))
  (segment (start 141.6736 94.6922) (end 137.6426 90.6612) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA5))
  (segment (start 138.7376 97.7562) (end 137.6426 96.6612) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA4))
  (segment (start 140.6736 97.6122) (end 139.5476 96.4862) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA3))
  (segment (start 139.5476 96.4862) (end 139.5476 95.5662) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA2))
  (segment (start 141.6736 96.3422) (end 141.6736 94.6922) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA1))
  (segment (start 139.5476 95.5662) (end 137.6426 93.6612) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959CA0))
  (segment (start 140.6736 102.6922) (end 139.9116 103.4542) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C9F))
  (segment (start 141.6736 102.6922) (end 140.6736 102.6922) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C9E))
  (segment (start 141.6736 101.4222) (end 140.6736 101.4222) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C9D))
  (segment (start 139.9116 103.4542) (end 139.8496 103.4542) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C9C))
  (segment (start 140.6736 101.4222) (end 139.4346 102.6612) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C9B))
  (segment (start 147.9756 126.9492) (end 150.6906 129.6642) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C9A))
  (segment (start 146.5656 128.2192) (end 146.5656 128.7692) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C99))
  (segment (start 150.4606 132.6642) (end 150.6906 132.6642) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C98))
  (segment (start 146.5656 128.7692) (end 150.4606 132.6642) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C97))
  (segment (start 141.1656 125.6792) (end 140.1656 125.6792) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C96))
  (segment (start 140.1656 123.1392) (end 139.0396 122.0132) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C95))
  (segment (start 138.9266 126.9182) (end 137.1346 126.9182) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C94))
  (segment (start 141.1656 124.4092) (end 137.6256 124.4092) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C93))
  (segment (start 140.1656 125.6792) (end 138.9266 126.9182) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C92))
  (segment (start 137.6256 124.4092) (end 137.1346 123.9182) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C91))
  (segment (start 141.1656 123.1392) (end 140.1656 123.1392) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C90))
  (segment (start 141.1656 128.2192) (end 141.1656 128.8872) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C8F))
  (segment (start 140.1656 126.9492) (end 139.4036 127.7112) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C8E))
  (segment (start 139.3416 127.7112) (end 137.1346 129.9182) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C8D))
  (segment (start 141.1656 128.8872) (end 137.1346 132.9182) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C8C))
  (segment (start 141.1656 126.9492) (end 140.1656 126.9492) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C8B))
  (segment (start 139.4036 127.7112) (end 139.3416 127.7112) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C8A))
  (segment (start 147.9466 121.4882) (end 147.9466 120.4082) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C89))
  (segment (start 146.5656 123.1392) (end 148.2156 123.1392) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C88))
  (segment (start 147.9466 120.4082) (end 150.6906 117.6642) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C87))
  (segment (start 146.5656 120.5992) (end 146.5656 118.7892) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C86))
  (segment (start 146.5656 118.7892) (end 150.6906 114.6642) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C85))
  (segment (start 148.2156 123.1392) (end 150.6906 120.6642) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C84))
  (segment (start 147.5656 121.8692) (end 147.9466 121.4882) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C83))
  (segment (start 146.5656 121.8692) (end 147.5656 121.8692) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C82))
  (segment (start 141.1656 118.9492) (end 137.1346 114.9182) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C81))
  (segment (start 140.1656 121.8692) (end 139.0396 120.7432) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C80))
  (segment (start 139.0396 120.7432) (end 139.0396 119.8232) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C7F))
  (segment (start 139.0396 122.0132) (end 138.2296 122.0132) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C7E))
  (segment (start 139.0396 119.8232) (end 137.1346 117.9182) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C7D))
  (segment (start 141.1656 120.5992) (end 141.1656 118.9492) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C7C))
  (segment (start 138.2296 122.0132) (end 137.1346 120.9182) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C7B))
  (segment (start 141.1656 121.8692) (end 140.1656 121.8692) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C7A))
  (segment (start 146.5656 125.6792) (end 149.7056 125.6792) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C79))
  (segment (start 146.5656 124.4092) (end 149.9456 124.4092) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C78))
  (segment (start 149.9456 124.4092) (end 150.6906 123.6642) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C77))
  (segment (start 146.5656 126.9492) (end 147.9756 126.9492) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C76))
  (segment (start 149.7056 125.6792) (end 150.6906 126.6642) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C75))
  (segment (start 123.3246 94.6592) (end 127.4496 90.5342) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C74))
  (segment (start 124.7056 97.3582) (end 124.7056 96.2782) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C73))
  (segment (start 123.3246 96.4692) (end 123.3246 94.6592) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C72))
  (segment (start 124.7056 96.2782) (end 127.4496 93.5342) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C71))
  (segment (start 123.3246 102.8192) (end 124.7346 102.8192) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C70))
  (segment (start 123.3246 104.6392) (end 127.2196 108.5342) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C6F))
  (segment (start 123.3246 101.5492) (end 126.4646 101.5492) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C6E))
  (segment (start 124.7346 102.8192) (end 127.4496 105.5342) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C6D))
  (segment (start 117.9246 104.0892) (end 117.9246 104.7572) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C6C))
  (segment (start 123.3246 104.0892) (end 123.3246 104.6392) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C6B))
  (segment (start 127.2196 108.5342) (end 127.4496 108.5342) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C6A))
  (segment (start 126.4646 101.5492) (end 127.4496 102.5342) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C69))
  (segment (start 116.9246 97.7392) (end 115.7986 96.6132) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C68))
  (segment (start 117.9246 97.7392) (end 116.9246 97.7392) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C67))
  (segment (start 114.9886 97.8832) (end 113.8936 96.7882) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C66))
  (segment (start 115.7986 95.6932) (end 113.8936 93.7882) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C65))
  (segment (start 115.7986 97.8832) (end 114.9886 97.8832) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C64))
  (segment (start 117.9246 96.4692) (end 117.9246 94.8192) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C63))
  (segment (start 117.9246 94.8192) (end 113.8936 90.7882) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C62))
  (segment (start 115.7986 96.6132) (end 115.7986 95.6932) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C61))
  (segment (start 117.9246 100.2792) (end 114.3846 100.2792) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C60))
  (segment (start 117.9246 99.0092) (end 116.9246 99.0092) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C5F))
  (segment (start 114.3846 100.2792) (end 113.8936 99.7882) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C5E))
  (segment (start 117.9246 101.5492) (end 116.9246 101.5492) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C5D))
  (segment (start 116.9246 101.5492) (end 115.6856 102.7882) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C5C))
  (segment (start 115.6856 102.7882) (end 113.8936 102.7882) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C5B))
  (segment (start 116.9246 99.0092) (end 115.7986 97.8832) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C5A))
  (segment (start 123.3246 100.2792) (end 126.7046 100.2792) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C59))
  (segment (start 126.7046 100.2792) (end 127.4496 99.5342) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C58))
  (segment (start 123.3246 99.0092) (end 124.9746 99.0092) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C57))
  (segment (start 124.9746 99.0092) (end 127.4496 96.5342) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C56))
  (segment (start 124.3246 97.7392) (end 124.7056 97.3582) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C55))
  (segment (start 123.3246 97.7392) (end 124.3246 97.7392) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C54))
  (segment (start 116.1006 103.5812) (end 113.8936 105.7882) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C53))
  (segment (start 116.9246 102.8192) (end 116.1626 103.5812) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C52))
  (segment (start 116.1626 103.5812) (end 116.1006 103.5812) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C51))
  (segment (start 117.9246 102.8192) (end 116.9246 102.8192) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C50))
  (segment (start 117.9246 104.7572) (end 113.8936 108.7882) (width 0.25) (layer B.Cu) (net 0) (tstamp 59959C4F))
  (segment (start 123.604 119.38) (end 123.604 118.83) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995980B))
  (segment (start 127.499 114.935) (end 127.729 114.935) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995980A))
  (segment (start 123.604 118.83) (end 127.499 114.935) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959809))
  (segment (start 123.604 120.65) (end 125.014 120.65) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959808))
  (segment (start 125.014 120.65) (end 127.729 117.935) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959807))
  (segment (start 123.604 121.92) (end 126.744 121.92) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959806))
  (segment (start 126.744 121.92) (end 127.729 120.935) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959805))
  (segment (start 123.604 123.19) (end 126.984 123.19) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959804))
  (segment (start 126.984 123.19) (end 127.729 123.935) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959803))
  (segment (start 123.604 124.46) (end 125.254 124.46) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959802))
  (segment (start 125.254 124.46) (end 127.729 126.935) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959801))
  (segment (start 124.985 126.111) (end 124.985 127.191) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959800))
  (segment (start 124.985 127.191) (end 127.729 129.935) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597FF))
  (segment (start 123.604 125.73) (end 124.604 125.73) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597FE))
  (segment (start 124.604 125.73) (end 124.985 126.111) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597FD))
  (segment (start 123.604 127) (end 123.604 128.81) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597FC))
  (segment (start 123.604 128.81) (end 127.729 132.935) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597FB))
  (segment (start 118.204 127) (end 118.204 128.65) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597FA))
  (segment (start 118.204 128.65) (end 114.173 132.681) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F9))
  (segment (start 116.078 126.856) (end 116.078 127.776) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F8))
  (segment (start 116.078 127.776) (end 114.173 129.681) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F7))
  (segment (start 117.204 125.73) (end 116.078 126.856) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F6))
  (segment (start 116.078 125.586) (end 115.268 125.586) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F5))
  (segment (start 115.268 125.586) (end 114.173 126.681) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F4))
  (segment (start 118.204 125.73) (end 117.204 125.73) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F3))
  (segment (start 118.204 124.46) (end 117.204 124.46) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F2))
  (segment (start 117.204 124.46) (end 116.078 125.586) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F1))
  (segment (start 118.204 123.19) (end 114.664 123.19) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597F0))
  (segment (start 114.664 123.19) (end 114.173 123.681) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597EF))
  (segment (start 118.204 121.92) (end 117.204 121.92) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597EE))
  (segment (start 117.204 121.92) (end 115.965 120.681) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597ED))
  (segment (start 118.204 120.65) (end 117.204 120.65) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597EC))
  (segment (start 117.204 120.65) (end 116.442 119.888) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597EB))
  (segment (start 115.965 120.681) (end 114.173 120.681) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597EA))
  (segment (start 116.442 119.888) (end 116.38 119.888) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597E9))
  (segment (start 116.38 119.888) (end 114.173 117.681) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597E8))
  (segment (start 118.204 119.38) (end 118.204 118.712) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597E7))
  (segment (start 118.204 118.712) (end 114.173 114.681) (width 0.25) (layer F.Cu) (net 0) (tstamp 599597E6))
  (segment (start 147.353 119.507) (end 147.353 118.957) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995972A))
  (segment (start 151.248 115.062) (end 151.478 115.062) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959729))
  (segment (start 147.353 118.957) (end 151.248 115.062) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959728))
  (segment (start 147.353 120.777) (end 148.763 120.777) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959727))
  (segment (start 148.763 120.777) (end 151.478 118.062) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959726))
  (segment (start 147.353 122.047) (end 150.493 122.047) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959725))
  (segment (start 150.493 122.047) (end 151.478 121.062) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959724))
  (segment (start 147.353 123.317) (end 150.733 123.317) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959723))
  (segment (start 150.733 123.317) (end 151.478 124.062) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959722))
  (segment (start 147.353 124.587) (end 149.003 124.587) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959721))
  (segment (start 149.003 124.587) (end 151.478 127.062) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959720))
  (segment (start 148.734 126.238) (end 148.734 127.318) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995971F))
  (segment (start 148.734 127.318) (end 151.478 130.062) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995971E))
  (segment (start 147.353 125.857) (end 148.353 125.857) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995971D))
  (segment (start 148.353 125.857) (end 148.734 126.238) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995971C))
  (segment (start 147.353 127.127) (end 147.353 128.937) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995971B))
  (segment (start 147.353 128.937) (end 151.478 133.062) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995971A))
  (segment (start 141.953 127.127) (end 141.953 128.777) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959719))
  (segment (start 141.953 128.777) (end 137.922 132.808) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959718))
  (segment (start 139.827 126.983) (end 139.827 127.903) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959717))
  (segment (start 139.827 127.903) (end 137.922 129.808) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959716))
  (segment (start 140.953 125.857) (end 139.827 126.983) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959715))
  (segment (start 139.827 125.713) (end 139.017 125.713) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959714))
  (segment (start 139.017 125.713) (end 137.922 126.808) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959713))
  (segment (start 141.953 125.857) (end 140.953 125.857) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959712))
  (segment (start 141.953 124.587) (end 140.953 124.587) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959711))
  (segment (start 140.953 124.587) (end 139.827 125.713) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959710))
  (segment (start 141.953 123.317) (end 138.413 123.317) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995970F))
  (segment (start 138.413 123.317) (end 137.922 123.808) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995970E))
  (segment (start 141.953 122.047) (end 140.953 122.047) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995970D))
  (segment (start 140.953 122.047) (end 139.714 120.808) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995970C))
  (segment (start 141.953 120.777) (end 140.953 120.777) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995970B))
  (segment (start 140.953 120.777) (end 140.191 120.015) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995970A))
  (segment (start 139.714 120.808) (end 137.922 120.808) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959709))
  (segment (start 140.191 120.015) (end 140.129 120.015) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959708))
  (segment (start 140.129 120.015) (end 137.922 117.808) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959707))
  (segment (start 141.953 119.507) (end 141.953 118.839) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959706))
  (segment (start 141.953 118.839) (end 137.922 114.808) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959705))
  (segment (start 146.845 95.25) (end 146.845 94.7) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959649))
  (segment (start 150.74 90.805) (end 150.97 90.805) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959648))
  (segment (start 146.845 94.7) (end 150.74 90.805) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959647))
  (segment (start 146.845 96.52) (end 148.255 96.52) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959646))
  (segment (start 148.255 96.52) (end 150.97 93.805) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959645))
  (segment (start 146.845 97.79) (end 149.985 97.79) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959644))
  (segment (start 149.985 97.79) (end 150.97 96.805) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959643))
  (segment (start 146.845 99.06) (end 150.225 99.06) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959642))
  (segment (start 150.225 99.06) (end 150.97 99.805) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959641))
  (segment (start 146.845 100.33) (end 148.495 100.33) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959640))
  (segment (start 148.495 100.33) (end 150.97 102.805) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995963F))
  (segment (start 148.226 101.981) (end 148.226 103.061) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995963E))
  (segment (start 148.226 103.061) (end 150.97 105.805) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995963D))
  (segment (start 146.845 101.6) (end 147.845 101.6) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995963C))
  (segment (start 147.845 101.6) (end 148.226 101.981) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995963B))
  (segment (start 146.845 102.87) (end 146.845 104.68) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995963A))
  (segment (start 146.845 104.68) (end 150.97 108.805) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959639))
  (segment (start 141.445 102.87) (end 141.445 104.52) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959638))
  (segment (start 141.445 104.52) (end 137.414 108.551) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959637))
  (segment (start 139.319 102.726) (end 139.319 103.646) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959636))
  (segment (start 139.319 103.646) (end 137.414 105.551) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959635))
  (segment (start 140.445 101.6) (end 139.319 102.726) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959634))
  (segment (start 139.319 101.456) (end 138.509 101.456) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959633))
  (segment (start 138.509 101.456) (end 137.414 102.551) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959632))
  (segment (start 141.445 101.6) (end 140.445 101.6) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959631))
  (segment (start 141.445 100.33) (end 140.445 100.33) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959630))
  (segment (start 140.445 100.33) (end 139.319 101.456) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995962F))
  (segment (start 141.445 99.06) (end 137.905 99.06) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995962E))
  (segment (start 137.905 99.06) (end 137.414 99.551) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995962D))
  (segment (start 141.445 97.79) (end 140.445 97.79) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995962C))
  (segment (start 140.445 97.79) (end 139.206 96.551) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995962B))
  (segment (start 141.445 96.52) (end 140.445 96.52) (width 0.25) (layer F.Cu) (net 0) (tstamp 5995962A))
  (segment (start 140.445 96.52) (end 139.683 95.758) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959629))
  (segment (start 139.206 96.551) (end 137.414 96.551) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959628))
  (segment (start 139.683 95.758) (end 139.621 95.758) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959627))
  (segment (start 139.621 95.758) (end 137.414 93.551) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959626))
  (segment (start 141.445 95.25) (end 141.445 94.582) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959625))
  (segment (start 141.445 94.582) (end 137.414 90.551) (width 0.25) (layer F.Cu) (net 0) (tstamp 59959624))
  (segment (start 123.096 94.869) (end 123.096 94.319) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 123.096 94.319) (end 126.991 90.424) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 126.991 90.424) (end 127.221 90.424) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 123.096 96.139) (end 124.506 96.139) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 124.506 96.139) (end 127.221 93.424) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 123.096 97.409) (end 126.236 97.409) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 126.236 97.409) (end 127.221 96.424) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 123.096 98.679) (end 126.476 98.679) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 126.476 98.679) (end 127.221 99.424) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 123.096 99.949) (end 124.746 99.949) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 124.746 99.949) (end 127.221 102.424) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 124.477 101.6) (end 124.477 102.68) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 124.477 102.68) (end 127.221 105.424) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 123.096 101.219) (end 124.096 101.219) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 124.096 101.219) (end 124.477 101.6) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 123.096 102.489) (end 123.096 104.299) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 123.096 104.299) (end 127.221 108.424) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 117.696 102.489) (end 117.696 104.139) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 117.696 104.139) (end 113.665 108.17) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 115.57 102.345) (end 115.57 103.265) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 115.57 103.265) (end 113.665 105.17) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 117.696 101.219) (end 116.696 101.219) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 116.696 101.219) (end 115.57 102.345) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 115.57 101.075) (end 114.76 101.075) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 114.76 101.075) (end 113.665 102.17) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 117.696 99.949) (end 116.696 99.949) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 116.696 99.949) (end 115.57 101.075) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 117.696 98.679) (end 114.156 98.679) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 114.156 98.679) (end 113.665 99.17) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 117.696 97.409) (end 116.696 97.409) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 115.457 96.17) (end 113.665 96.17) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 116.696 97.409) (end 115.457 96.17) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 115.934 95.377) (end 115.872 95.377) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 115.872 95.377) (end 113.665 93.17) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 117.696 96.139) (end 116.696 96.139) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 116.696 96.139) (end 115.934 95.377) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 117.696 94.869) (end 117.696 94.201) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 117.696 94.201) (end 113.665 90.17) (width 0.25) (layer F.Cu) (net 0))

)
