(module KeyElco-1043P (layer F.Cu) (tedit 5A15D06A)
  (fp_text reference REF** (at 0 9) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value KeyElco-1043P (at 0 -11) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 18650 (at 0 0) (layer F.SilkS)
    (effects (font (size 2 2) (thickness 0.15)))
  )
  (fp_text user - (at -35 -8) (layer F.SilkS)
    (effects (font (size 3 3) (thickness 0.15)))
  )
  (fp_text user + (at 36 -8) (layer F.SilkS)
    (effects (font (size 3 3) (thickness 0.15)))
  )
  (fp_line (start -38.75 10.325) (end -38.75 -10.35) (layer F.SilkS) (width 0.15))
  (fp_line (start 38.75 10.325) (end -38.75 10.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 38.75 -10.325) (end 38.75 10.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -38.75 -10.35) (end 38.75 -10.325) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 36.11 0) (size 2 2) (drill 1.32) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -36.11 0) (size 2 2) (drill 1.32) (layers *.Cu *.Mask))
  (pad ~ thru_hole circle (at 27.6 -8) (size 3.55 3.55) (drill 3.55) (layers *.Cu *.Mask))
  (pad ~ thru_hole circle (at -27.6 8) (size 3.55 3.55) (drill 3.55) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 36.11 8) (size 2.39 2.39) (drill 2.39) (layers *.Cu *.Mask))
)
