(module Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
  (fp_text reference R** (at -0.1 2.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Current_Sense_Resistor (at 0.3 -2.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.1 -1.1) (end 4.2 -1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -4 1.1) (end -4.1 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.1 1.1) (end -4.1 -1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.2 -1.1) (end 4.2 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.2 1.1) (end -4.1 1.1) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 5.715 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -5.715 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
)
