(module Screw_Connector_M5 (layer F.Cu) (tedit 58700478)
  (fp_text reference P** (at 0 8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Screw_Connector_M5 (at 0 -9.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at -5.5 -5.5) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 5.3 -5.5) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at -5.5 -0.29) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 5.3 -0.29) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at -5.5 4.92) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at 5.3 4.92) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
)
