(footprint "Colorlight_TE_1473149-4" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at -24 -45.2 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d54b2f00-233d-47f0-af87-28a92c5dd808)
  )
  (fp_text value "Colorlight_TE_1473149-4" (at 41.6 27 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 637c93da-5d66-4516-88d1-f6405c062c1c)
  )
  (fp_text user "${REFERENCE}" (at 41.6 28.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6dd27690-9678-40b7-a242-a65952efe4f1)
  )
  (fp_line (start -5.1 32.4) (end -5.1 35.55) (layer "F.SilkS") (width 0.12) (tstamp f4265868-3a2e-47e3-994d-2a7a6faa6a04))
  (pad "" np_thru_hole circle (at 0 -33.4) (size 1.6 1.6) (drill 1.6) (layers F&B.Cu *.Mask) (tstamp 067b5059-a757-44a8-9d2a-c4984509acd0))
  (pad "" np_thru_hole circle (at 0 33.4) (size 1.1 1.1) (drill 1.1) (layers F&B.Cu *.Mask) (tstamp 33583c74-1d77-488f-ab19-2f51e1e005a3))
  (pad "1" smd roundrect (at -4.1 -31.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a1e90bbb-0ba4-4632-a993-6aa7c8e8488e))
  (pad "2" smd roundrect (at 4.1 -31.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7e676ea9-a137-479c-8fec-22b6b2b1fd5f))
  (pad "3" smd roundrect (at -4.1 -31.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d10dc050-4f6d-4255-8e6a-24fe396adac0))
  (pad "4" smd roundrect (at 4.1 -30.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4028e93c-b5bc-4c19-935c-46353526ae80))
  (pad "5" smd roundrect (at -4.1 -30.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a9702f34-d193-489b-8ad9-32dc57d7b8a9))
  (pad "6" smd roundrect (at 4.1 -30.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 03f13c15-421f-4d29-843a-b94a0a3d9bfa))
  (pad "7" smd roundrect (at -4.1 -29.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 993b2882-3ae9-40f6-a037-f8ae06924912))
  (pad "8" smd roundrect (at 4.1 -29.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9bf15e68-49a9-424d-b349-961f386aaa1b))
  (pad "9" smd roundrect (at -4.1 -29.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c3a728b1-b905-4f39-bbf1-32ddb894e64a))
  (pad "10" smd roundrect (at 4.1 -28.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 67a20117-3d4e-482f-8ed6-63fa9d80e55a))
  (pad "11" smd roundrect (at -4.1 -28.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fe68793b-aba2-44e0-a518-80ae01e7aebc))
  (pad "12" smd roundrect (at 4.1 -28.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 074498f3-60a9-4062-a20a-7e0e600ef6f1))
  (pad "13" smd roundrect (at -4.1 -28.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2827be9d-83d4-44de-92f0-156dd6f83b7c))
  (pad "14" smd roundrect (at 4.1 -27.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c52db49f-dfc3-48ab-8ba0-0630251d350b))
  (pad "15" smd roundrect (at -4.1 -27.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f2714c59-5f7f-41e1-a57e-accfb3eb872e))
  (pad "16" smd roundrect (at 4.1 -27.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9ec44eea-7a4d-435a-86f4-8359710b2713))
  (pad "17" smd roundrect (at -4.1 -26.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e5b58f64-1275-444f-8802-b99c717801f6))
  (pad "18" smd roundrect (at 4.1 -26.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 804de261-be90-4953-a1b5-8010ded1ab67))
  (pad "19" smd roundrect (at -4.1 -26.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 83c6dad9-98b8-486c-81b7-ffc66c141c69))
  (pad "20" smd roundrect (at 4.1 -25.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 93964749-8632-43a4-b3ba-eba5d8135ad0))
  (pad "21" smd roundrect (at -4.1 -25.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ad2cc53f-3e88-4edb-9311-84e7f391f8c5))
  (pad "22" smd roundrect (at 4.1 -25.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a2fa8970-0b33-4af7-88dc-750ad98dee02))
  (pad "23" smd roundrect (at -4.1 -25.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b0cc9c5a-017c-40f0-b805-2ce63eeeff41))
  (pad "24" smd roundrect (at 4.1 -24.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 21bca255-2b30-4228-8dc8-ae03eede1409))
  (pad "25" smd roundrect (at -4.1 -24.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 898f35a1-cf2f-4491-b95c-38cb50b18095))
  (pad "26" smd roundrect (at 4.1 -24.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0315a570-edb6-4673-b2a0-92be1d87457c))
  (pad "27" smd roundrect (at -4.1 -23.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 82ffadd4-4309-4b9c-af07-67dfb7d5b4a7))
  (pad "28" smd roundrect (at 4.1 -23.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5d607bd0-3bd3-40eb-8d90-7307b52bc119))
  (pad "29" smd roundrect (at -4.1 -23.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7e0e36a9-203f-4468-9f8f-4c4acdb0390b))
  (pad "30" smd roundrect (at 4.1 -22.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b036e854-32ca-47af-8921-e35cb244ba8e))
  (pad "31" smd roundrect (at -4.1 -22.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 36b5949f-4d0b-4353-972c-07cfd1798110))
  (pad "32" smd roundrect (at 4.1 -22.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cade7c7c-7d82-48d0-8178-ca0999049f59))
  (pad "33" smd roundrect (at -4.1 -22.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 58762fb7-b9f1-45b2-96b5-a9d1a6780ad4))
  (pad "34" smd roundrect (at 4.1 -21.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 545f4b94-b3cc-4143-a776-933406f43d87))
  (pad "35" smd roundrect (at -4.1 -21.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d4b1282e-b6d7-450b-aa5c-82a7ea0dae67))
  (pad "36" smd roundrect (at 4.1 -21.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 67635a53-7f9b-41a4-b8ba-c7227c8e90a4))
  (pad "37" smd roundrect (at -4.1 -20.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3748eb66-8fe8-48b8-b867-6fbb31faf984))
  (pad "38" smd roundrect (at 4.1 -20.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b111c3d7-fbf7-4d87-8e99-0027bed77297))
  (pad "39" smd roundrect (at -4.1 -20.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6b457301-49f2-4d07-ba9f-84de179b8cc3))
  (pad "40" smd roundrect (at 4.1 -19.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4073320c-81fe-4e93-b881-597b2e1517a9))
  (pad "41" smd roundrect (at -4.1 -16.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp caabe49b-540e-4541-bb20-759376a8cf01))
  (pad "42" smd roundrect (at 4.1 -15.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 445d2fca-010e-4f66-8a46-82cba8784e54))
  (pad "43" smd roundrect (at -4.1 -15.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9ba66fda-bc1d-4ecc-bce0-8813949d7195))
  (pad "44" smd roundrect (at 4.1 -15.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 244f9d33-d553-48f4-bfd4-67828af6756e))
  (pad "45" smd roundrect (at -4.1 -14.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cde397d8-389f-4426-8557-120b774f26d6))
  (pad "46" smd roundrect (at 4.1 -14.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e8234af4-8b0b-4196-9174-0f3b37f0c881))
  (pad "47" smd roundrect (at -4.1 -14.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8a7dec7e-f6b4-4084-90ba-d8dc2b781d59))
  (pad "48" smd roundrect (at 4.1 -13.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dc5182d7-c7c7-4543-b03c-944b6e206a85))
  (pad "49" smd roundrect (at -4.1 -13.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2c422a45-b9fd-4aa0-8548-3fbb3b71618a))
  (pad "50" smd roundrect (at 4.1 -13.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5c3b46ab-9cfe-4c76-951b-bd68cbee0803))
  (pad "51" smd roundrect (at -4.1 -13.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d393a621-3e2c-40be-8faa-3e318e80929b))
  (pad "52" smd roundrect (at 4.1 -12.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e75d4882-4541-456d-806d-a02a331d4e84))
  (pad "53" smd roundrect (at -4.1 -12.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5adfa341-b614-4a12-b601-9ffabda0fdd2))
  (pad "54" smd roundrect (at 4.1 -12.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1127b6b3-80ee-4f94-a57b-75f7756c270d))
  (pad "55" smd roundrect (at -4.1 -11.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f6bab910-c860-4200-a489-368ef540a315))
  (pad "56" smd roundrect (at 4.1 -11.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d0675178-e4ee-4eb2-bc94-efa201c5a184))
  (pad "57" smd roundrect (at -4.1 -11.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e5630b1e-934a-4020-ab47-49dad54238ff))
  (pad "58" smd roundrect (at 4.1 -10.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ca06902e-bee7-4409-8577-e046720a4f06))
  (pad "59" smd roundrect (at -4.1 -10.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7d96f80c-5d63-4fec-94c5-5f71cf130db5))
  (pad "60" smd roundrect (at 4.1 -10.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 77f1dcdc-2a62-412d-8002-eade3a9c0fea))
  (pad "61" smd roundrect (at -4.1 -10.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 42293eb8-6b42-4912-acb6-2e03023fd908))
  (pad "62" smd roundrect (at 4.1 -9.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 038c2a47-68ec-42ac-a148-76e0f51e7729))
  (pad "63" smd roundrect (at -4.1 -9.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2cd53cf0-a7fa-4367-8df1-f80112e93dfb))
  (pad "64" smd roundrect (at 4.1 -9.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2b646a85-0c06-41be-9ba9-59640d9980fe))
  (pad "65" smd roundrect (at -4.1 -8.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 62a841ca-5b7d-4136-aed4-1c5cf3696812))
  (pad "66" smd roundrect (at 4.1 -8.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f8b7707d-159c-4ff3-a011-ae1fdbff1825))
  (pad "67" smd roundrect (at -4.1 -8.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e673b1fd-080d-418b-9b0b-b7c0731e108c))
  (pad "68" smd roundrect (at 4.1 -7.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f013914d-642a-4c19-8e65-a2e87743b5d1))
  (pad "69" smd roundrect (at -4.1 -7.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f6e23569-17e3-4209-be53-83daec87b0af))
  (pad "70" smd roundrect (at 4.1 -7.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c70882a7-4f05-4204-acb0-85bbe4b2f6c0))
  (pad "71" smd roundrect (at -4.1 -7.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c64820a6-d72c-4747-950f-790b899205c8))
  (pad "72" smd roundrect (at 4.1 -6.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7bb1cfba-9620-4349-8a6b-58b8d8d65ce1))
  (pad "73" smd roundrect (at -4.1 -6.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c61e2f25-8171-4c4b-9aef-9a42dd6a8744))
  (pad "74" smd roundrect (at 4.1 -6.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 28e55ae2-533d-4489-9379-fff11baafe50))
  (pad "75" smd roundrect (at -4.1 -5.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a436a1f1-3651-4da2-811a-98a95660671c))
  (pad "76" smd roundrect (at 4.1 -5.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9945ec38-fc89-4397-84ab-d7d934e2a341))
  (pad "77" smd roundrect (at -4.1 -5.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0c6f182c-1537-479a-97e1-5372e7df39f2))
  (pad "78" smd roundrect (at 4.1 -4.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9e5253d5-61f5-449f-a7ba-29ccde732b5f))
  (pad "79" smd roundrect (at -4.1 -4.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e3dc1238-33fa-4953-b623-45e115b61aad))
  (pad "80" smd roundrect (at 4.1 -4.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 56756b73-6bb0-4057-b7ea-2fe2bc0550f5))
  (pad "81" smd roundrect (at -4.1 -4.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e38dad62-b7ce-47ca-a7a2-c67368cf8a1e))
  (pad "82" smd roundrect (at 4.1 -3.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 527acdcd-e646-418a-91eb-6377ba6c105c))
  (pad "83" smd roundrect (at -4.1 -3.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 691fd369-7978-4c78-9ccf-0bb9ff418e27))
  (pad "84" smd roundrect (at 4.1 -3.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 347b42f7-a6a2-4df5-bc08-a9908c6cec6f))
  (pad "85" smd roundrect (at -4.1 -2.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cb9cef84-bc6a-4c3f-abc5-358fb11de53c))
  (pad "86" smd roundrect (at 4.1 -2.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 42c8754e-2617-43eb-a434-2c1ab04eaaf5))
  (pad "87" smd roundrect (at -4.1 -2.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 17dc7f61-be87-4985-921e-7c001f1bcdf7))
  (pad "88" smd roundrect (at 4.1 -1.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ad48a55d-9460-4207-b9b1-977157295b88))
  (pad "89" smd roundrect (at -4.1 -1.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b0d33d72-d2d6-4c1a-9299-494d7373abf6))
  (pad "90" smd roundrect (at 4.1 -1.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ddc3d9a9-deb4-4677-9e1f-deef8b911a13))
  (pad "91" smd roundrect (at -4.1 -1.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dca09e8f-7b8c-4d0a-85da-66e31f4dd424))
  (pad "92" smd roundrect (at 4.1 -0.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2e14f65b-80b6-4bb4-b44a-48b28c7fc364))
  (pad "93" smd roundrect (at -4.1 -0.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c3e496f2-e085-4f0d-8443-4559f8a1fded))
  (pad "94" smd roundrect (at 4.1 -0.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 80405940-3d35-4095-9204-f662daee5642))
  (pad "95" smd roundrect (at -4.1 0.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 74fd1de2-f89a-4b27-b333-c63ddf63def3))
  (pad "96" smd roundrect (at 4.1 0.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a3416a60-8b34-4f02-ae78-d742606102ef))
  (pad "97" smd roundrect (at -4.1 0.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f9986e9f-eda7-49ac-b38c-d47c9f034949))
  (pad "98" smd roundrect (at 4.1 1.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f0a7e61c-af7f-4545-9c27-6782b93fa5f1))
  (pad "99" smd roundrect (at -4.1 1.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e2d6558b-8c5f-4ff3-97a6-79187beb29a1))
  (pad "100" smd roundrect (at 4.1 1.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7d5a1dbb-648b-48fb-a255-1c9c27fbe224))
  (pad "101" smd roundrect (at -4.1 1.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a9cc2c4b-bc38-4aa4-a7fb-c318747e3861))
  (pad "102" smd roundrect (at 4.1 2.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 012b34cf-47ec-41c7-87b4-78a2cde2cab4))
  (pad "103" smd roundrect (at -4.1 2.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 12c56681-16aa-4f03-b3a7-2292c94f793f))
  (pad "104" smd roundrect (at 4.1 2.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4aeb9c22-e7f4-4af4-8979-c6d74c469071))
  (pad "105" smd roundrect (at -4.1 3.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d890a60d-2393-499b-aba5-558ec36eeeba))
  (pad "106" smd roundrect (at 4.1 3.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8e51d3fa-a265-4dd0-92f6-80ddaf57ef9b))
  (pad "107" smd roundrect (at -4.1 3.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a563e81c-728b-4c72-87f8-c3bee1016980))
  (pad "108" smd roundrect (at 4.1 4.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d09713bb-cf0b-4148-a2a0-1574778ead27))
  (pad "109" smd roundrect (at -4.1 4.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ef967711-38e8-4708-bcbb-b33436b9ba56))
  (pad "110" smd roundrect (at 4.1 4.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 39a02fa5-2e88-49b7-a07e-b5086d53b0dd))
  (pad "111" smd roundrect (at -4.1 4.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 42f53693-8b92-4146-9e22-6a6e4fefc162))
  (pad "112" smd roundrect (at 4.1 5.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6a938db2-8482-4ff9-8ba9-fb9f7b71e0c8))
  (pad "113" smd roundrect (at -4.1 5.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a32b901d-dcd9-443e-a1e1-86f3e0c151bb))
  (pad "114" smd roundrect (at 4.1 5.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 32fdbbd0-9304-44d8-946a-bb28ad001a10))
  (pad "115" smd roundrect (at -4.1 6.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cd6b7b6d-0498-4677-b9db-c24d096669d6))
  (pad "116" smd roundrect (at 4.1 6.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5592b158-5ef6-498d-8ddf-92adaa39ae88))
  (pad "117" smd roundrect (at -4.1 6.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 85c65209-5de5-4a63-8514-56582e7312c4))
  (pad "118" smd roundrect (at 4.1 7.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0e2e59c1-e08d-4ef7-b56d-854653df1bff))
  (pad "119" smd roundrect (at -4.1 7.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ed4ea340-3b90-45c2-8448-be8130bf8b14))
  (pad "120" smd roundrect (at 4.1 7.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 69471622-23f2-4519-994f-70ddfdf2c839))
  (pad "121" smd roundrect (at -4.1 7.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5dbe2c07-a661-4537-b868-52dde24a6bc4))
  (pad "122" smd roundrect (at 4.1 8.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a86904d7-d883-44f8-b741-5cc86b3353d2))
  (pad "123" smd roundrect (at -4.1 8.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 54021a06-a522-4692-ad2a-d7324e67322d))
  (pad "124" smd roundrect (at 4.1 8.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6701acbb-3f5c-4d83-8dba-2028e66dafca))
  (pad "125" smd roundrect (at -4.1 9.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 427d623c-2a5b-43d9-a764-c83eda860777))
  (pad "126" smd roundrect (at 4.1 9.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 930fdcbb-11ec-4a06-bf3d-52dd4cbc34fd))
  (pad "127" smd roundrect (at -4.1 9.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 31912927-ef62-4c64-aafa-52119d293e8f))
  (pad "128" smd roundrect (at 4.1 10.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f9ab967e-b475-4c24-9b71-112fe9679457))
  (pad "129" smd roundrect (at -4.1 10.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5fb79af5-2195-4f5f-b0f1-9ec4a053cdb2))
  (pad "130" smd roundrect (at 4.1 10.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9b7832c7-f7da-4e86-ac83-41589082de11))
  (pad "131" smd roundrect (at -4.1 10.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 13376da5-3a9e-4c1f-99f4-2788045ffefe))
  (pad "132" smd roundrect (at 4.1 11.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b9ef1a77-f015-48fb-8bcc-23054516e9be))
  (pad "133" smd roundrect (at -4.1 11.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a3035f6f-d9cb-4d30-9d51-d151fe396261))
  (pad "134" smd roundrect (at 4.1 11.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bd9378b3-e7a6-4735-b8a5-ae30b641d33c))
  (pad "135" smd roundrect (at -4.1 12.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 89ca56ba-a98f-40c8-8046-fc224b50af82))
  (pad "136" smd roundrect (at 4.1 12.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bcb48b4c-edb2-46fe-ad73-f37acb2af627))
  (pad "137" smd roundrect (at -4.1 12.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp be17e076-c7b6-49f3-b7ef-8d321c39ca20))
  (pad "138" smd roundrect (at 4.1 13.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 75c56499-b5db-4071-abd9-9236cdb6c5b9))
  (pad "139" smd roundrect (at -4.1 13.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5752ea70-46fe-4394-90f3-1d91e078ad0d))
  (pad "140" smd roundrect (at 4.1 13.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f46c3b67-dce8-45e1-869d-73e871a8acf9))
  (pad "141" smd roundrect (at -4.1 13.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fdba2f13-9f74-4020-b162-bcb45087d76c))
  (pad "142" smd roundrect (at 4.1 14.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 047ef7af-b97c-42f0-bbe2-f1959cabef70))
  (pad "143" smd roundrect (at -4.1 14.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 87e9b8b2-60f6-49c7-8cdb-e9aafe2479cc))
  (pad "144" smd roundrect (at 4.1 14.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b40c661a-a70f-4334-aba9-4c93e1b6e0b4))
  (pad "145" smd roundrect (at -4.1 15.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 89fce37e-2121-4530-aadd-70c3ad7ee1d4))
  (pad "146" smd roundrect (at 4.1 15.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ac3fdcf5-0097-4cb6-ac3d-9d9d9fe106d7))
  (pad "147" smd roundrect (at -4.1 15.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e9fd84c2-edee-4ee9-820f-716fe4ee8502))
  (pad "148" smd roundrect (at 4.1 16.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5188507d-50da-484b-9f6b-c8d2a1ef37d6))
  (pad "149" smd roundrect (at -4.1 16.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fb2e9671-d3cf-4a88-a311-077278181812))
  (pad "150" smd roundrect (at 4.1 16.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5e6ccc8e-e886-4145-8f37-2b2ac2983bd8))
  (pad "151" smd roundrect (at -4.1 16.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b63a5c2e-0afb-46fb-a5a9-820340d749bb))
  (pad "152" smd roundrect (at 4.1 17.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 45b68ea0-8ae4-498f-b3cf-5346f5d2a5b2))
  (pad "153" smd roundrect (at -4.1 17.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 54af1a63-547b-4a91-8bef-a1b56441cd4d))
  (pad "154" smd roundrect (at 4.1 17.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4008735d-6b28-4bb7-90ec-8064d0411436))
  (pad "155" smd roundrect (at -4.1 18.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e1373ba6-adbf-4a05-9188-9c05661206f2))
  (pad "156" smd roundrect (at 4.1 18.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ef63979b-3689-417c-9be0-c815ef623ec4))
  (pad "157" smd roundrect (at -4.1 18.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 50550c46-4f22-46ef-a309-08abe0cbb462))
  (pad "158" smd roundrect (at 4.1 19.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3f5f01a0-c55a-4fbb-a70f-844d4a1d2a84))
  (pad "159" smd roundrect (at -4.1 19.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4e3986e2-57b7-4287-9b85-3edb69e2231a))
  (pad "160" smd roundrect (at 4.1 19.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 96fc04d5-a8cc-4f0d-a379-fcc5b4d80d16))
  (pad "161" smd roundrect (at -4.1 19.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2df57005-2770-4b72-b958-e0460cd0d2ba))
  (pad "162" smd roundrect (at 4.1 20.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e9de9fb5-b6ea-448b-bdf0-3055fec78281))
  (pad "163" smd roundrect (at -4.1 20.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4d6cae4c-ecfd-4185-94a8-c42015b0c6eb))
  (pad "164" smd roundrect (at 4.1 20.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2f5beb9e-826e-4529-ba60-889a1198ed30))
  (pad "165" smd roundrect (at -4.1 21.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0892b13c-803d-4cbf-8677-ceb7e5a9e854))
  (pad "166" smd roundrect (at 4.1 21.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2dac146d-6516-4aa6-a0ef-b5c5473040b0))
  (pad "167" smd roundrect (at -4.1 21.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8ebcd359-bef1-480b-a29f-7177dcf3c436))
  (pad "168" smd roundrect (at 4.1 22.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8c705637-c069-42c9-aa33-fc8b7ce366be))
  (pad "169" smd roundrect (at -4.1 22.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp caaca47c-323c-4513-8d75-e0be1349794e))
  (pad "170" smd roundrect (at 4.1 22.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e6a36faf-fefd-4e62-801e-10791111c1db))
  (pad "171" smd roundrect (at -4.1 22.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2e1d679d-53cc-4d0a-a60a-ad2794879099))
  (pad "172" smd roundrect (at 4.1 23.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1e310147-c42a-478f-a399-603575b1502f))
  (pad "173" smd roundrect (at -4.1 23.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8bea4613-d645-45cb-a714-768c7d0b3b71))
  (pad "174" smd roundrect (at 4.1 23.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4ee43990-7d03-4209-877c-0aa3e271bce0))
  (pad "175" smd roundrect (at -4.1 24.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e689b023-18ab-4465-a5c8-0e23f43a7226))
  (pad "176" smd roundrect (at 4.1 24.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e972151a-495a-4cb1-a0bf-54756d68117a))
  (pad "177" smd roundrect (at -4.1 24.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 979a0ac1-2923-4f15-b6e3-31dbf96fae9f))
  (pad "178" smd roundrect (at 4.1 25.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4a1391a7-c433-4117-91d9-ee084a772153))
  (pad "179" smd roundrect (at -4.1 25.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3b6912c9-91e8-4f31-a7fd-8b45f1654143))
  (pad "180" smd roundrect (at 4.1 25.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7ed54439-7076-45a8-84cb-7ec6154bac94))
  (pad "181" smd roundrect (at -4.1 25.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fe4f2f9f-97c3-43e4-99d5-0c6cc2814f6f))
  (pad "182" smd roundrect (at 4.1 26.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 35e01383-592e-4a3f-9d6a-8a71f3fad6ad))
  (pad "183" smd roundrect (at -4.1 26.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0dbd7f24-8297-4ee1-9375-e2a0f8cb42ac))
  (pad "184" smd roundrect (at 4.1 26.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 04d49d44-68b1-415a-86c5-59fb86588b73))
  (pad "185" smd roundrect (at -4.1 27.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 143be012-448f-497d-8394-3e60f9a519ef))
  (pad "186" smd roundrect (at 4.1 27.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 29dc6837-0493-464e-af63-7fbaec388229))
  (pad "187" smd roundrect (at -4.1 27.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cd3f361c-5044-4e34-90d5-c66521015f33))
  (pad "188" smd roundrect (at 4.1 28.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 14619db5-b942-4958-bcc2-4a0c32c45d4a))
  (pad "189" smd roundrect (at -4.1 28.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fceb6ac4-1956-4594-a634-c758b1c43a85))
  (pad "190" smd roundrect (at 4.1 28.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 13c597c1-9514-4d9c-a3c2-99848f949a26))
  (pad "191" smd roundrect (at -4.1 28.95) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 66ae23a7-f5b0-4acc-a035-6d547882a0c8))
  (pad "192" smd roundrect (at 4.1 29.25) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 578749f7-808c-4130-bec0-946996a513fb))
  (pad "193" smd roundrect (at -4.1 29.55) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 822c41ec-41e0-4dea-8c65-7639fc6deddd))
  (pad "194" smd roundrect (at 4.1 29.85) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2b9faa7f-33c7-457d-b770-b73c62b97e58))
  (pad "195" smd roundrect (at -4.1 30.15) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c9409ffd-9c83-46b7-88fa-e7a191e34eae))
  (pad "196" smd roundrect (at 4.1 30.45) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp af128547-1649-4a37-8981-c823dd35e46b))
  (pad "197" smd roundrect (at -4.1 30.75) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 36da00c2-916f-4ee6-aaa8-1e96e3247be1))
  (pad "198" smd roundrect (at 4.1 31.05) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2cf1f38c-831b-4925-9f47-c8b737a38a5c))
  (pad "199" smd roundrect (at -4.1 31.35) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4c311214-9afe-4795-a93a-cd81ddab8944))
  (pad "200" smd roundrect (at 4.1 31.65) (size 2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 518e41ba-9469-40a2-818f-77eed530e5a0))
  (pad "MEC0" smd rect (at 12 -32.55) (size 4.6 4.5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp cdf1a4ba-842a-4de2-801d-fcaaf25ed5ec))
  (pad "MEC0" smd rect (at 12 32.55) (size 4.6 4.5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp feae808f-cb1a-4ba6-847e-4e571314fb24))
)
