(export (version D)
  (design
    (source /home/isthatme/kicad-projects/stm32f030-basic/stm32f030-basic.sch)
    (date "Sat 11 Feb 2017 09:49:05 PM MST")
    (tool "Eeschema 4.0.5-e0-6337~49~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source stm32f030-basic.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value STM32F030K6T6)
      (footprint Housings_QFP:LQFP-32_7x7mm_Pitch0.8mm)
      (libsource (lib stm32f030k6t6) (part STM32F030K6T6))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FD65B))
    (comp (ref P1)
      (value CONN_01X06)
      (footprint Socket_Strips:Socket_Strip_Straight_1x06)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FD838))
    (comp (ref Y1)
      (value Crystal)
      (footprint Crystals:Crystal_SMD_HC49-SD_HandSoldering)
      (libsource (lib device) (part Crystal))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FDB39))
    (comp (ref C1)
      (value C_Small)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FDCD1))
    (comp (ref C2)
      (value C_Small)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FDD2E))
    (comp (ref CON1)
      (value Micro_SD_Card)
      (footprint microSD:microSD-5031821852)
      (libsource (lib conn) (part Micro_SD_Card))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FDFA5))
    (comp (ref P2)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FEC3B))
    (comp (ref P3)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FEC8C))
    (comp (ref P6)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FECCF))
    (comp (ref P7)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FED11))
    (comp (ref P4)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF13E))
    (comp (ref P5)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF18C))
    (comp (ref P9)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF465))
    (comp (ref P10)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF4A8))
    (comp (ref P8)
      (value CONN_01X08)
      (footprint Socket_Strips:Socket_Strip_Straight_1x08)
      (libsource (lib conn) (part CONN_01X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF52C))
    (comp (ref P11)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A00A91))
    (comp (ref P12)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A00AF5))
    (comp (ref U2)
      (value LD3985M)
      (footprint TO_SOT_Packages_SMD:SOT-23-5)
      (libsource (lib regul) (part LD3985M))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A00B5D))
    (comp (ref C4)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A019C0))
    (comp (ref C3)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A01A5B)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X06)
      (description "Connector, single row, 01x06")
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_01X08)
      (description "Connector, single row, 01x08")
      (footprints
        (fp Pin_Header_Straight_1X08)
        (fp Pin_Header_Angled_1X08)
        (fp Socket_Strip_Straight_1X08)
        (fp Socket_Strip_Angled_1X08))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X08))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Crystal)
      (description "Two pin crystal")
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib regul) (part LD3985M)
      (description "150 mA Low Dropout Voltage Regulator")
      (docs http://www.st.com/internet/analog/product/69230.jsp)
      (fields
        (field (name Reference) U)
        (field (name Value) LD3985M)
        (field (name Footprint) SOT-23-5))
      (pins
        (pin (num 1) (name VIN) (type input))
        (pin (num 2) (name GND) (type input))
        (pin (num 3) (name INH) (type input))
        (pin (num 4) (name BYP) (type input))
        (pin (num 5) (name VOUT) (type input))))
    (libpart (lib conn) (part Micro_SD_Card)
      (description "Micro SD Card Socket")
      (docs http://katalog.we-online.de/em/datasheet/693072010801.pdf)
      (fields
        (field (name Reference) CON)
        (field (name Value) Micro_SD_Card))
      (pins
        (pin (num 1) (name DAT2) (type BiDi))
        (pin (num 2) (name DAT3/CD) (type BiDi))
        (pin (num 3) (name CMD) (type input))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type power_in))
        (pin (num 7) (name DAT0) (type input))
        (pin (num 8) (name DAT1) (type input))
        (pin (num 9) (name SHIELD) (type passive))))
    (libpart (lib stm32f030k6t6) (part STM32F030K6T6)
      (description "STM32F030K6T6 - 32 Bit ARM Microcontroller")
      (docs http://www.st.com/content/ccc/resource/technical/document/datasheet/a4/5d/0b/0e/87/c4/4d/71/DM00088500.pdf/files/DM00088500.pdf/jcr:content/translations/en.DM00088500.pdf)
      (footprints
        (fp LQFP-32_7x7mm_Pitch0.8mm))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F030K6T6))
      (pins
        (pin (num 1) (name Vdd) (type power_in))
        (pin (num 2) (name PF0) (type input))
        (pin (num 3) (name PF1) (type output))
        (pin (num 4) (name NRST) (type input))
        (pin (num 5) (name Vdda) (type power_in))
        (pin (num 6) (name PA0) (type BiDi))
        (pin (num 7) (name PA1) (type BiDi))
        (pin (num 8) (name PA2) (type BiDi))
        (pin (num 9) (name PA3) (type BiDi))
        (pin (num 10) (name PA4) (type BiDi))
        (pin (num 11) (name PA5) (type BiDi))
        (pin (num 12) (name PA6) (type BiDi))
        (pin (num 13) (name PA7) (type BiDi))
        (pin (num 14) (name PB0) (type BiDi))
        (pin (num 15) (name PB1) (type BiDi))
        (pin (num 16) (name Vss) (type power_in))
        (pin (num 17) (name Vdd) (type power_in))
        (pin (num 18) (name PA8) (type BiDi))
        (pin (num 19) (name PA9) (type BiDi))
        (pin (num 20) (name PA10) (type BiDi))
        (pin (num 21) (name PA11) (type BiDi))
        (pin (num 22) (name PA12) (type BiDi))
        (pin (num 23) (name PA13/SWDIO) (type BiDi))
        (pin (num 24) (name PA14/SWCLK) (type BiDi))
        (pin (num 25) (name PA15) (type BiDi))
        (pin (num 26) (name PB3) (type BiDi))
        (pin (num 27) (name PB4) (type BiDi))
        (pin (num 28) (name PB5) (type BiDi))
        (pin (num 29) (name PB6) (type BiDi))
        (pin (num 30) (name PB7) (type BiDi))
        (pin (num 31) (name BOOT0) (type input))
        (pin (num 32) (name Vss) (type power_in)))))
  (libraries
    (library (logical regul)
      (uri /usr/share/kicad/library/regul.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical stm32f030k6t6)
      (uri /home/isthatme/kicad-projects/Custom-Parts/stm32f030k6t6.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib)))
  (nets
    (net (code 1) (name "Net-(C1-Pad2)")
      (node (ref U1) (pin 2))
      (node (ref C1) (pin 2)))
    (net (code 2) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1))
      (node (ref U1) (pin 6)))
    (net (code 3) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 4) (name "Net-(P4-Pad1)")
      (node (ref P4) (pin 1))
      (node (ref U1) (pin 8)))
    (net (code 5) (name "Net-(P5-Pad1)")
      (node (ref P5) (pin 1))
      (node (ref U1) (pin 9)))
    (net (code 6) (name "Net-(P6-Pad1)")
      (node (ref U1) (pin 10))
      (node (ref P6) (pin 1)))
    (net (code 7) (name GND)
      (node (ref P7) (pin 2))
      (node (ref P1) (pin 5))
      (node (ref P1) (pin 6))
      (node (ref P11) (pin 2))
      (node (ref P12) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref P6) (pin 2))
      (node (ref P3) (pin 2))
      (node (ref P2) (pin 2))
      (node (ref CON1) (pin 9))
      (node (ref CON1) (pin 6))
      (node (ref U1) (pin 32))
      (node (ref P8) (pin 7))
      (node (ref P8) (pin 6))
      (node (ref P8) (pin 5))
      (node (ref P5) (pin 2))
      (node (ref P4) (pin 2))
      (node (ref P8) (pin 8))
      (node (ref U1) (pin 16))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2)))
    (net (code 10) (name "Net-(P7-Pad1)")
      (node (ref P7) (pin 1))
      (node (ref U1) (pin 11)))
    (net (code 11) (name "Net-(P1-Pad4)")
      (node (ref U1) (pin 4))
      (node (ref P1) (pin 4)))
    (net (code 12) (name "Net-(C1-Pad1)")
      (node (ref Y1) (pin 2))
      (node (ref C1) (pin 1)))
    (net (code 13) (name "Net-(C2-Pad1)")
      (node (ref Y1) (pin 1))
      (node (ref C2) (pin 1)))
    (net (code 14) (name "Net-(C2-Pad2)")
      (node (ref C2) (pin 2))
      (node (ref U1) (pin 3)))
    (net (code 15) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 16) (name +Vdd)
      (node (ref CON1) (pin 4))
      (node (ref U2) (pin 5))
      (node (ref U1) (pin 1))
      (node (ref U1) (pin 17))
      (node (ref C4) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref P1) (pin 1))
      (node (ref P12) (pin 1)))
    (net (code 17) (name /+12V)
      (node (ref P11) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref C3) (pin 1)))
    (net (code 18) (name "Net-(P8-Pad1)")
      (node (ref U1) (pin 12))
      (node (ref P8) (pin 1)))
    (net (code 19) (name "Net-(P8-Pad2)")
      (node (ref U1) (pin 13))
      (node (ref P8) (pin 2)))
    (net (code 20) (name "Net-(P8-Pad3)")
      (node (ref U1) (pin 18))
      (node (ref P8) (pin 3)))
    (net (code 21) (name "Net-(P8-Pad4)")
      (node (ref P8) (pin 4))
      (node (ref U1) (pin 25)))
    (net (code 22) (name "Net-(U1-Pad31)")
      (node (ref U1) (pin 31)))
    (net (code 23) (name "Net-(CON1-Pad1)")
      (node (ref CON1) (pin 1)))
    (net (code 24) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30)))
    (net (code 25) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 26) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 27) (name /I2C1_SCL)
      (node (ref U1) (pin 19))
      (node (ref P9) (pin 1)))
    (net (code 28) (name /I2C1_SDA)
      (node (ref P9) (pin 2))
      (node (ref U1) (pin 20)))
    (net (code 29) (name /I2C2_SCL)
      (node (ref U1) (pin 21))
      (node (ref P10) (pin 1)))
    (net (code 30) (name /I2C2_SDA)
      (node (ref P10) (pin 2))
      (node (ref U1) (pin 22)))
    (net (code 31) (name "Net-(CON1-Pad8)")
      (node (ref CON1) (pin 8)))
    (net (code 32) (name /SPI1_CLK)
      (node (ref CON1) (pin 5))
      (node (ref U1) (pin 26)))
    (net (code 33) (name /SPI1_MISO)
      (node (ref CON1) (pin 7))
      (node (ref U1) (pin 27)))
    (net (code 34) (name /SPI1_MOSI)
      (node (ref U1) (pin 28))
      (node (ref CON1) (pin 3)))
    (net (code 35) (name /SPI_CS)
      (node (ref U1) (pin 29))
      (node (ref CON1) (pin 2)))
    (net (code 36) (name /SWDIO)
      (node (ref U1) (pin 23))
      (node (ref P1) (pin 2)))
    (net (code 37) (name /SWCLK)
      (node (ref P1) (pin 3))
      (node (ref U1) (pin 24)))))