(export (version D)
  (design
    (source /home/isthatme/kicad-projects/Uno-Switch-Shield/Uno-Switch-Shield.sch)
    (date "Thu 27 Jul 2017 01:52:40 PM MDT")
    (tool "Eeschema 4.0.6-e0-6349~53~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date "lun. 30 mars 2015")
        (source Uno-Switch-Shield.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P1)
      (value Power)
      (footprint Socket_Arduino_Uno:Socket_Strip_Arduino_1x08)
      (libsource (lib conn) (part CONN_01X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D70129))
    (comp (ref P2)
      (value Analog)
      (footprint Socket_Arduino_Uno:Socket_Strip_Arduino_1x06)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D70DD8))
    (comp (ref P5)
      (value CONN_01X01)
      (footprint Socket_Arduino_Uno:Arduino_1pin)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D71177))
    (comp (ref P6)
      (value CONN_01X01)
      (footprint Socket_Arduino_Uno:Arduino_1pin)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D71274))
    (comp (ref P7)
      (value CONN_01X01)
      (footprint Socket_Arduino_Uno:Arduino_1pin)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D712A8))
    (comp (ref P8)
      (value CONN_01X01)
      (footprint Socket_Arduino_Uno:Arduino_1pin)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D712DB))
    (comp (ref P4)
      (value Digital)
      (footprint Socket_Arduino_Uno:Socket_Strip_Arduino_1x08)
      (libsource (lib conn) (part CONN_01X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D7164F))
    (comp (ref P3)
      (value Digital)
      (footprint Socket_Arduino_Uno:Socket_Strip_Arduino_1x10)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D721E0))
    (comp (ref P9)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A3729))
    (comp (ref Q1)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A446E))
    (comp (ref R3)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4660))
    (comp (ref R1)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A46FA))
    (comp (ref P10)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4D30))
    (comp (ref Q2)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4D48))
    (comp (ref R4)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4D52))
    (comp (ref R2)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4D5E))
    (comp (ref P11)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A504A))
    (comp (ref Q3)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5062))
    (comp (ref R7)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A506C))
    (comp (ref R5)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5078))
    (comp (ref P12)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A525C))
    (comp (ref Q4)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5274))
    (comp (ref R8)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A527E))
    (comp (ref R6)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A528A))
    (comp (ref JP1)
      (value Jumper)
      (footprint Custom_Footprints:Jumper_SMD)
      (libsource (lib device) (part Jumper))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5424))
    (comp (ref JP2)
      (value Jumper)
      (footprint Custom_Footprints:Jumper_SMD)
      (libsource (lib device) (part Jumper))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5726))
    (comp (ref R11)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5AED))
    (comp (ref R12)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5BD5))
    (comp (ref R9)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5DF6))
    (comp (ref R10)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5ECD)))
  (libparts
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01")
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X06)
      (description "Connector, single row, 01x06")
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_01X08)
      (description "Connector, single row, 01x08")
      (footprints
        (fp Pin_Header_Straight_1X08)
        (fp Pin_Header_Angled_1X08)
        (fp Socket_Strip_Straight_1X08)
        (fp Socket_Strip_Angled_1X08))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X08))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib conn) (part CONN_01X10)
      (description "Connector, single row, 01x10")
      (footprints
        (fp Pin_Header_Straight_1X10)
        (fp Pin_Header_Angled_1X10)
        (fp Socket_Strip_Straight_1X10)
        (fp Socket_Strip_Angled_1X10))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X10))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib device) (part Jumper)
      (description "Jumper, generic, normally closed")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part Q_NPN_BEC)
      (description "Transistor NPN (general)")
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NPN_BEC))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib)))
  (nets
    (net (code 1) (name +5V)
      (node (ref JP2) (pin 1))
      (node (ref P1) (pin 5))
      (node (ref JP1) (pin 1))
      (node (ref Q3) (pin 3))
      (node (ref Q2) (pin 3))
      (node (ref Q1) (pin 3))
      (node (ref Q4) (pin 3)))
    (net (code 2) (name GND)
      (node (ref P1) (pin 7))
      (node (ref R3) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref P1) (pin 6))
      (node (ref R11) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref P3) (pin 4)))
    (net (code 3) (name "Net-(Q3-Pad2)")
      (node (ref R5) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref Q3) (pin 2)))
    (net (code 4) (name "Net-(P11-Pad1)")
      (node (ref P11) (pin 10))
      (node (ref R5) (pin 2))
      (node (ref P11) (pin 1)))
    (net (code 5) (name /A2)
      (node (ref Q3) (pin 1))
      (node (ref P2) (pin 3)))
    (net (code 6) (name /8)
      (node (ref P9) (pin 8))
      (node (ref P11) (pin 8))
      (node (ref P3) (pin 10))
      (node (ref P12) (pin 8))
      (node (ref P10) (pin 8)))
    (net (code 7) (name /7)
      (node (ref P4) (pin 1))
      (node (ref P12) (pin 7))
      (node (ref P9) (pin 7))
      (node (ref P11) (pin 7))
      (node (ref P10) (pin 7)))
    (net (code 8) (name /4)
      (node (ref P4) (pin 4))
      (node (ref P9) (pin 4))
      (node (ref P10) (pin 4))
      (node (ref P11) (pin 4))
      (node (ref P12) (pin 4)))
    (net (code 9) (name /2)
      (node (ref P9) (pin 2))
      (node (ref P10) (pin 2))
      (node (ref P4) (pin 6))
      (node (ref P12) (pin 2))
      (node (ref P11) (pin 2)))
    (net (code 10) (name "/3(**)")
      (node (ref P11) (pin 3))
      (node (ref P10) (pin 3))
      (node (ref P12) (pin 3))
      (node (ref P4) (pin 5))
      (node (ref P9) (pin 3)))
    (net (code 11) (name "Net-(Q2-Pad2)")
      (node (ref R4) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref Q2) (pin 2)))
    (net (code 12) (name "Net-(P10-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref P10) (pin 10))
      (node (ref P10) (pin 1)))
    (net (code 13) (name /A1)
      (node (ref Q2) (pin 1))
      (node (ref P2) (pin 2)))
    (net (code 14) (name "/9(**)")
      (node (ref P11) (pin 9))
      (node (ref P9) (pin 9))
      (node (ref P3) (pin 9))
      (node (ref P12) (pin 9))
      (node (ref P10) (pin 9)))
    (net (code 15) (name "/6(**)")
      (node (ref P4) (pin 2))
      (node (ref P9) (pin 6))
      (node (ref P11) (pin 6))
      (node (ref P12) (pin 6))
      (node (ref P10) (pin 6)))
    (net (code 16) (name "/13(SCK)")
      (node (ref P3) (pin 5))
      (node (ref R9) (pin 2)))
    (net (code 17) (name "Net-(JP2-Pad2)")
      (node (ref R12) (pin 1))
      (node (ref R10) (pin 2))
      (node (ref JP2) (pin 2)))
    (net (code 18) (name "/12(MISO)")
      (node (ref P3) (pin 6))
      (node (ref R10) (pin 1)))
    (net (code 19) (name "Net-(JP1-Pad2)")
      (node (ref JP1) (pin 2))
      (node (ref R11) (pin 1))
      (node (ref R9) (pin 1)))
    (net (code 20) (name "/5(**)")
      (node (ref P4) (pin 3))
      (node (ref P11) (pin 5))
      (node (ref P10) (pin 5))
      (node (ref P12) (pin 5))
      (node (ref P9) (pin 5)))
    (net (code 21) (name "Net-(P12-Pad1)")
      (node (ref R6) (pin 2))
      (node (ref P12) (pin 1))
      (node (ref P12) (pin 10)))
    (net (code 22) (name "Net-(Q4-Pad2)")
      (node (ref Q4) (pin 2))
      (node (ref R8) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 23) (name /A3)
      (node (ref Q4) (pin 1))
      (node (ref P2) (pin 4)))
    (net (code 24) (name "Net-(P7-Pad1)")
      (node (ref P7) (pin 1)))
    (net (code 25) (name "Net-(P8-Pad1)")
      (node (ref P8) (pin 1)))
    (net (code 26) (name "Net-(P6-Pad1)")
      (node (ref P6) (pin 1)))
    (net (code 27) (name "Net-(P5-Pad1)")
      (node (ref P5) (pin 1)))
    (net (code 28) (name "/A5(SCL)")
      (node (ref P2) (pin 6))
      (node (ref P3) (pin 1)))
    (net (code 29) (name "/A4(SDA)")
      (node (ref P2) (pin 5))
      (node (ref P3) (pin 2)))
    (net (code 30) (name +3V3)
      (node (ref P1) (pin 4)))
    (net (code 31) (name /Vin)
      (node (ref P1) (pin 8)))
    (net (code 32) (name /IOREF)
      (node (ref P1) (pin 2)))
    (net (code 33) (name "/1(Tx)")
      (node (ref P4) (pin 7)))
    (net (code 34) (name "/11(**/MOSI)")
      (node (ref P3) (pin 7)))
    (net (code 35) (name "/10(**/SS)")
      (node (ref P3) (pin 8)))
    (net (code 36) (name "/0(Rx)")
      (node (ref P4) (pin 8)))
    (net (code 37) (name /Reset)
      (node (ref P1) (pin 3)))
    (net (code 38) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1)))
    (net (code 39) (name /AREF)
      (node (ref P3) (pin 3)))
    (net (code 40) (name "Net-(P9-Pad1)")
      (node (ref P9) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref P9) (pin 10)))
    (net (code 41) (name "Net-(Q1-Pad2)")
      (node (ref Q1) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 42) (name /A0)
      (node (ref Q1) (pin 1))
      (node (ref P2) (pin 1)))))