(export (version D)
  (design
    (source /home/isthatme/kicad-projects/stm32f030-eth/stm32f030-eth.sch)
    (date "Thu 23 Mar 2017 09:16:57 PM MDT")
    (tool "Eeschema 4.0.6-e0-6349~53~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source stm32f030-eth.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P1)
      (value CONN_01X06)
      (footprint Socket_Strips:Socket_Strip_Straight_1x06)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FD838))
    (comp (ref Y1)
      (value Crystal)
      (footprint Crystals:Crystal_SMD_HC49-SD_HandSoldering)
      (libsource (lib device) (part Crystal))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FDB39))
    (comp (ref C1)
      (value C_Small)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FDCD1))
    (comp (ref C2)
      (value C_Small)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FDD2E))
    (comp (ref CON1)
      (value Micro_SD_Card)
      (footprint microSD:microSD-5031821852)
      (libsource (lib conn) (part Micro_SD_Card))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FDFA5))
    (comp (ref P2)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FEC3B))
    (comp (ref P3)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FEC8C))
    (comp (ref P6)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FECCF))
    (comp (ref P7)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FED11))
    (comp (ref P4)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF13E))
    (comp (ref P5)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF18C))
    (comp (ref P9)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF465))
    (comp (ref P10)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF4A8))
    (comp (ref P8)
      (value CONN_01X08)
      (footprint Socket_Strips:Socket_Strip_Straight_1x08)
      (libsource (lib conn) (part CONN_01X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 589FF52C))
    (comp (ref P11)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A00A91))
    (comp (ref P12)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A00AF5))
    (comp (ref U2)
      (value LD3985M)
      (footprint TO_SOT_Packages_SMD:SOT-23-5)
      (libsource (lib regul) (part LD3985M))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A00B5D))
    (comp (ref C4)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A019C0))
    (comp (ref C3)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A01A5B))
    (comp (ref U4)
      (value W5500)
      (footprint Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm)
      (libsource (lib w5500) (part W5500))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0AE89))
    (comp (ref P13)
      (value CONN_01X02)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0B8A2))
    (comp (ref U3)
      (value LD3985M)
      (footprint TO_SOT_Packages_SMD:SOT-23-5)
      (libsource (lib regul) (part LD3985M))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0B8A8))
    (comp (ref C6)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0B8C3))
    (comp (ref C5)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0B8C9))
    (comp (ref R2)
      (value 12K4)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0D138))
    (comp (ref C9)
      (value 4.7uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0D506))
    (comp (ref Y2)
      (value 25MHz)
      (footprint Crystals:Crystal_SMD_HC49-SD_HandSoldering)
      (libsource (lib device) (part Crystal))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0DA0B))
    (comp (ref R1)
      (value 1M)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0DCD2))
    (comp (ref C8)
      (value 18uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0DE5E))
    (comp (ref C7)
      (value 18uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0DED1))
    (comp (ref D4)
      (value LED)
      (footprint LEDs:LED_0805)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0E73C))
    (comp (ref D2)
      (value LED)
      (footprint LEDs:LED_0805)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0E8BB))
    (comp (ref R5)
      (value 499)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0F1DD))
    (comp (ref R3)
      (value 390K)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0F313))
    (comp (ref R6)
      (value 499)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A0F452))
    (comp (ref JP1)
      (value Jumper_NO_Small)
      (footprint Custom_Footprints:Jumper_SMD)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A1267E))
    (comp (ref JP2)
      (value Jumper_NO_Small)
      (footprint Custom_Footprints:Jumper_SMD)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A1276F))
    (comp (ref JP3)
      (value Jumper_NO_Small)
      (footprint Custom_Footprints:Jumper_SMD)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A12AAE))
    (comp (ref C11)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A15447))
    (comp (ref C12)
      (value 0.1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A15595))
    (comp (ref R9)
      (value 49R9)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A15C52))
    (comp (ref R10)
      (value 49R9)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A1602A))
    (comp (ref U1)
      (value STM32F030R8T6)
      (footprint Housings_QFP:LQFP-64_10x10mm_Pitch0.5mm)
      (libsource (lib stm32f030r8t6) (part STM32F030R8T6))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A128EE))
    (comp (ref P14)
      (value CNT-RJ45)
      (footprint Custom_Footprints:8p8c-RB1-125BAG1A)
      (libsource (lib conn) (part CNT-RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A1CB56))
    (comp (ref R4)
      (value 390K)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A1EBE9))
    (comp (ref R7)
      (value 49R9)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A1FB24))
    (comp (ref R8)
      (value 49R9)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 58A1FC32))
    (comp (ref SW1)
      (value SW_Push)
      (footprint Buttons_Switches_SMD:SW_SPST_B3S-1000)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 58D48FFE))
    (comp (ref C10)
      (value 0.1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 58D4933D)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CNT-RJ45)
      (description " RJ-45 with LEDs and shield")
      (fields
        (field (name Reference) P)
        (field (name Value) CNT-RJ45))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X06)
      (description "Connector, single row, 01x06")
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_01X08)
      (description "Connector, single row, 01x08")
      (footprints
        (fp Pin_Header_Straight_1X08)
        (fp Pin_Header_Angled_1X08)
        (fp Socket_Strip_Straight_1X08)
        (fp Socket_Strip_Angled_1X08))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X08))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Crystal)
      (description "Two pin crystal")
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part Jumper_NO_Small)
      (description "Jumper, normally open")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib regul) (part LD3985M)
      (description "150 mA Low Dropout Voltage Regulator")
      (docs http://www.st.com/internet/analog/product/69230.jsp)
      (fields
        (field (name Reference) U)
        (field (name Value) LD3985M)
        (field (name Footprint) SOT-23-5))
      (pins
        (pin (num 1) (name VIN) (type input))
        (pin (num 2) (name GND) (type input))
        (pin (num 3) (name INH) (type input))
        (pin (num 4) (name BYP) (type input))
        (pin (num 5) (name VOUT) (type input))))
    (libpart (lib device) (part LED)
      (description "LED generic")
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib conn) (part Micro_SD_Card)
      (description "Micro SD Card Socket")
      (docs http://katalog.we-online.de/em/datasheet/693072010801.pdf)
      (fields
        (field (name Reference) CON)
        (field (name Value) Micro_SD_Card))
      (pins
        (pin (num 1) (name DAT2) (type BiDi))
        (pin (num 2) (name DAT3/CD) (type BiDi))
        (pin (num 3) (name CMD) (type input))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type power_in))
        (pin (num 7) (name DAT0) (type input))
        (pin (num 8) (name DAT1) (type input))
        (pin (num 9) (name SHIELD) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32f030r8t6) (part STM32F030R8T6)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F030R8T6))
      (pins
        (pin (num 1) (name Vdd) (type power_in))
        (pin (num 2) (name PC13) (type BiDi))
        (pin (num 3) (name PC14) (type BiDi))
        (pin (num 4) (name PC15) (type BiDi))
        (pin (num 5) (name PF0/OSC_IN) (type power_in))
        (pin (num 6) (name PF1/OSC_OUT) (type power_in))
        (pin (num 7) (name NRST) (type input))
        (pin (num 8) (name PC0) (type BiDi))
        (pin (num 9) (name PC1) (type BiDi))
        (pin (num 10) (name PC2) (type BiDi))
        (pin (num 11) (name PC3) (type BiDi))
        (pin (num 12) (name Vssa) (type power_in))
        (pin (num 13) (name Vdda) (type power_in))
        (pin (num 14) (name PA0) (type BiDi))
        (pin (num 15) (name PA1) (type BiDi))
        (pin (num 16) (name PA2) (type BiDi))
        (pin (num 17) (name PA3) (type BiDi))
        (pin (num 18) (name PF4) (type BiDi))
        (pin (num 19) (name PF5) (type BiDi))
        (pin (num 20) (name PA4) (type BiDi))
        (pin (num 21) (name PA5) (type BiDi))
        (pin (num 22) (name PA6) (type BiDi))
        (pin (num 23) (name PA7) (type BiDi))
        (pin (num 24) (name PC4) (type BiDi))
        (pin (num 25) (name PC5) (type BiDi))
        (pin (num 26) (name PB0) (type BiDi))
        (pin (num 27) (name PB1) (type BiDi))
        (pin (num 28) (name PB2) (type BiDi))
        (pin (num 29) (name PB10) (type BiDi))
        (pin (num 30) (name PB11) (type BiDi))
        (pin (num 31) (name Vss) (type power_in))
        (pin (num 32) (name Vdd) (type power_in))
        (pin (num 33) (name PB12) (type BiDi))
        (pin (num 34) (name PB13) (type BiDi))
        (pin (num 35) (name PB14) (type BiDi))
        (pin (num 36) (name PB15) (type BiDi))
        (pin (num 37) (name PC6) (type BiDi))
        (pin (num 38) (name PC7) (type BiDi))
        (pin (num 39) (name PC8) (type BiDi))
        (pin (num 40) (name PC9) (type BiDi))
        (pin (num 41) (name PA8) (type BiDi))
        (pin (num 42) (name PA9) (type BiDi))
        (pin (num 43) (name PA10) (type BiDi))
        (pin (num 44) (name PA11) (type BiDi))
        (pin (num 45) (name PA12) (type BiDi))
        (pin (num 46) (name PA13/SWDIO) (type BiDi))
        (pin (num 47) (name PF6) (type BiDi))
        (pin (num 48) (name PF7) (type BiDi))
        (pin (num 49) (name PA14/SWCLK) (type BiDi))
        (pin (num 50) (name PA15) (type BiDi))
        (pin (num 51) (name PC10) (type BiDi))
        (pin (num 52) (name PC11) (type BiDi))
        (pin (num 53) (name PC12) (type BiDi))
        (pin (num 54) (name PD2) (type BiDi))
        (pin (num 55) (name PB3) (type BiDi))
        (pin (num 56) (name PB4) (type BiDi))
        (pin (num 57) (name PB5) (type BiDi))
        (pin (num 58) (name PB6) (type BiDi))
        (pin (num 59) (name PB7) (type BiDi))
        (pin (num 60) (name BOOT0) (type input))
        (pin (num 61) (name PB8) (type BiDi))
        (pin (num 62) (name PB9) (type BiDi))
        (pin (num 63) (name Vss) (type power_in))
        (pin (num 64) (name Vdd) (type power_in))))
    (libpart (lib switches) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib w5500) (part W5500)
      (fields
        (field (name Reference) U)
        (field (name Value) W5500))
      (pins
        (pin (num 1) (name TXN) (type output))
        (pin (num 2) (name TXP) (type output))
        (pin (num 3) (name AGND) (type power_in))
        (pin (num 4) (name AVDD) (type power_in))
        (pin (num 5) (name RXN) (type input))
        (pin (num 6) (name RXP) (type input))
        (pin (num 7) (name DNC) (type BiDi))
        (pin (num 8) (name AVDD) (type power_in))
        (pin (num 9) (name AGND) (type power_in))
        (pin (num 10) (name EXRES1) (type passive))
        (pin (num 11) (name AVDD) (type power_in))
        (pin (num 12) (name ~) (type NotConnected))
        (pin (num 13) (name ~) (type NotConnected))
        (pin (num 14) (name AGND) (type power_in))
        (pin (num 15) (name AVDD) (type power_in))
        (pin (num 16) (name AGND) (type power_in))
        (pin (num 17) (name AVDD) (type power_in))
        (pin (num 18) (name VBG) (type NotConnected))
        (pin (num 19) (name AGND) (type power_in))
        (pin (num 20) (name TOCAP) (type passive))
        (pin (num 21) (name AVDD) (type power_in))
        (pin (num 22) (name 1V2O) (type power_out))
        (pin (num 23) (name RSVD) (type input))
        (pin (num 24) (name SPDLED) (type output))
        (pin (num 25) (name LINKLED) (type output))
        (pin (num 26) (name DUPLED) (type output))
        (pin (num 27) (name ACTLED) (type output))
        (pin (num 28) (name VDD) (type power_in))
        (pin (num 29) (name GND) (type power_in))
        (pin (num 30) (name XI) (type input))
        (pin (num 31) (name XO) (type output))
        (pin (num 32) (name SCSn) (type input))
        (pin (num 33) (name SCLK) (type input))
        (pin (num 34) (name MISO) (type input))
        (pin (num 35) (name MOSI) (type input))
        (pin (num 36) (name INTn) (type output))
        (pin (num 37) (name RSTn) (type input))
        (pin (num 38) (name RSVD) (type NotConnected))
        (pin (num 39) (name RSVD) (type NotConnected))
        (pin (num 40) (name RSVD) (type NotConnected))
        (pin (num 41) (name RSVD) (type NotConnected))
        (pin (num 42) (name RSVD) (type NotConnected))
        (pin (num 43) (name PMODE2) (type input))
        (pin (num 44) (name PMODE1) (type input))
        (pin (num 45) (name PMODE0) (type input))
        (pin (num 46) (name ~) (type NotConnected))
        (pin (num 47) (name ~) (type NotConnected))
        (pin (num 48) (name AGND) (type power_in)))))
  (libraries
    (library (logical stm32f030r8t6)
      (uri /home/isthatme/kicad-projects/Custom-Parts/stm32f030r8t6.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical regul)
      (uri /usr/share/kicad/library/regul.lib))
    (library (logical w5500)
      (uri /home/isthatme/kicad-projects/Custom-Parts/w5500.lib))
    (library (logical switches)
      (uri /usr/share/kicad/library/switches.lib)))
  (nets
    (net (code 1) (name "Net-(U1-Pad62)")
      (node (ref U1) (pin 62)))
    (net (code 2) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30)))
    (net (code 3) (name "Net-(U1-Pad61)")
      (node (ref U1) (pin 61)))
    (net (code 4) (name "Net-(U1-Pad33)")
      (node (ref U1) (pin 33)))
    (net (code 5) (name "Net-(U1-Pad59)")
      (node (ref U1) (pin 59)))
    (net (code 6) (name "Net-(U1-Pad29)")
      (node (ref U1) (pin 29)))
    (net (code 7) (name "Net-(U1-Pad55)")
      (node (ref U1) (pin 55)))
    (net (code 9) (name "Net-(U1-Pad56)")
      (node (ref U1) (pin 56)))
    (net (code 10) (name "Net-(U1-Pad28)")
      (node (ref U1) (pin 28)))
    (net (code 12) (name "Net-(R2-Pad1)")
      (node (ref U4) (pin 10))
      (node (ref R2) (pin 1)))
    (net (code 13) (name /PMODE2)
      (node (ref JP3) (pin 2))
      (node (ref U4) (pin 43)))
    (net (code 14) (name /PMODE1)
      (node (ref U4) (pin 44))
      (node (ref JP2) (pin 2)))
    (net (code 15) (name /PMODE0)
      (node (ref U4) (pin 45))
      (node (ref JP1) (pin 2)))
    (net (code 16) (name "Net-(D4-Pad2)")
      (node (ref D4) (pin 2))
      (node (ref R5) (pin 2)))
    (net (code 17) (name "Net-(R3-Pad1)")
      (node (ref R3) (pin 1))
      (node (ref U4) (pin 25)))
    (net (code 18) (name "Net-(R4-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref U4) (pin 27)))
    (net (code 19) (name "Net-(P14-Pad11)")
      (node (ref P14) (pin 11))
      (node (ref R3) (pin 2)))
    (net (code 20) (name "Net-(D2-Pad2)")
      (node (ref R6) (pin 2))
      (node (ref D2) (pin 2)))
    (net (code 21) (name "Net-(P14-Pad13)")
      (node (ref R4) (pin 2))
      (node (ref P14) (pin 13)))
    (net (code 22) (name "Net-(P14-Pad4)")
      (node (ref P14) (pin 4)))
    (net (code 23) (name "Net-(P14-Pad5)")
      (node (ref P14) (pin 5)))
    (net (code 24) (name "Net-(P14-Pad6)")
      (node (ref P14) (pin 6)))
    (net (code 25) (name +Vdd)
      (node (ref P1) (pin 1))
      (node (ref P12) (pin 1))
      (node (ref CON1) (pin 4))
      (node (ref C12) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref U1) (pin 48))
      (node (ref P14) (pin 3))
      (node (ref C11) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref U2) (pin 5))
      (node (ref C4) (pin 1))
      (node (ref U4) (pin 28))
      (node (ref U1) (pin 13))
      (node (ref U1) (pin 32))
      (node (ref U1) (pin 64))
      (node (ref U1) (pin 1)))
    (net (code 26) (name /STM32-OI)
      (node (ref U1) (pin 5))
      (node (ref C2) (pin 2)))
    (net (code 27) (name /STM32-OO)
      (node (ref U1) (pin 6))
      (node (ref C1) (pin 2)))
    (net (code 28) (name /NRST)
      (node (ref SW1) (pin 2))
      (node (ref U1) (pin 7))
      (node (ref P1) (pin 4))
      (node (ref C10) (pin 1)))
    (net (code 29) (name "Net-(U1-Pad60)")
      (node (ref U1) (pin 60)))
    (net (code 30) (name /RX+)
      (node (ref R7) (pin 2))
      (node (ref P14) (pin 7))
      (node (ref U4) (pin 6)))
    (net (code 31) (name /RX-)
      (node (ref U4) (pin 5))
      (node (ref P14) (pin 8))
      (node (ref R8) (pin 2)))
    (net (code 32) (name /TX+)
      (node (ref R10) (pin 2))
      (node (ref P14) (pin 1))
      (node (ref U4) (pin 2)))
    (net (code 33) (name /TX-)
      (node (ref P14) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref U4) (pin 1)))
    (net (code 34) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 35) (name /+12V-Digital)
      (node (ref U2) (pin 1))
      (node (ref P11) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 36) (name "Net-(R6-Pad1)")
      (node (ref U4) (pin 26))
      (node (ref R6) (pin 1)))
    (net (code 37) (name "Net-(U4-Pad18)")
      (node (ref U4) (pin 18)))
    (net (code 38) (name "Net-(U4-Pad40)")
      (node (ref U4) (pin 40)))
    (net (code 39) (name "Net-(U4-Pad41)")
      (node (ref U4) (pin 41)))
    (net (code 40) (name "Net-(U4-Pad42)")
      (node (ref U4) (pin 42)))
    (net (code 41) (name "Net-(U4-Pad7)")
      (node (ref U4) (pin 7)))
    (net (code 42) (name AGND)
      (node (ref P12) (pin 2))
      (node (ref P11) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref U4) (pin 29))
      (node (ref U4) (pin 16))
      (node (ref C6) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref JP1) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref D2) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref P8) (pin 7))
      (node (ref U4) (pin 3))
      (node (ref P13) (pin 2))
      (node (ref P8) (pin 5))
      (node (ref P6) (pin 2))
      (node (ref P8) (pin 8))
      (node (ref JP2) (pin 1))
      (node (ref U4) (pin 14))
      (node (ref P5) (pin 2))
      (node (ref CON1) (pin 9))
      (node (ref P4) (pin 2))
      (node (ref CON1) (pin 6))
      (node (ref P7) (pin 2))
      (node (ref P3) (pin 2))
      (node (ref P1) (pin 6))
      (node (ref P2) (pin 2))
      (node (ref P1) (pin 5))
      (node (ref U4) (pin 48))
      (node (ref U4) (pin 19))
      (node (ref P8) (pin 6))
      (node (ref U4) (pin 9))
      (node (ref JP3) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref C12) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref U1) (pin 31))
      (node (ref U1) (pin 12))
      (node (ref U1) (pin 63))
      (node (ref U1) (pin 47))
      (node (ref P14) (pin 12))
      (node (ref P14) (pin 14))
      (node (ref P14) (pin 10))
      (node (ref U2) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref P14) (pin 9)))
    (net (code 43) (name "Net-(C9-Pad1)")
      (node (ref U4) (pin 20))
      (node (ref C9) (pin 1)))
    (net (code 44) (name "Net-(U4-Pad12)")
      (node (ref U4) (pin 12)))
    (net (code 45) (name "Net-(U4-Pad22)")
      (node (ref U4) (pin 22)))
    (net (code 46) (name "Net-(U4-Pad13)")
      (node (ref U4) (pin 13)))
    (net (code 47) (name "Net-(U4-Pad23)")
      (node (ref U4) (pin 23)))
    (net (code 48) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref U4) (pin 24)))
    (net (code 49) (name "Net-(CON1-Pad1)")
      (node (ref CON1) (pin 1)))
    (net (code 50) (name /SPI1_CS1)
      (node (ref U1) (pin 57))
      (node (ref CON1) (pin 2)))
    (net (code 51) (name "Net-(CON1-Pad8)")
      (node (ref CON1) (pin 8)))
    (net (code 52) (name /SPI1_CLK)
      (node (ref CON1) (pin 5))
      (node (ref U4) (pin 33))
      (node (ref U1) (pin 34)))
    (net (code 53) (name /SPI1_MISO)
      (node (ref U4) (pin 34))
      (node (ref U1) (pin 35))
      (node (ref CON1) (pin 7)))
    (net (code 54) (name /SPI1_MOSI)
      (node (ref CON1) (pin 3))
      (node (ref U1) (pin 36))
      (node (ref U4) (pin 35)))
    (net (code 55) (name "Net-(C1-Pad1)")
      (node (ref Y1) (pin 2))
      (node (ref C1) (pin 1)))
    (net (code 56) (name "Net-(C2-Pad1)")
      (node (ref Y1) (pin 1))
      (node (ref C2) (pin 1)))
    (net (code 57) (name /I2C2_SDA)
      (node (ref U1) (pin 45))
      (node (ref P10) (pin 2)))
    (net (code 58) (name "Net-(P8-Pad1)")
      (node (ref P8) (pin 1))
      (node (ref U1) (pin 22)))
    (net (code 59) (name "Net-(P8-Pad2)")
      (node (ref P8) (pin 2))
      (node (ref U1) (pin 23)))
    (net (code 60) (name "Net-(P8-Pad3)")
      (node (ref P8) (pin 3))
      (node (ref U1) (pin 41)))
    (net (code 61) (name "Net-(P8-Pad4)")
      (node (ref P8) (pin 4))
      (node (ref U1) (pin 50)))
    (net (code 62) (name /I2C1_SDA)
      (node (ref U1) (pin 43))
      (node (ref P9) (pin 2)))
    (net (code 63) (name /I2C2_SCL)
      (node (ref U1) (pin 44))
      (node (ref P10) (pin 1)))
    (net (code 64) (name "Net-(P6-Pad1)")
      (node (ref U1) (pin 20))
      (node (ref P6) (pin 1)))
    (net (code 65) (name /SWDIO)
      (node (ref P1) (pin 2))
      (node (ref U1) (pin 46)))
    (net (code 66) (name /SWCLK)
      (node (ref U1) (pin 49))
      (node (ref P1) (pin 3)))
    (net (code 67) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1))
      (node (ref U1) (pin 14)))
    (net (code 68) (name "Net-(P3-Pad1)")
      (node (ref U1) (pin 15))
      (node (ref P3) (pin 1)))
    (net (code 69) (name "Net-(P7-Pad1)")
      (node (ref U1) (pin 21))
      (node (ref P7) (pin 1)))
    (net (code 70) (name "Net-(P4-Pad1)")
      (node (ref U1) (pin 16))
      (node (ref P4) (pin 1)))
    (net (code 71) (name "Net-(P5-Pad1)")
      (node (ref U1) (pin 17))
      (node (ref P5) (pin 1)))
    (net (code 72) (name /I2C1_SCL)
      (node (ref P9) (pin 1))
      (node (ref U1) (pin 42)))
    (net (code 73) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 74) (name +AVdd)
      (node (ref U4) (pin 17))
      (node (ref U4) (pin 21))
      (node (ref U4) (pin 4))
      (node (ref U4) (pin 8))
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 15))
      (node (ref U3) (pin 5))
      (node (ref C6) (pin 1)))
    (net (code 75) (name /+12V-Analog)
      (node (ref P13) (pin 1))
      (node (ref U3) (pin 3))
      (node (ref U3) (pin 1))
      (node (ref C5) (pin 1)))
    (net (code 76) (name "Net-(U4-Pad47)")
      (node (ref U4) (pin 47)))
    (net (code 77) (name "Net-(U4-Pad46)")
      (node (ref U4) (pin 46)))
    (net (code 78) (name "Net-(U4-Pad38)")
      (node (ref U4) (pin 38)))
    (net (code 79) (name "Net-(U4-Pad39)")
      (node (ref U4) (pin 39)))
    (net (code 80) (name /SPI1_CS2)
      (node (ref U4) (pin 32))
      (node (ref U1) (pin 58)))
    (net (code 81) (name /W5500_RST)
      (node (ref U4) (pin 37))
      (node (ref U1) (pin 26)))
    (net (code 82) (name /W5500_INT)
      (node (ref U1) (pin 27))
      (node (ref U4) (pin 36)))
    (net (code 83) (name "Net-(C7-Pad1)")
      (node (ref U4) (pin 30))
      (node (ref C7) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref Y2) (pin 1)))
    (net (code 84) (name "Net-(C8-Pad1)")
      (node (ref R1) (pin 2))
      (node (ref C8) (pin 1))
      (node (ref U4) (pin 31))
      (node (ref Y2) (pin 2)))))