(export (version D)
  (design
    (source C:/Users/David/Documents/kicad-projects/Uno-Switch-Shield/Uno-Switch-Shield.sch)
    (date "2017-12-02 9:28:57 PM")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date "lun. 30 mars 2015")
        (source Uno-Switch-Shield.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P1)
      (value Power)
      (footprint Socket_Arduino_Uno:Socket_Strip_Arduino_1x08)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D70129))
    (comp (ref P2)
      (value Analog)
      (footprint Socket_Arduino_Uno:Socket_Strip_Arduino_1x06)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D70DD8))
    (comp (ref P5)
      (value CONN_01X01)
      (footprint Socket_Arduino_Uno:Arduino_1pin)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D71177))
    (comp (ref P6)
      (value CONN_01X01)
      (footprint Socket_Arduino_Uno:Arduino_1pin)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D71274))
    (comp (ref P7)
      (value CONN_01X01)
      (footprint Socket_Arduino_Uno:Arduino_1pin)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D712A8))
    (comp (ref P8)
      (value CONN_01X01)
      (footprint Socket_Arduino_Uno:Arduino_1pin)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D712DB))
    (comp (ref P4)
      (value Digital)
      (footprint Socket_Arduino_Uno:Socket_Strip_Arduino_1x08)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D7164F))
    (comp (ref P3)
      (value Digital)
      (footprint Socket_Arduino_Uno:Socket_Strip_Arduino_1x10)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 56D721E0))
    (comp (ref P9)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10_Pitch2.54mm)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A3729))
    (comp (ref Q1)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A446E))
    (comp (ref R3)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4660))
    (comp (ref R1)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A46FA))
    (comp (ref P10)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10_Pitch2.54mm)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4D30))
    (comp (ref Q2)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4D48))
    (comp (ref R4)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4D52))
    (comp (ref R2)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A4D5E))
    (comp (ref P11)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10_Pitch2.54mm)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A504A))
    (comp (ref Q3)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5062))
    (comp (ref R7)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A506C))
    (comp (ref R5)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5078))
    (comp (ref P12)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10_Pitch2.54mm)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A525C))
    (comp (ref Q4)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5274))
    (comp (ref R8)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A527E))
    (comp (ref R6)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A528A))
    (comp (ref JP1)
      (value Jumper)
      (footprint Custom_Footprints:Jumper_SMD)
      (libsource (lib device) (part Jumper))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5424))
    (comp (ref JP2)
      (value Jumper)
      (footprint Custom_Footprints:Jumper_SMD)
      (libsource (lib device) (part Jumper))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5726))
    (comp (ref R11)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5AED))
    (comp (ref R12)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5BD5))
    (comp (ref R9)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5DF6))
    (comp (ref R10)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 597A5ECD))
    (comp (ref P13)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10_Pitch2.54mm)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A222B25))
    (comp (ref Q5)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A222B38))
    (comp (ref R15)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A222B41))
    (comp (ref R13)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A222B4D))
    (comp (ref P14)
      (value CONN_01X10)
      (footprint Socket_Strips:Socket_Strip_Straight_1x10_Pitch2.54mm)
      (libsource (lib Uno-Switch-Shield-cache) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A222B5D))
    (comp (ref Q6)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NPN_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A222B70))
    (comp (ref R16)
      (value 10K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A222B79))
    (comp (ref R14)
      (value 1K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A222B85)))
  (libparts
    (libpart (lib Uno-Switch-Shield-cache) (part CONN_01X01)
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib Uno-Switch-Shield-cache) (part CONN_01X06)
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib Uno-Switch-Shield-cache) (part CONN_01X08)
      (footprints
        (fp Pin_Header_Straight_1X08)
        (fp Pin_Header_Angled_1X08)
        (fp Socket_Strip_Straight_1X08)
        (fp Socket_Strip_Angled_1X08))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X08))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib Uno-Switch-Shield-cache) (part CONN_01X10)
      (footprints
        (fp Pin_Header_Straight_1X10)
        (fp Pin_Header_Angled_1X10)
        (fp Socket_Strip_Straight_1X10)
        (fp Socket_Strip_Angled_1X10))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X10))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib device) (part Jumper)
      (description "Jumper, generic, normally closed")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part Q_NPN_BEC)
      (description "Transistor NPN (general)")
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NPN_BEC))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical Uno-Switch-Shield-cache)
      (uri C:\Users\David\Documents\kicad-projects\Uno-Switch-Shield\Uno-Switch-Shield-cache.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref R4) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref P1) (pin 6))
      (node (ref P1) (pin 7))
      (node (ref R16) (pin 2))
      (node (ref P3) (pin 4))
      (node (ref R11) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref R12) (pin 2)))
    (net (code 2) (name "Net-(JP2-Pad2)")
      (node (ref R10) (pin 2))
      (node (ref R12) (pin 1))
      (node (ref JP2) (pin 2)))
    (net (code 3) (name "/12(MISO)")
      (node (ref R10) (pin 1))
      (node (ref P3) (pin 6)))
    (net (code 4) (name "/13(SCK)")
      (node (ref R9) (pin 2))
      (node (ref P3) (pin 5)))
    (net (code 5) (name "Net-(JP1-Pad2)")
      (node (ref JP1) (pin 2))
      (node (ref R9) (pin 1))
      (node (ref R11) (pin 1)))
    (net (code 6) (name +5V)
      (node (ref Q6) (pin 3))
      (node (ref Q3) (pin 3))
      (node (ref Q4) (pin 3))
      (node (ref Q5) (pin 3))
      (node (ref P1) (pin 5))
      (node (ref Q2) (pin 3))
      (node (ref Q1) (pin 3))
      (node (ref JP1) (pin 1))
      (node (ref JP2) (pin 1)))
    (net (code 7) (name "Net-(P11-Pad1)")
      (node (ref P11) (pin 10))
      (node (ref P11) (pin 1))
      (node (ref R5) (pin 2)))
    (net (code 8) (name "/6(**)")
      (node (ref P10) (pin 6))
      (node (ref P12) (pin 6))
      (node (ref P14) (pin 6))
      (node (ref P4) (pin 2))
      (node (ref P9) (pin 6))
      (node (ref P13) (pin 6))
      (node (ref P11) (pin 6)))
    (net (code 9) (name "/9(**)")
      (node (ref P14) (pin 9))
      (node (ref P10) (pin 9))
      (node (ref P9) (pin 9))
      (node (ref P13) (pin 9))
      (node (ref P12) (pin 9))
      (node (ref P3) (pin 9))
      (node (ref P11) (pin 9)))
    (net (code 10) (name "Net-(P12-Pad1)")
      (node (ref P12) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref P12) (pin 10)))
    (net (code 11) (name "Net-(P9-Pad1)")
      (node (ref R1) (pin 2))
      (node (ref P9) (pin 10))
      (node (ref P9) (pin 1)))
    (net (code 12) (name /2)
      (node (ref P10) (pin 2))
      (node (ref P13) (pin 2))
      (node (ref P14) (pin 2))
      (node (ref P9) (pin 2))
      (node (ref P4) (pin 6))
      (node (ref P12) (pin 2))
      (node (ref P11) (pin 2)))
    (net (code 13) (name "Net-(Q3-Pad2)")
      (node (ref Q3) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref R5) (pin 1)))
    (net (code 14) (name "Net-(Q4-Pad2)")
      (node (ref Q4) (pin 2))
      (node (ref R6) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 15) (name /A3)
      (node (ref P2) (pin 4))
      (node (ref Q4) (pin 1)))
    (net (code 16) (name /8)
      (node (ref P11) (pin 8))
      (node (ref P9) (pin 8))
      (node (ref P13) (pin 8))
      (node (ref P10) (pin 8))
      (node (ref P14) (pin 8))
      (node (ref P12) (pin 8))
      (node (ref P3) (pin 10)))
    (net (code 17) (name /7)
      (node (ref P9) (pin 7))
      (node (ref P11) (pin 7))
      (node (ref P10) (pin 7))
      (node (ref P4) (pin 1))
      (node (ref P13) (pin 7))
      (node (ref P14) (pin 7))
      (node (ref P12) (pin 7)))
    (net (code 18) (name /4)
      (node (ref P10) (pin 4))
      (node (ref P14) (pin 4))
      (node (ref P12) (pin 4))
      (node (ref P13) (pin 4))
      (node (ref P9) (pin 4))
      (node (ref P4) (pin 4))
      (node (ref P11) (pin 4)))
    (net (code 19) (name "Net-(Q6-Pad2)")
      (node (ref Q6) (pin 2))
      (node (ref R14) (pin 1))
      (node (ref R16) (pin 1)))
    (net (code 20) (name "/A5(SCL)")
      (node (ref P2) (pin 6))
      (node (ref Q6) (pin 1)))
    (net (code 21) (name "/3(**)")
      (node (ref P9) (pin 3))
      (node (ref P13) (pin 3))
      (node (ref P4) (pin 5))
      (node (ref P11) (pin 3))
      (node (ref P14) (pin 3))
      (node (ref P12) (pin 3))
      (node (ref P10) (pin 3)))
    (net (code 22) (name "Net-(P13-Pad1)")
      (node (ref P13) (pin 10))
      (node (ref P13) (pin 1))
      (node (ref R13) (pin 2)))
    (net (code 23) (name "Net-(P3-Pad2)")
      (node (ref P3) (pin 2)))
    (net (code 24) (name "Net-(P14-Pad1)")
      (node (ref R14) (pin 2))
      (node (ref P14) (pin 10))
      (node (ref P14) (pin 1)))
    (net (code 25) (name "/5(**)")
      (node (ref P9) (pin 5))
      (node (ref P14) (pin 5))
      (node (ref P4) (pin 3))
      (node (ref P11) (pin 5))
      (node (ref P10) (pin 5))
      (node (ref P13) (pin 5))
      (node (ref P12) (pin 5)))
    (net (code 26) (name "Net-(Q5-Pad2)")
      (node (ref R13) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref Q5) (pin 2)))
    (net (code 27) (name "/A4(SDA)")
      (node (ref Q5) (pin 1))
      (node (ref P2) (pin 5)))
    (net (code 28) (name +3V3)
      (node (ref P1) (pin 4)))
    (net (code 29) (name /Vin)
      (node (ref P1) (pin 8)))
    (net (code 30) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1)))
    (net (code 31) (name /IOREF)
      (node (ref P1) (pin 2)))
    (net (code 32) (name "/0(Rx)")
      (node (ref P4) (pin 8)))
    (net (code 33) (name "/1(Tx)")
      (node (ref P4) (pin 7)))
    (net (code 34) (name "Net-(P8-Pad1)")
      (node (ref P8) (pin 1)))
    (net (code 35) (name "/11(**/MOSI)")
      (node (ref P3) (pin 7)))
    (net (code 36) (name /AREF)
      (node (ref P3) (pin 3)))
    (net (code 37) (name "Net-(P7-Pad1)")
      (node (ref P7) (pin 1)))
    (net (code 38) (name "/10(**/SS)")
      (node (ref P3) (pin 8)))
    (net (code 39) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1)))
    (net (code 40) (name "Net-(P6-Pad1)")
      (node (ref P6) (pin 1)))
    (net (code 41) (name "Net-(P5-Pad1)")
      (node (ref P5) (pin 1)))
    (net (code 42) (name /Reset)
      (node (ref P1) (pin 3)))
    (net (code 43) (name /A1)
      (node (ref P2) (pin 2))
      (node (ref Q2) (pin 1)))
    (net (code 44) (name "Net-(Q2-Pad2)")
      (node (ref Q2) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 45) (name "Net-(P10-Pad1)")
      (node (ref P10) (pin 1))
      (node (ref P10) (pin 10))
      (node (ref R2) (pin 2)))
    (net (code 46) (name /A2)
      (node (ref P2) (pin 3))
      (node (ref Q3) (pin 1)))
    (net (code 47) (name /A0)
      (node (ref P2) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 48) (name "Net-(Q1-Pad2)")
      (node (ref R1) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref Q1) (pin 2)))))