(export (version D)
  (design
    (source /home/isthatme/Documents/kicad-projects/AC-LED-Control/AC-LED-Control.sch)
    (date "Wed 11 Jul 2018 03:19:06 PM MDT")
    (tool "Eeschema 4.0.2+dfsg1-stable")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source AC-LED-Control.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /Output-BankA/) (tstamps /5B46698C/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Output-BankB.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /Output-BankB/) (tstamps /5B477E02/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Output-BankB.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U102)
      (value STM32F030F4P6)
      (footprint Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm)
      (libsource (lib stm32f030f4p6) (part STM32F030F4P6))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B453204))
    (comp (ref P101)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B453C99))
    (comp (ref P102)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B453DC6))
    (comp (ref R104)
      (value 2K)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B453F03))
    (comp (ref R105)
      (value 2K)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B453F30))
    (comp (ref C101)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B454AFF))
    (comp (ref C103)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B454B6E))
    (comp (ref C105)
      (value 4.7uF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B454BFE))
    (comp (ref C102)
      (value 10nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B454E7E))
    (comp (ref C104)
      (value 1uF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B454ED5))
    (comp (ref U104)
      (value 74HC595)
      (footprint Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B45537E))
    (comp (ref U103)
      (value 74HC595)
      (footprint Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B455418))
    (comp (ref R103)
      (value 10K)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B45725E))
    (comp (ref SW101)
      (value SW_PUSH)
      (footprint Buttons_Switches_SMD:SW_SPST_EVPBF)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B4574FB))
    (comp (ref P103)
      (value CONN_01X04)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B459213))
    (comp (ref R101)
      (value 16K)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B46350A))
    (comp (ref U101)
      (value FOD814-D)
      (footprint onsemi:OnSemi_PDIP4)
      (libsource (lib fod814-d) (part FOD814-D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B46379C))
    (comp (ref R102)
      (value 16K)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B463817))
    (comp (ref R106)
      (value 2K)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B463CCD))
    (comp (ref P104)
      (value CONN_01X02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B47C991))
    (comp (ref U201)
      (value LTV-846S)
      (footprint lite-on:Lite-On_SMD-16)
      (libsource (lib ltv-846s) (part LTV-846S))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46AB5A))
    (comp (ref R201)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46AD18))
    (comp (ref R202)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46ADE1))
    (comp (ref R203)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46AE05))
    (comp (ref R204)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46AE2D))
    (comp (ref U202)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46B23B))
    (comp (ref R209)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46B74F))
    (comp (ref R213)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46B7A0))
    (comp (ref C201)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46B7E2))
    (comp (ref R205)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46B82D))
    (comp (ref U203)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46BFA2))
    (comp (ref R210)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46BFA8))
    (comp (ref R214)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46BFAE))
    (comp (ref C202)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46BFB4))
    (comp (ref R206)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46BFBA))
    (comp (ref U204)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C433))
    (comp (ref R211)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C439))
    (comp (ref R215)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C43F))
    (comp (ref C203)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C445))
    (comp (ref R207)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C44B))
    (comp (ref U205)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C45F))
    (comp (ref R212)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C465))
    (comp (ref R216)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C46B))
    (comp (ref C204)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C471))
    (comp (ref R208)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B46C477))
    (comp (ref P201)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4722B1))
    (comp (ref P203)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B472657))
    (comp (ref P204)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B472C67))
    (comp (ref P202)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B472F34))
    (comp (ref U206)
      (value LTV-846S)
      (footprint lite-on:Lite-On_SMD-16)
      (libsource (lib ltv-846s) (part LTV-846S))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4747C4))
    (comp (ref R217)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4747CE))
    (comp (ref R218)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4747D6))
    (comp (ref R219)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4747DC))
    (comp (ref R220)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4747E2))
    (comp (ref U207)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4747FB))
    (comp (ref R225)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474801))
    (comp (ref R229)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474807))
    (comp (ref C205)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B47480D))
    (comp (ref R221)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474813))
    (comp (ref U208)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474824))
    (comp (ref R226)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B47482A))
    (comp (ref R230)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474830))
    (comp (ref C206)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474836))
    (comp (ref R222)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B47483C))
    (comp (ref U209)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B47484D))
    (comp (ref R227)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474853))
    (comp (ref R231)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474859))
    (comp (ref C207)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B47485F))
    (comp (ref R223)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474865))
    (comp (ref U210)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474876))
    (comp (ref R228)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B47487C))
    (comp (ref R232)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474882))
    (comp (ref C208)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B474888))
    (comp (ref R224)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B47488E))
    (comp (ref P205)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4748B9))
    (comp (ref P207)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4748C4))
    (comp (ref P208)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4748D1))
    (comp (ref P206)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankA/) (tstamps /5B46698C/))
      (tstamp 5B4748DC))
    (comp (ref U301)
      (value LTV-846S)
      (footprint lite-on:Lite-On_SMD-16)
      (libsource (lib ltv-846s) (part LTV-846S))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46AB5A))
    (comp (ref R301)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46AD18))
    (comp (ref R302)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46ADE1))
    (comp (ref R303)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46AE05))
    (comp (ref R304)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46AE2D))
    (comp (ref U302)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46B23B))
    (comp (ref R309)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46B74F))
    (comp (ref R313)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46B7A0))
    (comp (ref C301)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46B7E2))
    (comp (ref R305)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46B82D))
    (comp (ref U303)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46BFA2))
    (comp (ref R310)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46BFA8))
    (comp (ref R314)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46BFAE))
    (comp (ref C302)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46BFB4))
    (comp (ref R306)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46BFBA))
    (comp (ref U304)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C433))
    (comp (ref R311)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C439))
    (comp (ref R315)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C43F))
    (comp (ref C303)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C445))
    (comp (ref R307)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C44B))
    (comp (ref U305)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C45F))
    (comp (ref R312)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C465))
    (comp (ref R316)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C46B))
    (comp (ref C304)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C471))
    (comp (ref R308)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B46C477))
    (comp (ref P301)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4722B1))
    (comp (ref P303)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B472657))
    (comp (ref P304)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B472C67))
    (comp (ref P302)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B472F34))
    (comp (ref U306)
      (value LTV-846S)
      (footprint lite-on:Lite-On_SMD-16)
      (libsource (lib ltv-846s) (part LTV-846S))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4747C4))
    (comp (ref R317)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4747CE))
    (comp (ref R318)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4747D6))
    (comp (ref R319)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4747DC))
    (comp (ref R320)
      (value 660)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4747E2))
    (comp (ref U307)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4747FB))
    (comp (ref R325)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474801))
    (comp (ref R329)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474807))
    (comp (ref C305)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B47480D))
    (comp (ref R321)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474813))
    (comp (ref U308)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474824))
    (comp (ref R326)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B47482A))
    (comp (ref R330)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474830))
    (comp (ref C306)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474836))
    (comp (ref R322)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B47483C))
    (comp (ref U309)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B47484D))
    (comp (ref R327)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474853))
    (comp (ref R331)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474859))
    (comp (ref C307)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B47485F))
    (comp (ref R323)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474865))
    (comp (ref U310)
      (value TRIAC)
      (libsource (lib device) (part TRIAC))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474876))
    (comp (ref R328)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B47487C))
    (comp (ref R332)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474882))
    (comp (ref C308)
      (value 22nF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B474888))
    (comp (ref R324)
      (value 56)
      (footprint Resistors_SMD:R_0603_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B47488E))
    (comp (ref P305)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4748B9))
    (comp (ref P307)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4748C4))
    (comp (ref P308)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4748D1))
    (comp (ref P306)
      (value CONN_01X02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /Output-BankB/) (tstamps /5B477E02/))
      (tstamp 5B4748DC)))
  (libparts
    (libpart (lib 74xx) (part 74HC595)
      (aliases
        (alias 74LS596)
        (alias 74LS595))
      (description "8 bits serial in // out Shift Register 3 State Out")
      (docs 74xx/74HC595.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 74HC595))
      (pins
        (pin (num 1) (name QB) (type 3state))
        (pin (num 2) (name QC) (type 3state))
        (pin (num 3) (name QD) (type 3state))
        (pin (num 4) (name QE) (type 3state))
        (pin (num 5) (name QF) (type 3state))
        (pin (num 6) (name QG) (type 3state))
        (pin (num 7) (name QH) (type 3state))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name ~QH) (type output))
        (pin (num 10) (name SRCLR) (type input))
        (pin (num 11) (name SRCLK) (type input))
        (pin (num 12) (name RCLK) (type input))
        (pin (num 13) (name G) (type input))
        (pin (num 14) (name SER) (type input))
        (pin (num 15) (name QA) (type 3state))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib fod814-d) (part FOD814-D)
      (fields
        (field (name Reference) U)
        (field (name Value) FOD814-D))
      (pins
        (pin (num 1) (name AC) (type input))
        (pin (num 2) (name AC) (type input))
        (pin (num 3) (name EMITTER) (type input))
        (pin (num 4) (name COLLECTOR) (type input))))
    (libpart (lib ltv-846s) (part LTV-846S)
      (fields
        (field (name Reference) U)
        (field (name Value) LTV-846S))
      (pins
        (pin (num 1) (name AN_A) (type input))
        (pin (num 2) (name CAT_A) (type input))
        (pin (num 3) (name AN_B) (type input))
        (pin (num 4) (name CAT_B) (type input))
        (pin (num 5) (name AN_C) (type input))
        (pin (num 6) (name CAT_C) (type input))
        (pin (num 7) (name AN_D) (type input))
        (pin (num 8) (name CAT_D) (type input))
        (pin (num 9) (name EMIT_D) (type input))
        (pin (num 10) (name COLL_D) (type input))
        (pin (num 11) (name EMIT_C) (type input))
        (pin (num 12) (name COLL_C) (type input))
        (pin (num 13) (name EMIT_B) (type input))
        (pin (num 14) (name COLL_B) (type input))
        (pin (num 15) (name EMIT_A) (type input))
        (pin (num 16) (name COLL_A) (type input))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib stm32f030f4p6) (part STM32F030F4P6)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F030F4P6))
      (pins
        (pin (num 1) (name BOOT0) (type input))
        (pin (num 2) (name PF0-OSC_IN) (type input))
        (pin (num 3) (name PF1-OSC_OUT) (type input))
        (pin (num 4) (name NRST) (type input))
        (pin (num 5) (name VDDA) (type power_in))
        (pin (num 6) (name PA0) (type 3state))
        (pin (num 7) (name PA1) (type 3state))
        (pin (num 8) (name PA2) (type 3state))
        (pin (num 9) (name PA3) (type 3state))
        (pin (num 10) (name PA4) (type 3state))
        (pin (num 11) (name PA5) (type 3state))
        (pin (num 12) (name PA6) (type 3state))
        (pin (num 13) (name PA7) (type 3state))
        (pin (num 14) (name PB1) (type 3state))
        (pin (num 15) (name VSS) (type power_in))
        (pin (num 16) (name VDD) (type power_in))
        (pin (num 17) (name PA9) (type 3state))
        (pin (num 18) (name PA10) (type 3state))
        (pin (num 19) (name PA13) (type 3state))
        (pin (num 20) (name PA14) (type 3state))))
    (libpart (lib device) (part SW_PUSH)
      (description Button)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part TRIAC)
      (fields
        (field (name Reference) U)
        (field (name Value) TRIAC))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type input)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical ltv-846s)
      (uri /home/isthatme/Documents/kicad-projects/Custom-Parts/ltv-846s.lib))
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical stm32f030f4p6)
      (uri /home/isthatme/Documents/kicad-projects/Custom-Parts/stm32f030f4p6.lib))
    (library (logical fod814-d)
      (uri /home/isthatme/Documents/kicad-projects/Custom-Parts/fod814-d.lib)))
  (nets
    (net (code 1) (name /STM_SWCLK)
      (node (ref U102) (pin 20))
      (node (ref P103) (pin 2)))
    (net (code 2) (name /STM_SWDIO)
      (node (ref U102) (pin 19))
      (node (ref P103) (pin 1)))
    (net (code 3) (name GND)
      (node (ref U102) (pin 15))
      (node (ref U306) (pin 8))
      (node (ref U306) (pin 6))
      (node (ref U306) (pin 4))
      (node (ref U306) (pin 2))
      (node (ref U102) (pin 1))
      (node (ref C105) (pin 2))
      (node (ref C103) (pin 2))
      (node (ref C101) (pin 2))
      (node (ref C104) (pin 2))
      (node (ref C102) (pin 2))
      (node (ref U206) (pin 8))
      (node (ref U206) (pin 6))
      (node (ref U301) (pin 2))
      (node (ref U206) (pin 4))
      (node (ref U301) (pin 4))
      (node (ref U206) (pin 2))
      (node (ref U301) (pin 6))
      (node (ref U301) (pin 8))
      (node (ref U104) (pin 8))
      (node (ref U103) (pin 8))
      (node (ref U201) (pin 6))
      (node (ref U201) (pin 2))
      (node (ref U201) (pin 8))
      (node (ref P103) (pin 4))
      (node (ref U101) (pin 3))
      (node (ref U201) (pin 4))
      (node (ref SW101) (pin 1)))
    (net (code 4) (name "Net-(R102-Pad1)")
      (node (ref U101) (pin 2))
      (node (ref R102) (pin 1)))
    (net (code 5) (name AC-H)
      (node (ref P302) (pin 2))
      (node (ref P204) (pin 2))
      (node (ref P207) (pin 2))
      (node (ref P301) (pin 2))
      (node (ref P202) (pin 2))
      (node (ref P206) (pin 2))
      (node (ref P304) (pin 2))
      (node (ref P208) (pin 2))
      (node (ref P203) (pin 2))
      (node (ref R101) (pin 2))
      (node (ref P303) (pin 2))
      (node (ref P104) (pin 1))
      (node (ref P307) (pin 2))
      (node (ref P305) (pin 2))
      (node (ref P201) (pin 2))
      (node (ref P308) (pin 2))
      (node (ref P205) (pin 2))
      (node (ref P306) (pin 2)))
    (net (code 6) (name "Net-(R101-Pad1)")
      (node (ref U101) (pin 1))
      (node (ref R101) (pin 1)))
    (net (code 7) (name "Net-(U104-Pad9)")
      (node (ref U104) (pin 9)))
    (net (code 8) (name "Net-(U103-Pad9)")
      (node (ref U104) (pin 14))
      (node (ref U103) (pin 9)))
    (net (code 9) (name /STM_~RST)
      (node (ref U102) (pin 4))
      (node (ref SW101) (pin 2))
      (node (ref R103) (pin 2)))
    (net (code 10) (name "Net-(U102-Pad3)")
      (node (ref U102) (pin 3)))
    (net (code 11) (name "Net-(U102-Pad2)")
      (node (ref U102) (pin 2)))
    (net (code 12) (name "Net-(U102-Pad13)")
      (node (ref U102) (pin 13)))
    (net (code 13) (name "Net-(U102-Pad12)")
      (node (ref U102) (pin 12)))
    (net (code 14) (name /Output-BankB/OUT-H)
      (node (ref R320) (pin 2))
      (node (ref U104) (pin 7)))
    (net (code 15) (name /Output-BankB/OUT-G)
      (node (ref U104) (pin 6))
      (node (ref R319) (pin 2)))
    (net (code 16) (name /Output-BankB/OUT-F)
      (node (ref U104) (pin 5))
      (node (ref R318) (pin 2)))
    (net (code 17) (name /Output-BankB/OUT-E)
      (node (ref U104) (pin 4))
      (node (ref R317) (pin 2)))
    (net (code 18) (name /Output-BankB/OUT-D)
      (node (ref U104) (pin 3))
      (node (ref R304) (pin 2)))
    (net (code 19) (name /Output-BankB/OUT-C)
      (node (ref R303) (pin 2))
      (node (ref U104) (pin 2)))
    (net (code 20) (name /Output-BankB/OUT-B)
      (node (ref R302) (pin 2))
      (node (ref U104) (pin 1)))
    (net (code 21) (name /Output-BankB/OUT-A)
      (node (ref R301) (pin 2))
      (node (ref U104) (pin 15)))
    (net (code 22) (name /Output-BankA/OUT-H)
      (node (ref U103) (pin 7))
      (node (ref R220) (pin 2)))
    (net (code 23) (name AC-N)
      (node (ref U304) (pin 1))
      (node (ref C305) (pin 1))
      (node (ref U204) (pin 1))
      (node (ref U309) (pin 1))
      (node (ref R321) (pin 2))
      (node (ref C204) (pin 1))
      (node (ref U205) (pin 1))
      (node (ref C302) (pin 1))
      (node (ref R207) (pin 2))
      (node (ref C203) (pin 1))
      (node (ref U308) (pin 1))
      (node (ref C202) (pin 1))
      (node (ref R306) (pin 2))
      (node (ref R206) (pin 2))
      (node (ref R208) (pin 2))
      (node (ref R323) (pin 2))
      (node (ref R224) (pin 2))
      (node (ref U307) (pin 1))
      (node (ref U310) (pin 1))
      (node (ref C308) (pin 1))
      (node (ref C307) (pin 1))
      (node (ref C207) (pin 1))
      (node (ref C208) (pin 1))
      (node (ref R223) (pin 2))
      (node (ref U202) (pin 1))
      (node (ref U210) (pin 1))
      (node (ref C301) (pin 1))
      (node (ref R305) (pin 2))
      (node (ref C201) (pin 1))
      (node (ref R205) (pin 2))
      (node (ref R322) (pin 2))
      (node (ref C306) (pin 1))
      (node (ref U303) (pin 1))
      (node (ref R324) (pin 2))
      (node (ref U203) (pin 1))
      (node (ref C303) (pin 1))
      (node (ref R221) (pin 2))
      (node (ref C304) (pin 1))
      (node (ref U305) (pin 1))
      (node (ref R307) (pin 2))
      (node (ref U208) (pin 1))
      (node (ref P104) (pin 2))
      (node (ref R102) (pin 2))
      (node (ref U302) (pin 1))
      (node (ref U207) (pin 1))
      (node (ref C206) (pin 1))
      (node (ref R222) (pin 2))
      (node (ref R308) (pin 2))
      (node (ref C205) (pin 1))
      (node (ref U209) (pin 1)))
    (net (code 24) (name /Output-BankA/OUT-G)
      (node (ref R219) (pin 2))
      (node (ref U103) (pin 6)))
    (net (code 25) (name /Output-BankA/OUT-E)
      (node (ref R217) (pin 2))
      (node (ref U103) (pin 4)))
    (net (code 26) (name /Output-BankA/OUT-F)
      (node (ref R218) (pin 2))
      (node (ref U103) (pin 5)))
    (net (code 27) (name +3V3)
      (node (ref C105) (pin 1))
      (node (ref C103) (pin 1))
      (node (ref C101) (pin 1))
      (node (ref C104) (pin 1))
      (node (ref C102) (pin 1))
      (node (ref R105) (pin 1))
      (node (ref U104) (pin 16))
      (node (ref P103) (pin 3))
      (node (ref U102) (pin 16))
      (node (ref R104) (pin 1))
      (node (ref U102) (pin 5))
      (node (ref R103) (pin 1))
      (node (ref U103) (pin 16))
      (node (ref R106) (pin 1)))
    (net (code 28) (name /I2C_SDA)
      (node (ref U102) (pin 18))
      (node (ref P101) (pin 2))
      (node (ref R105) (pin 2))
      (node (ref P102) (pin 2)))
    (net (code 29) (name /Shift_RCLK)
      (node (ref U102) (pin 9))
      (node (ref U104) (pin 12))
      (node (ref U103) (pin 12)))
    (net (code 30) (name "Net-(U102-Pad14)")
      (node (ref U102) (pin 14)))
    (net (code 31) (name /ZERO_CROSS)
      (node (ref U101) (pin 4))
      (node (ref R106) (pin 2))
      (node (ref U102) (pin 11)))
    (net (code 32) (name /Shift_~OE)
      (node (ref U103) (pin 13))
      (node (ref U102) (pin 10))
      (node (ref U104) (pin 13)))
    (net (code 33) (name /Shift_~SRCLR)
      (node (ref U102) (pin 8))
      (node (ref U103) (pin 10))
      (node (ref U104) (pin 10)))
    (net (code 34) (name /Shift_SER)
      (node (ref U103) (pin 14))
      (node (ref U102) (pin 6)))
    (net (code 35) (name /I2C_SCL)
      (node (ref P102) (pin 1))
      (node (ref R104) (pin 2))
      (node (ref U102) (pin 17))
      (node (ref P101) (pin 1)))
    (net (code 36) (name /Output-BankA/OUT-A)
      (node (ref R201) (pin 2))
      (node (ref U103) (pin 15)))
    (net (code 37) (name /Shift_SRCLK)
      (node (ref U102) (pin 7))
      (node (ref U103) (pin 11))
      (node (ref U104) (pin 11)))
    (net (code 38) (name /Output-BankA/OUT-D)
      (node (ref R204) (pin 2))
      (node (ref U103) (pin 3)))
    (net (code 39) (name /Output-BankA/OUT-C)
      (node (ref U103) (pin 2))
      (node (ref R203) (pin 2)))
    (net (code 40) (name /Output-BankA/OUT-B)
      (node (ref R202) (pin 2))
      (node (ref U103) (pin 1)))
    (net (code 41) (name /Output-BankA/AC_LOAD-B)
      (node (ref U203) (pin 2))
      (node (ref U208) (pin 2))
      (node (ref R230) (pin 1))
      (node (ref P206) (pin 1))
      (node (ref R214) (pin 1))
      (node (ref P202) (pin 1)))
    (net (code 42) (name "Net-(C205-Pad2)")
      (node (ref C205) (pin 2))
      (node (ref R225) (pin 1))
      (node (ref R229) (pin 2)))
    (net (code 43) (name /Output-BankA/AC_LOAD-C)
      (node (ref R215) (pin 1))
      (node (ref U204) (pin 2))
      (node (ref P207) (pin 1))
      (node (ref R231) (pin 1))
      (node (ref P203) (pin 1))
      (node (ref U209) (pin 2)))
    (net (code 44) (name "Net-(C206-Pad2)")
      (node (ref C206) (pin 2))
      (node (ref R230) (pin 2))
      (node (ref R226) (pin 1)))
    (net (code 45) (name "Net-(R227-Pad2)")
      (node (ref R227) (pin 2))
      (node (ref U206) (pin 12)))
    (net (code 46) (name "Net-(R217-Pad1)")
      (node (ref U206) (pin 1))
      (node (ref R217) (pin 1)))
    (net (code 47) (name "Net-(R225-Pad2)")
      (node (ref U206) (pin 16))
      (node (ref R225) (pin 2)))
    (net (code 48) (name "Net-(R221-Pad1)")
      (node (ref U206) (pin 15))
      (node (ref R221) (pin 1))
      (node (ref U207) (pin 3)))
    (net (code 49) (name "Net-(R226-Pad2)")
      (node (ref U206) (pin 14))
      (node (ref R226) (pin 2)))
    (net (code 50) (name "Net-(R222-Pad1)")
      (node (ref U208) (pin 3))
      (node (ref R222) (pin 1))
      (node (ref U206) (pin 13)))
    (net (code 51) (name "Net-(R223-Pad1)")
      (node (ref U206) (pin 11))
      (node (ref R223) (pin 1))
      (node (ref U209) (pin 3)))
    (net (code 52) (name "Net-(R228-Pad2)")
      (node (ref U206) (pin 10))
      (node (ref R228) (pin 2)))
    (net (code 53) (name "Net-(R220-Pad1)")
      (node (ref R220) (pin 1))
      (node (ref U206) (pin 7)))
    (net (code 54) (name "Net-(R219-Pad1)")
      (node (ref R219) (pin 1))
      (node (ref U206) (pin 5)))
    (net (code 55) (name "Net-(R218-Pad1)")
      (node (ref R218) (pin 1))
      (node (ref U206) (pin 3)))
    (net (code 56) (name /Output-BankA/AC_LOAD-A)
      (node (ref P201) (pin 1))
      (node (ref U207) (pin 2))
      (node (ref P205) (pin 1))
      (node (ref R213) (pin 1))
      (node (ref R229) (pin 1))
      (node (ref U202) (pin 2)))
    (net (code 57) (name /Output-BankA/AC_LOAD-D)
      (node (ref U210) (pin 2))
      (node (ref R232) (pin 1))
      (node (ref P208) (pin 1))
      (node (ref U205) (pin 2))
      (node (ref R216) (pin 1))
      (node (ref P204) (pin 1)))
    (net (code 58) (name "Net-(C208-Pad2)")
      (node (ref C208) (pin 2))
      (node (ref R228) (pin 1))
      (node (ref R232) (pin 2)))
    (net (code 59) (name "Net-(C207-Pad2)")
      (node (ref R227) (pin 1))
      (node (ref R231) (pin 2))
      (node (ref C207) (pin 2)))
    (net (code 60) (name "Net-(R224-Pad1)")
      (node (ref U210) (pin 3))
      (node (ref R224) (pin 1))
      (node (ref U206) (pin 9)))
    (net (code 61) (name "Net-(C201-Pad2)")
      (node (ref R209) (pin 1))
      (node (ref R213) (pin 2))
      (node (ref C201) (pin 2)))
    (net (code 62) (name "Net-(C202-Pad2)")
      (node (ref C202) (pin 2))
      (node (ref R214) (pin 2))
      (node (ref R210) (pin 1)))
    (net (code 63) (name "Net-(R201-Pad1)")
      (node (ref R201) (pin 1))
      (node (ref U201) (pin 1)))
    (net (code 64) (name "Net-(R209-Pad2)")
      (node (ref R209) (pin 2))
      (node (ref U201) (pin 16)))
    (net (code 65) (name "Net-(R205-Pad1)")
      (node (ref U201) (pin 15))
      (node (ref R205) (pin 1))
      (node (ref U202) (pin 3)))
    (net (code 66) (name "Net-(R210-Pad2)")
      (node (ref R210) (pin 2))
      (node (ref U201) (pin 14)))
    (net (code 67) (name "Net-(R206-Pad1)")
      (node (ref U201) (pin 13))
      (node (ref R206) (pin 1))
      (node (ref U203) (pin 3)))
    (net (code 68) (name "Net-(R211-Pad2)")
      (node (ref R211) (pin 2))
      (node (ref U201) (pin 12)))
    (net (code 69) (name "Net-(R212-Pad2)")
      (node (ref U201) (pin 10))
      (node (ref R212) (pin 2)))
    (net (code 70) (name "Net-(R204-Pad1)")
      (node (ref R204) (pin 1))
      (node (ref U201) (pin 7)))
    (net (code 71) (name "Net-(R203-Pad1)")
      (node (ref R203) (pin 1))
      (node (ref U201) (pin 5)))
    (net (code 72) (name "Net-(R202-Pad1)")
      (node (ref R202) (pin 1))
      (node (ref U201) (pin 3)))
    (net (code 73) (name "Net-(C203-Pad2)")
      (node (ref R211) (pin 1))
      (node (ref R215) (pin 2))
      (node (ref C203) (pin 2)))
    (net (code 74) (name "Net-(R207-Pad1)")
      (node (ref U201) (pin 11))
      (node (ref R207) (pin 1))
      (node (ref U204) (pin 3)))
    (net (code 75) (name "Net-(R208-Pad1)")
      (node (ref U201) (pin 9))
      (node (ref R208) (pin 1))
      (node (ref U205) (pin 3)))
    (net (code 76) (name "Net-(C204-Pad2)")
      (node (ref R212) (pin 1))
      (node (ref C204) (pin 2))
      (node (ref R216) (pin 2)))
    (net (code 77) (name /Output-BankB/AC_LOAD-B)
      (node (ref R330) (pin 1))
      (node (ref U303) (pin 2))
      (node (ref P302) (pin 1))
      (node (ref P306) (pin 1))
      (node (ref U308) (pin 2))
      (node (ref R314) (pin 1)))
    (net (code 78) (name "Net-(C305-Pad2)")
      (node (ref C305) (pin 2))
      (node (ref R329) (pin 2))
      (node (ref R325) (pin 1)))
    (net (code 79) (name /Output-BankB/AC_LOAD-C)
      (node (ref R315) (pin 1))
      (node (ref U304) (pin 2))
      (node (ref P303) (pin 1))
      (node (ref R331) (pin 1))
      (node (ref U309) (pin 2))
      (node (ref P307) (pin 1)))
    (net (code 80) (name "Net-(C306-Pad2)")
      (node (ref R326) (pin 1))
      (node (ref R330) (pin 2))
      (node (ref C306) (pin 2)))
    (net (code 81) (name "Net-(R327-Pad2)")
      (node (ref U306) (pin 12))
      (node (ref R327) (pin 2)))
    (net (code 82) (name "Net-(R317-Pad1)")
      (node (ref U306) (pin 1))
      (node (ref R317) (pin 1)))
    (net (code 83) (name "Net-(R325-Pad2)")
      (node (ref U306) (pin 16))
      (node (ref R325) (pin 2)))
    (net (code 84) (name "Net-(R321-Pad1)")
      (node (ref U306) (pin 15))
      (node (ref R321) (pin 1))
      (node (ref U307) (pin 3)))
    (net (code 85) (name "Net-(R326-Pad2)")
      (node (ref R326) (pin 2))
      (node (ref U306) (pin 14)))
    (net (code 86) (name "Net-(R322-Pad1)")
      (node (ref R322) (pin 1))
      (node (ref U308) (pin 3))
      (node (ref U306) (pin 13)))
    (net (code 87) (name "Net-(R323-Pad1)")
      (node (ref U306) (pin 11))
      (node (ref U309) (pin 3))
      (node (ref R323) (pin 1)))
    (net (code 88) (name "Net-(R328-Pad2)")
      (node (ref R328) (pin 2))
      (node (ref U306) (pin 10)))
    (net (code 89) (name "Net-(R320-Pad1)")
      (node (ref U306) (pin 7))
      (node (ref R320) (pin 1)))
    (net (code 90) (name "Net-(R319-Pad1)")
      (node (ref U306) (pin 5))
      (node (ref R319) (pin 1)))
    (net (code 91) (name "Net-(R318-Pad1)")
      (node (ref U306) (pin 3))
      (node (ref R318) (pin 1)))
    (net (code 92) (name /Output-BankB/AC_LOAD-A)
      (node (ref U302) (pin 2))
      (node (ref R313) (pin 1))
      (node (ref P305) (pin 1))
      (node (ref P301) (pin 1))
      (node (ref U307) (pin 2))
      (node (ref R329) (pin 1)))
    (net (code 93) (name /Output-BankB/AC_LOAD-D)
      (node (ref P304) (pin 1))
      (node (ref R316) (pin 1))
      (node (ref U305) (pin 2))
      (node (ref R332) (pin 1))
      (node (ref P308) (pin 1))
      (node (ref U310) (pin 2)))
    (net (code 94) (name "Net-(C308-Pad2)")
      (node (ref R328) (pin 1))
      (node (ref C308) (pin 2))
      (node (ref R332) (pin 2)))
    (net (code 95) (name "Net-(C307-Pad2)")
      (node (ref C307) (pin 2))
      (node (ref R327) (pin 1))
      (node (ref R331) (pin 2)))
    (net (code 96) (name "Net-(R324-Pad1)")
      (node (ref U306) (pin 9))
      (node (ref R324) (pin 1))
      (node (ref U310) (pin 3)))
    (net (code 97) (name "Net-(C301-Pad2)")
      (node (ref R313) (pin 2))
      (node (ref R309) (pin 1))
      (node (ref C301) (pin 2)))
    (net (code 98) (name "Net-(C302-Pad2)")
      (node (ref R314) (pin 2))
      (node (ref C302) (pin 2))
      (node (ref R310) (pin 1)))
    (net (code 99) (name "Net-(R311-Pad2)")
      (node (ref U301) (pin 12))
      (node (ref R311) (pin 2)))
    (net (code 100) (name "Net-(R301-Pad1)")
      (node (ref U301) (pin 1))
      (node (ref R301) (pin 1)))
    (net (code 101) (name "Net-(R309-Pad2)")
      (node (ref R309) (pin 2))
      (node (ref U301) (pin 16)))
    (net (code 102) (name "Net-(R305-Pad1)")
      (node (ref R305) (pin 1))
      (node (ref U301) (pin 15))
      (node (ref U302) (pin 3)))
    (net (code 103) (name "Net-(R310-Pad2)")
      (node (ref R310) (pin 2))
      (node (ref U301) (pin 14)))
    (net (code 104) (name "Net-(R306-Pad1)")
      (node (ref U301) (pin 13))
      (node (ref R306) (pin 1))
      (node (ref U303) (pin 3)))
    (net (code 105) (name "Net-(R312-Pad2)")
      (node (ref R312) (pin 2))
      (node (ref U301) (pin 10)))
    (net (code 106) (name "Net-(R304-Pad1)")
      (node (ref U301) (pin 7))
      (node (ref R304) (pin 1)))
    (net (code 107) (name "Net-(R303-Pad1)")
      (node (ref U301) (pin 5))
      (node (ref R303) (pin 1)))
    (net (code 108) (name "Net-(R302-Pad1)")
      (node (ref U301) (pin 3))
      (node (ref R302) (pin 1)))
    (net (code 109) (name "Net-(C304-Pad2)")
      (node (ref R312) (pin 1))
      (node (ref R316) (pin 2))
      (node (ref C304) (pin 2)))
    (net (code 110) (name "Net-(C303-Pad2)")
      (node (ref C303) (pin 2))
      (node (ref R311) (pin 1))
      (node (ref R315) (pin 2)))
    (net (code 111) (name "Net-(R307-Pad1)")
      (node (ref U304) (pin 3))
      (node (ref U301) (pin 11))
      (node (ref R307) (pin 1)))
    (net (code 112) (name "Net-(R308-Pad1)")
      (node (ref U301) (pin 9))
      (node (ref U305) (pin 3))
      (node (ref R308) (pin 1)))))