(export (version D)
  (design
    (source /home/isthatme/kicad-projects/Fused-Distrib/Fused-Distrib.sch)
    (date "Sun 13 Aug 2017 07:39:43 PM MDT")
    (tool "Eeschema 4.0.6-e0-6349~53~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Fused-Distrib.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref F1)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_lateral_Type-II)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FB9E1))
    (comp (ref F2)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_lateral_Type-II)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FBA07))
    (comp (ref F3)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_lateral_Type-II)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FBA29))
    (comp (ref F4)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_lateral_Type-II)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FBA4A))
    (comp (ref F5)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_lateral_Type-II)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FBC12))
    (comp (ref F6)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_lateral_Type-II)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FBC18))
    (comp (ref F7)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_lateral_Type-II)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FBC1E))
    (comp (ref F8)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_lateral_Type-II)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FBC24))
    (comp (ref P1)
      (value CONN_01X01)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FC470))
    (comp (ref P2)
      (value CONN_01X01)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FC4D0))
    (comp (ref P3)
      (value CONN_01X01)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FC57E))
    (comp (ref P4)
      (value CONN_01X01)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FC584))
    (comp (ref P5)
      (value CONN_01X01)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FC6C2))
    (comp (ref P6)
      (value CONN_01X01)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FC6C8))
    (comp (ref P7)
      (value CONN_01X01)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FC6CE))
    (comp (ref P8)
      (value CONN_01X01)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FC6D4))
    (comp (ref P17)
      (value CONN_01X06)
      (footprint Custom_Footprints:Screw_Connector_M5)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 598FD4E8))
    (comp (ref P18)
      (value CONN_01X06)
      (footprint Custom_Footprints:Screw_Connector_M5)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 59910047)))
  (libparts
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01")
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X06)
      (description "Connector, single row, 01x06")
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib)))
  (nets
    (net (code 1) (name "Net-(F6-Pad1)")
      (node (ref P6) (pin 1))
      (node (ref F6) (pin 1)))
    (net (code 2) (name "Net-(F7-Pad1)")
      (node (ref P7) (pin 1))
      (node (ref F7) (pin 1)))
    (net (code 3) (name "Net-(F8-Pad1)")
      (node (ref P8) (pin 1))
      (node (ref F8) (pin 1)))
    (net (code 4) (name "Net-(F5-Pad1)")
      (node (ref P5) (pin 1))
      (node (ref F5) (pin 1)))
    (net (code 5) (name +12V)
      (node (ref F3) (pin 2))
      (node (ref F4) (pin 2))
      (node (ref F2) (pin 2))
      (node (ref F5) (pin 2))
      (node (ref F1) (pin 2))
      (node (ref F6) (pin 2))
      (node (ref F7) (pin 2))
      (node (ref F8) (pin 2))
      (node (ref P17) (pin 1))
      (node (ref P17) (pin 2))
      (node (ref P17) (pin 3))
      (node (ref P17) (pin 4))
      (node (ref P17) (pin 5))
      (node (ref P17) (pin 6))
      (node (ref P18) (pin 2))
      (node (ref P18) (pin 3))
      (node (ref P18) (pin 4))
      (node (ref P18) (pin 5))
      (node (ref P18) (pin 6))
      (node (ref P18) (pin 1)))
    (net (code 6) (name "Net-(F2-Pad1)")
      (node (ref P2) (pin 1))
      (node (ref F2) (pin 1)))
    (net (code 7) (name "Net-(F3-Pad1)")
      (node (ref F3) (pin 1))
      (node (ref P3) (pin 1)))
    (net (code 8) (name "Net-(F4-Pad1)")
      (node (ref F4) (pin 1))
      (node (ref P4) (pin 1)))
    (net (code 9) (name "Net-(F1-Pad1)")
      (node (ref P1) (pin 1))
      (node (ref F1) (pin 1)))))