(export (version D)
  (design
    (source C:/Users/David/Documents/kicad-projects/Altoids-PowerSupply/Altoids-PowerSupply.sch)
    (date "2017-11-27 7:00:28 PM")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Altoids-PowerSupply.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value MC34063)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib Altoids-PowerSupply-cache) (part MC34063))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15E34B))
    (comp (ref C2)
      (value Ct)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15E433))
    (comp (ref L1)
      (value L)
      (footprint Inductors_THT:L_Radial_D9.5mm_P5.00mm_Fastron_07HVP)
      (libsource (lib device) (part L))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15E508))
    (comp (ref R3)
      (value 180)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15E557))
    (comp (ref R4)
      (value Rsc)
      (footprint Resistors_SMD:R_1206_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15E5D6))
    (comp (ref C1)
      (value 100uF)
      (footprint Capacitors_SMD:CP_Elec_5x5.3)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15E73E))
    (comp (ref R1)
      (value R1)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15E79E))
    (comp (ref R2)
      (value R2)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15E80E))
    (comp (ref C3)
      (value Co)
      (footprint Capacitors_SMD:CP_Elec_5x5.3)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15E86B))
    (comp (ref D1)
      (value 1N5819)
      (footprint Diodes_SMD:D_0805)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15EC29))
    (comp (ref U2)
      (value MC34063)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib Altoids-PowerSupply-cache) (part MC34063))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F7F9))
    (comp (ref C5)
      (value Ct)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F809))
    (comp (ref L2)
      (value L)
      (footprint Inductors_THT:L_Radial_D9.5mm_P5.00mm_Fastron_07HVP)
      (libsource (lib device) (part L))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F819))
    (comp (ref R5)
      (value 180)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F81F))
    (comp (ref R6)
      (value Rsc)
      (footprint Resistors_SMD:R_1206_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F825))
    (comp (ref C4)
      (value 100uF)
      (footprint Capacitors_SMD:CP_Elec_5x5.3)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F82B))
    (comp (ref R8)
      (value R1)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F831))
    (comp (ref R7)
      (value R2)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F837))
    (comp (ref C6)
      (value Co)
      (footprint Capacitors_SMD:CP_Elec_5x5.3)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F83D))
    (comp (ref D2)
      (value 1N5819)
      (footprint Diodes_SMD:D_0805)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A15F857))
    (comp (ref U3)
      (value KeyElco-1043P)
      (footprint cust_footprints:KeyElco-1043P)
      (libsource (lib Altoids-PowerSupply-cache) (part KeyElco-1043P))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A160252))
    (comp (ref U5)
      (value AP2127K-3.3TRG1)
      (footprint TO_SOT_Packages_SMD:SOT-23-5)
      (libsource (lib Altoids-PowerSupply-cache) (part AP2127K-3.3TRG1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A160656))
    (comp (ref C7)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A160743))
    (comp (ref C8)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1607C9))
    (comp (ref J2)
      (value Conn_01x04_Female)
      (footprint Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04_Female))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A160CDD))
    (comp (ref J1)
      (value Conn_01x04_Male)
      (footprint Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04_Male))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A160DBE))
    (comp (ref J4)
      (value Conn_01x04_Female)
      (footprint Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04_Female))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1614C1))
    (comp (ref J3)
      (value Conn_01x04_Male)
      (footprint Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04_Male))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1614C7))
    (comp (ref J6)
      (value Conn_01x04_Female)
      (footprint Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04_Female))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A161636))
    (comp (ref J5)
      (value Conn_01x04_Male)
      (footprint Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x04_Male))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A16163C))
    (comp (ref U6)
      (value ATTINY45-20SU)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib atmel) (part ATTINY45-20SU))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A162E44))
    (comp (ref J8)
      (value Conn_01x02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A163794))
    (comp (ref D3)
      (value LED)
      (footprint LEDs:LED_0805_HandSoldering)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1640F0))
    (comp (ref R9)
      (value 499)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A164335))
    (comp (ref J7)
      (value Conn_01x06)
      (footprint Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x06))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A164A21))
    (comp (ref Q1)
      (value Q_PMOS_GDS)
      (footprint TO_SOT_Packages_SMD:TO-263-2)
      (libsource (lib device) (part Q_PMOS_GDS))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A166556))
    (comp (ref U4)
      (value BQ24230)
      (footprint Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm_ThermalVias)
      (libsource (lib Altoids-PowerSupply-cache) (part BQ24230))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1719CB))
    (comp (ref SW2)
      (value SW_DIP_x01)
      (footprint Buttons_Switches_SMD:SW_DIP_x1_W5.08mm_Slide_Copal_CHS-A)
      (libsource (lib switches) (part SW_DIP_x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A17420B))
    (comp (ref J9)
      (value USB_OTG)
      (footprint Connectors:USB_Micro-B)
      (libsource (lib conn) (part USB_OTG))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A17515A))
    (comp (ref J10)
      (value USB_A)
      (footprint Connectors:USB_A)
      (libsource (lib conn) (part USB_A))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A175249))
    (comp (ref R11)
      (value ISET)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A177114))
    (comp (ref R10)
      (value 10K)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A177EE9))
    (comp (ref D5)
      (value LED)
      (footprint LEDs:LED_0805_HandSoldering)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A178EEE))
    (comp (ref D4)
      (value LED)
      (footprint LEDs:LED_0805_HandSoldering)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A178FD9))
    (comp (ref R12)
      (value 499)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A17912D))
    (comp (ref R13)
      (value 499)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1791E0))
    (comp (ref L4)
      (value 1uH)
      (footprint Inductors_THT:L_Axial_L12.0mm_D5.0mm_P5.08mm_Vertical_Fastron_MISC)
      (libsource (lib device) (part L))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1900CD))
    (comp (ref C10)
      (value Cfilter)
      (footprint Capacitors_SMD:CP_Elec_5x5.3)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A190556))
    (comp (ref L3)
      (value 1uH)
      (footprint Inductors_THT:L_Axial_L12.0mm_D5.0mm_P5.08mm_Vertical_Fastron_MISC)
      (libsource (lib device) (part L))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A190D8F))
    (comp (ref C9)
      (value Cfilter)
      (footprint Capacitors_SMD:CP_Elec_5x5.3)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A190F32))
    (comp (ref SW1)
      (value SW_Push)
      (footprint Buttons_Switches_SMD:SW_SPST_PTS810)
      (libsource (lib switches) (part SW_Push))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A1958A7))
    (comp (ref R14)
      (value 10K)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A195C64)))
  (libparts
    (libpart (lib Altoids-PowerSupply-cache) (part AP2127K-3.3TRG1)
      (fields
        (field (name Reference) U)
        (field (name Value) AP2127K-3.3TRG1))
      (pins
        (pin (num 1) (name VIN) (type input))
        (pin (num 2) (name GND) (type input))
        (pin (num 3) (name ~SHTDWN) (type input))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name VOUT) (type power_out))))
    (libpart (lib atmel) (part ATTINY25-20SU)
      (aliases
        (alias ATTINY45-20SU)
        (alias ATTINY85-20SU))
      (description "SO8 Wide, 2k Flash, 128B SRAM, 128B EEPROM, Debug Wire")
      (docs http://www.atmel.com/images/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) ATTINY25-20SU)
        (field (name Footprint) Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm))
      (pins
        (pin (num 1) (name "PB5(~RESET~/dW/ADC0/PCINT5)") (type BiDi))
        (pin (num 2) (name "PB3(XTAL1/CLKI/~OC1B~/ADC3/PCINT3)") (type BiDi))
        (pin (num 3) (name "PB4(XTAL2/CLKO/OC1B/ADC2/PCINT4)") (type BiDi))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name "PB0(MOSI/DI/SDA/AIN0/OC0A/~OC1A~/AREF/PCINT0)") (type BiDi))
        (pin (num 6) (name "PB1(MISO/DO/AIN1/OC0B/OC1A/PCINT1)") (type BiDi))
        (pin (num 7) (name "PB2(SCK/USCK/SCL/T0/INT0/ADC1/PCINT2)") (type BiDi))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib Altoids-PowerSupply-cache) (part BQ24230)
      (fields
        (field (name Reference) U)
        (field (name Value) BQ24230))
      (pins
        (pin (num 1) (name TS) (type input))
        (pin (num 2) (name BAT) (type input))
        (pin (num 3) (name BAT) (type input))
        (pin (num 4) (name ~CE) (type input))
        (pin (num 5) (name EN2) (type input))
        (pin (num 6) (name EN1) (type input))
        (pin (num 7) (name ~PGOOD) (type output))
        (pin (num 8) (name VSS) (type input))
        (pin (num 9) (name ~CHG) (type output))
        (pin (num 10) (name OUT) (type input))
        (pin (num 11) (name OUT) (type input))
        (pin (num 12) (name ILIM) (type input))
        (pin (num 13) (name IN) (type input))
        (pin (num 14) (name TMR) (type input))
        (pin (num 15) (name ITERM) (type input))
        (pin (num 16) (name ISET) (type input))
        (pin (num 17) (name PAD) (type output))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x02)
      (description "Generic connector, single row, 01x02")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib conn) (part Conn_01x04_Female)
      (description "Generic connector, single row, 01x04")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04_Female))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib conn) (part Conn_01x04_Male)
      (description "Generic connector, single row, 01x04")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib conn) (part Conn_01x06)
      (description "Generic connector, single row, 01x06")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Altoids-PowerSupply-cache) (part KeyElco-1043P)
      (fields
        (field (name Reference) U)
        (field (name Value) KeyElco-1043P))
      (pins
        (pin (num 1) (name BT+) (type input))
        (pin (num 2) (name BT-) (type input))))
    (libpart (lib device) (part L)
      (description Inductor)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part LED)
      (description "LED generic")
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Altoids-PowerSupply-cache) (part MC34063)
      (description "Switching Power Supply Controller")
      (fields
        (field (name Reference) U)
        (field (name Value) MC34063))
      (pins
        (pin (num 1) (name SW_C) (type input))
        (pin (num 2) (name SW_E) (type input))
        (pin (num 3) (name Ct) (type input))
        (pin (num 4) (name GND) (type input))
        (pin (num 5) (name C_INV) (type input))
        (pin (num 6) (name VCC) (type input))
        (pin (num 7) (name I_Sense) (type input))
        (pin (num 8) (name DRV_C) (type input))))
    (libpart (lib device) (part Q_PMOS_GDS)
      (description "Transistor P-MOSFET with substrate diode (general)")
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PMOS_GDS))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib switches) (part SW_DIP_x01)
      (description "1x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
      (footprints
        (fp SW?DIP?x1*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x01))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib switches) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib conn) (part USB_A)
      (description "USB Type A connector")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_A))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name Shield) (type passive))))
    (libpart (lib conn) (part USB_OTG)
      (description "USB mini/micro connector")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_OTG))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name Shield) (type passive)))))
  (libraries
    (library (logical switches)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\switches.lib"))
    (library (logical atmel)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\atmel.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical Altoids-PowerSupply-cache)
      (uri C:\Users\David\Documents\kicad-projects\Altoids-PowerSupply\Altoids-PowerSupply-cache.lib)))
  (nets
    (net (code 1) (name "Net-(L2-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref U2) (pin 7))
      (node (ref L2) (pin 2))
      (node (ref R6) (pin 1)))
    (net (code 2) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref U2) (pin 8)))
    (net (code 3) (name "Net-(R7-Pad2)")
      (node (ref R8) (pin 1))
      (node (ref U2) (pin 5))
      (node (ref R7) (pin 2)))
    (net (code 4) (name "Net-(C5-Pad1)")
      (node (ref U2) (pin 3))
      (node (ref C5) (pin 1)))
    (net (code 5) (name "Net-(D1-Pad2)")
      (node (ref U1) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref L1) (pin 1)))
    (net (code 6) (name "Net-(D2-Pad2)")
      (node (ref L2) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 7) (name "Net-(C6-Pad1)")
      (node (ref L4) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 8) (name "Net-(U4-Pad15)")
      (node (ref U4) (pin 15)))
    (net (code 9) (name "Net-(J9-Pad2)")
      (node (ref J9) (pin 2)))
    (net (code 10) (name "Net-(J9-Pad3)")
      (node (ref J9) (pin 3)))
    (net (code 11) (name "Net-(L1-Pad2)")
      (node (ref U1) (pin 7))
      (node (ref L1) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 12) (name "Net-(R3-Pad1)")
      (node (ref U1) (pin 8))
      (node (ref R3) (pin 1)))
    (net (code 13) (name "Net-(C3-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref L3) (pin 2)))
    (net (code 14) (name "Net-(R1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref U1) (pin 5)))
    (net (code 15) (name "Net-(C2-Pad1)")
      (node (ref U1) (pin 3))
      (node (ref C2) (pin 1)))
    (net (code 16) (name "Net-(R14-Pad1)")
      (node (ref SW1) (pin 1))
      (node (ref R14) (pin 1)))
    (net (code 17) (name /CHG)
      (node (ref D5) (pin 2))
      (node (ref U4) (pin 9)))
    (net (code 18) (name "Net-(R10-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref U4) (pin 1)))
    (net (code 19) (name "Net-(R11-Pad1)")
      (node (ref U4) (pin 16))
      (node (ref R11) (pin 1)))
    (net (code 20) (name Earth)
      (node (ref R9) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref J6) (pin 3))
      (node (ref J3) (pin 4))
      (node (ref J3) (pin 3))
      (node (ref U4) (pin 5))
      (node (ref C1) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref J5) (pin 4))
      (node (ref J7) (pin 6))
      (node (ref U3) (pin 2))
      (node (ref J4) (pin 4))
      (node (ref J4) (pin 3))
      (node (ref J1) (pin 4))
      (node (ref J1) (pin 3))
      (node (ref J2) (pin 4))
      (node (ref J2) (pin 3))
      (node (ref C8) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref U5) (pin 2))
      (node (ref J6) (pin 4))
      (node (ref U4) (pin 8))
      (node (ref C6) (pin 2))
      (node (ref J8) (pin 2))
      (node (ref U6) (pin 4))
      (node (ref U4) (pin 17))
      (node (ref U1) (pin 4))
      (node (ref J5) (pin 3))
      (node (ref J10) (pin 5))
      (node (ref R12) (pin 2))
      (node (ref J9) (pin 6))
      (node (ref J10) (pin 4))
      (node (ref U2) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref J9) (pin 5))
      (node (ref R11) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref R14) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref R13) (pin 2)))
    (net (code 21) (name BAT)
      (node (ref U3) (pin 1))
      (node (ref U4) (pin 3))
      (node (ref U4) (pin 2)))
    (net (code 22) (name "Net-(J10-Pad2)")
      (node (ref J10) (pin 3))
      (node (ref J10) (pin 2)))
    (net (code 23) (name "Net-(J9-Pad1)")
      (node (ref U4) (pin 13))
      (node (ref J9) (pin 1))
      (node (ref U4) (pin 6)))
    (net (code 24) (name /PGOOD)
      (node (ref U4) (pin 7))
      (node (ref D4) (pin 2)))
    (net (code 25) (name "Net-(D5-Pad1)")
      (node (ref D5) (pin 1))
      (node (ref R13) (pin 1)))
    (net (code 26) (name /MISO)
      (node (ref U6) (pin 6))
      (node (ref U4) (pin 4))
      (node (ref J7) (pin 1)))
    (net (code 27) (name +12V)
      (node (ref C10) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref J4) (pin 2))
      (node (ref J3) (pin 1))
      (node (ref L4) (pin 1))
      (node (ref J3) (pin 2)))
    (net (code 28) (name "Net-(U5-Pad4)")
      (node (ref U5) (pin 4)))
    (net (code 29) (name +3V3)
      (node (ref U5) (pin 5))
      (node (ref J5) (pin 2))
      (node (ref J5) (pin 1))
      (node (ref J6) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref C8) (pin 1)))
    (net (code 30) (name "Net-(C1-Pad1)")
      (node (ref C7) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref U5) (pin 3))
      (node (ref U5) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 6))
      (node (ref C4) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref Q1) (pin 3))
      (node (ref U2) (pin 6)))
    (net (code 31) (name "Net-(D3-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref D3) (pin 1)))
    (net (code 32) (name +5V)
      (node (ref C9) (pin 1))
      (node (ref L3) (pin 1))
      (node (ref J10) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 1)))
    (net (code 33) (name "Net-(J9-Pad4)")
      (node (ref J9) (pin 4)))
    (net (code 34) (name "Net-(D4-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 35) (name "Net-(U4-Pad14)")
      (node (ref U4) (pin 14)))
    (net (code 36) (name /SCK)
      (node (ref J7) (pin 3))
      (node (ref SW1) (pin 2))
      (node (ref U6) (pin 7)))
    (net (code 37) (name /~RES)
      (node (ref J7) (pin 5))
      (node (ref SW2) (pin 2))
      (node (ref U6) (pin 1)))
    (net (code 38) (name Cutoff)
      (node (ref Q1) (pin 1))
      (node (ref J7) (pin 4))
      (node (ref U6) (pin 5)))
    (net (code 39) (name /IND)
      (node (ref D3) (pin 2))
      (node (ref U6) (pin 2)))
    (net (code 40) (name "Net-(U4-Pad12)")
      (node (ref U4) (pin 12)))
    (net (code 41) (name OUT)
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 10))
      (node (ref U6) (pin 3))
      (node (ref Q1) (pin 2))
      (node (ref J7) (pin 2))
      (node (ref U6) (pin 8))
      (node (ref J8) (pin 1))
      (node (ref SW2) (pin 1)))))