(kicad_sch (version 20211123) (generator eeschema)

  (uuid 0ae02a7a-b99d-4d94-adf9-eab03e178faa)

  (paper "A4")

  (lib_symbols
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (stroke (width 0.3302) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (stroke (width 0.3048) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Sonar:MCP4726" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 -8.89 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "MCP4726" (id 1) (at 0 8.89 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (id 2) (at -1.27 -12.7 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22272C.pdf" (id 3) (at -1.27 -12.7 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "MPN" "MCP4726A0T-E/CH" (id 4) (at -1.27 -12.7 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Manufacturer" "Microchip Technology" (id 5) (at -1.27 -12.7 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "DPN" "MCP4726A0T-E/CHCT-ND" (id 6) (at -1.27 -12.7 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Distributor" "DigiKey" (id 7) (at -1.27 -12.7 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "ki_keywords" "I2C DAC 12bit" (id 8) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "12-bit I2C DAC, buffered or unbuffered external reference" (id 9) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "MCP4726_0_1"
        (rectangle (start -6.35 7.62) (end 6.35 -7.62)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "MCP4726_1_1"
        (pin output line (at 8.89 6.35 180) (length 2.54)
          (name "V_{OUT}" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at -8.89 -6.35 0) (length 2.54)
          (name "V_{SS}" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at -8.89 6.35 0) (length 2.54)
          (name "V_{DD}" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -8.89 0 0) (length 2.54)
          (name "SDA" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -8.89 -2.54 0) (length 2.54)
          (name "SCL" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -8.89 3.81 0) (length 2.54)
          (name "VREF" (effects (font (size 1.27 1.27))))
          (number "6" (effects (font (size 1.27 1.27))))
        )
      )
    )
  )


  (wire (pts (xy 83.82 54.61) (xy 91.44 54.61))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 05f6d416-1481-42a6-a2df-1aa4de38097b)
  )
  (wire (pts (xy 97.79 77.47) (xy 97.79 81.28))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 09f7b182-1851-46a6-8ba4-68c4c6be33db)
  )
  (wire (pts (xy 83.82 63.5) (xy 91.44 63.5))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 151720bf-19df-415a-85de-e086fe20b3cc)
  )
  (wire (pts (xy 97.79 86.36) (xy 97.79 92.71))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 21f0ce83-fd52-4e29-a8d8-466ea0e32bff)
  )
  (wire (pts (xy 83.82 67.31) (xy 91.44 67.31))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 2fc769bd-5381-4800-be05-52880a1d767e)
  )
  (wire (pts (xy 83.82 60.96) (xy 91.44 60.96))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 8237cd7a-5748-48a4-a358-abfdd1e1993e)
  )
  (wire (pts (xy 97.79 92.71) (xy 101.6 92.71))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid acb72e3b-4a91-4ccf-8f62-f4c015c0fbd9)
  )
  (wire (pts (xy 109.22 54.61) (xy 115.57 54.61))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid d7b0dea2-f8b7-4812-ab94-1e01fb755712)
  )
  (wire (pts (xy 83.82 57.15) (xy 91.44 57.15))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid dd82203b-1e1d-4d36-a17d-0a38ff651817)
  )
  (wire (pts (xy 95.25 77.47) (xy 97.79 77.47))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ff55bf9c-82ee-4699-af43-0b4a39a3c09b)
  )

  (hierarchical_label "+3V3" (shape input) (at 83.82 54.61 180)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid 022f79e9-008e-40b5-8692-c6bc4022a89b)
  )
  (hierarchical_label "+2V5_REF" (shape input) (at 83.82 57.15 180)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid 320ef64d-2b38-42f1-b75a-10ccb22cd9ca)
  )
  (hierarchical_label "GND" (shape input) (at 83.82 67.31 180)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid 663ef596-6d16-4f1e-9272-601261e11b84)
  )
  (hierarchical_label "+3V3" (shape input) (at 95.25 77.47 180)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid 7dc3edb1-6b21-4218-80cc-16bc8647f2bc)
  )
  (hierarchical_label "GAIN_CTRL" (shape output) (at 115.57 54.61 0)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid 81a73dae-a3ce-4b4e-b562-1aa875e51aab)
  )
  (hierarchical_label "GND" (shape input) (at 101.6 92.71 0)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid 87b66faa-72fe-4ceb-b7fc-fd8ff1f366da)
  )
  (hierarchical_label "I2C_SDA" (shape bidirectional) (at 83.82 60.96 180)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid 9ac6e32d-f34c-407f-9067-8ccdb425a9ee)
  )
  (hierarchical_label "I2C_SCL" (shape input) (at 83.82 63.5 180)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid a34c012d-3152-42a1-96cd-df014071b9f9)
  )

  (symbol (lib_id "Sonar:MCP4726") (at 100.33 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 040531cf-5466-4ca0-aa82-1c9a5b494328)
    (property "Reference" "U1001" (id 0) (at 100.33 38.1 0))
    (property "Value" "MCP4726" (id 1) (at 100.33 40.64 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (id 2) (at 99.06 73.66 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22272C.pdf" (id 3) (at 99.06 73.66 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MPN" "MCP4726A3T-E/CH" (id 4) (at 100.33 43.18 0))
    (property "Manufacturer" "Microchip Technology" (id 5) (at 100.33 45.72 0))
    (property "DPN" "MCP4726A3T-E/CHCT-ND" (id 6) (at 100.33 48.26 0))
    (property "Distributor" "DigiKey" (id 7) (at 100.33 50.8 0))
    (pin "1" (uuid 10b900a2-dd8a-460f-b992-ed11ff73e307))
    (pin "2" (uuid 940167cb-514b-42e1-97b7-21c2c94af37d))
    (pin "3" (uuid 079d3827-04f1-4f6b-a9a7-62e1c937bc35))
    (pin "4" (uuid a02a6697-b0e0-4992-9f2e-a72d3b460f14))
    (pin "5" (uuid 3b97eb30-dee1-473d-9b7e-49ca2c032876))
    (pin "6" (uuid 71a27d87-14d4-43d1-8393-7cab13148570))
  )

  (symbol (lib_id "Device:C_Small") (at 97.79 83.82 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid ac22bef0-2497-448e-a1d8-ea4f348d9dd1)
    (property "Reference" "C1001" (id 0) (at 100.33 82.5435 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "0u1" (id 1) (at 100.33 85.0835 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 97.79 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 97.79 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MPN" "CL10B104KB8NNWC" (id 4) (at 97.79 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Samsung Electro-Mechanics" (id 5) (at 97.79 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "DPN" "1276-1935-1-ND" (id 6) (at 97.79 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Distributor" "DigiKey" (id 7) (at 97.79 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid d5210051-ea67-4dad-8caa-3c1c0d05da0c))
    (pin "2" (uuid 96576bca-5310-49bb-8518-1b07daf50f5d))
  )
)
