(kicad_sch (version 20211123) (generator eeschema)

  (uuid 0df39628-7b95-439d-9ca6-7093c71d17f5)

  (paper "A4")

  (lib_symbols
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (stroke (width 0.3302) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (stroke (width 0.3048) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Sonar:AZ1117CH-3.3" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U?" (id 0) (at 0 7.62 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "AZ1117CH-3.3" (id 1) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "Package_TO_SOT_SMD:SOT-223" (id 2) (at 0 6.35 0)
        (effects (font (size 1.27 1.27) italic) hide)
      )
      (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 0 -20.32 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "MPN" "AZ1117CH-3.3TRG1" (id 4) (at 0 -20.32 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Manufacturer" "Diodes Incorporated" (id 5) (at 0 -20.32 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "DPN" "AZ1117CH-3.3TRG1DICT-ND" (id 6) (at 1.27 -20.32 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Distributor" "DigiKey" (id 7) (at 0 -20.32 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "Fixed Voltage Regulator 1A Positive LDO" (id 8) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "1A 20V Fixed LDO Linear Regulator, 3.3V, SOT-89/SOT-223/TO-220/TO-252/TO-263" (id 9) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "SOT?223* SOT?89* TO?220* TO?252* TO?263*" (id 10) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "AZ1117CH-3.3_0_1"
        (rectangle (start -5.08 1.905) (end 5.08 -5.08)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "AZ1117CH-3.3_1_1"
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin power_out line (at 7.62 0 180) (length 2.54) hide
          (name "VO" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
      )
    )
  )

  (junction (at 135.89 88.9) (diameter 0) (color 0 0 0 0)
    (uuid 5fd78558-7ba0-4459-9308-ffc8d0d3f62c)
  )
  (junction (at 143.51 78.74) (diameter 0) (color 0 0 0 0)
    (uuid 687eb8b4-30cd-452d-b80e-5841290d5bee)
  )
  (junction (at 125.73 88.9) (diameter 0) (color 0 0 0 0)
    (uuid 7da4e2d0-95e6-4acf-a308-17a73589a85d)
  )
  (junction (at 109.22 78.74) (diameter 0) (color 0 0 0 0)
    (uuid ad391f97-d13f-4818-9256-e60e2eb66a80)
  )
  (junction (at 135.89 78.74) (diameter 0) (color 0 0 0 0)
    (uuid fbe72edf-8986-4963-af67-75dfb3f0413e)
  )

  (wire (pts (xy 143.51 78.74) (xy 143.51 81.28))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 0625fd72-d280-447b-b97d-7a013686f1d7)
  )
  (wire (pts (xy 133.35 78.74) (xy 135.89 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 0e0028e5-4a5b-4abb-868d-b48b34b8f175)
  )
  (wire (pts (xy 104.14 78.74) (xy 109.22 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 132afb49-e385-4cc7-80ea-ae15e59ea2a5)
  )
  (wire (pts (xy 125.73 88.9) (xy 125.73 92.71))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 209f95e3-b8d9-4435-bf62-9b124f2b157a)
  )
  (wire (pts (xy 109.22 78.74) (xy 118.11 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 3bca5294-c6c3-4433-a922-0ad8f74c566f)
  )
  (wire (pts (xy 125.73 88.9) (xy 135.89 88.9))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 4c2e1233-b213-49c1-9a09-efce6fb2c010)
  )
  (wire (pts (xy 125.73 92.71) (xy 121.92 92.71))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 5dddbe13-34bc-485e-8dc5-b3d975cbf31e)
  )
  (wire (pts (xy 135.89 78.74) (xy 135.89 81.28))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 7b6eeaa1-5ab4-4b48-bd01-6fbcbf0a9445)
  )
  (wire (pts (xy 125.73 86.36) (xy 125.73 88.9))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a047f9f5-238b-4eb9-8100-936ecc658fd7)
  )
  (wire (pts (xy 109.22 88.9) (xy 125.73 88.9))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a04e084e-a54c-4043-b606-1b909a189f16)
  )
  (wire (pts (xy 143.51 86.36) (xy 143.51 88.9))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid b117a71b-10c4-43a6-aaf6-b97a4824464b)
  )
  (wire (pts (xy 135.89 88.9) (xy 143.51 88.9))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid b7e7705d-4a93-4186-9c10-92a6a3b19658)
  )
  (wire (pts (xy 135.89 78.74) (xy 143.51 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid d1bd11c9-a643-483e-aba1-5aa075b08d34)
  )
  (wire (pts (xy 109.22 86.36) (xy 109.22 88.9))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid dd328226-8583-4d8a-9bb9-81312dbe9892)
  )
  (wire (pts (xy 135.89 86.36) (xy 135.89 88.9))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ddcce2b9-034d-41f0-ae9a-de5ab8fc13a8)
  )
  (wire (pts (xy 109.22 81.28) (xy 109.22 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid f2ca549d-d156-47e6-8591-ef260f70e04b)
  )
  (wire (pts (xy 143.51 78.74) (xy 153.67 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid f3fe83b4-78c4-44fc-8583-d340ec359d94)
  )

  (text "Power Requirements:\n- 4x ADCs (22mA max * 4 = 88mA)\n- Gain DAC (xxmA, budget 50mA)\n- I2C pulldowns (worst case 2kOhm, ~4mA)\n- 2.5V Vref (capable of 20mA, so budget that)\n- Variable clock gen (20mA)\n\nThe Colorlight module takes 5V, so does not factor in.\n\nTotal requirements: 182mA at max, a 500mA reg is overkill,\nbut also provides a bit of headroom in case I forgot anything."
    (at 17.78 38.1 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 70c96b82-0607-4148-a5e8-a34064137031)
  )

  (hierarchical_label "+5V" (shape input) (at 104.14 78.74 180)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid 3f33bc5e-38b4-47e5-9112-7ccef6129463)
  )
  (hierarchical_label "+3V3" (shape output) (at 153.67 78.74 0)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid 99dac2b4-b217-4469-8cf3-c6117e955a04)
  )
  (hierarchical_label "GND" (shape input) (at 121.92 92.71 180)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid e8296b60-02a4-470f-a0b1-e7717b7f30ff)
  )

  (symbol (lib_id "Device:C_Small") (at 109.22 83.82 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 2561258a-f3b8-4968-bbf3-26c7aeaa6255)
    (property "Reference" "C801" (id 0) (at 111.76 82.5562 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "10u" (id 1) (at 111.76 85.0962 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 109.22 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 109.22 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MPN" "CL21B106KPQNNNE" (id 4) (at 109.22 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Samsung Electro-Mechanics" (id 5) (at 109.22 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "DPN" "1276-1764-1-ND" (id 6) (at 109.22 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Distributor" "DigiKey" (id 7) (at 109.22 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 05c74362-afad-4c61-a2dd-fac91b27bcac))
    (pin "2" (uuid 69bd5840-0ca1-409a-bc72-1c3269c148e8))
  )

  (symbol (lib_id "Device:C_Small") (at 135.89 83.82 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 2ee2debb-1030-44e6-b429-d5887bc5a696)
    (property "Reference" "C802" (id 0) (at 138.43 82.5562 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "10u" (id 1) (at 138.43 85.0962 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 135.89 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 135.89 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MPN" "CL21B106KPQNNNE" (id 4) (at 135.89 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Samsung Electro-Mechanics" (id 5) (at 135.89 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "DPN" "1276-1764-1-ND" (id 6) (at 135.89 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Distributor" "DigiKey" (id 7) (at 135.89 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid e745e009-3318-46da-b759-f71c7c11c6ff))
    (pin "2" (uuid cd649380-c910-40c0-97eb-24a647e68c3e))
  )

  (symbol (lib_id "Device:C_Small") (at 143.51 83.82 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 6f47a975-11fa-4196-bfc8-48ab9939c4e2)
    (property "Reference" "C803" (id 0) (at 146.05 82.5562 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "10u" (id 1) (at 146.05 85.0962 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 143.51 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 143.51 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MPN" "CL21B106KPQNNNE" (id 4) (at 143.51 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Samsung Electro-Mechanics" (id 5) (at 143.51 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "DPN" "1276-1764-1-ND" (id 6) (at 143.51 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Distributor" "DigiKey" (id 7) (at 143.51 83.82 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 0011ad76-5548-483c-ad5a-6e8639850f6c))
    (pin "2" (uuid b393899b-1351-4d59-9b0b-220a8c8fd866))
  )

  (symbol (lib_id "Sonar:AZ1117CH-3.3") (at 125.73 78.74 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid b00e0a47-5e60-420c-961c-271ec09e9a49)
    (property "Reference" "U801" (id 0) (at 125.73 71.12 0))
    (property "Value" "AZ1117CH-3.3" (id 1) (at 125.73 73.66 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-223" (id 2) (at 125.73 72.39 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf" (id 3) (at 125.73 99.06 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MPN" "AZ1117CH-3.3TRG1" (id 4) (at 125.73 99.06 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Diodes Incorporated" (id 5) (at 125.73 99.06 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "DPN" "AZ1117CH-3.3TRG1DICT-ND" (id 6) (at 127 99.06 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Distributor" "DigiKey" (id 7) (at 125.73 99.06 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 79886e25-11c3-4e17-a409-c8ebd150709b))
    (pin "2" (uuid 580c7b87-e660-45cf-bd80-9b773dc317f9))
    (pin "3" (uuid 02701791-b3de-455a-9aba-152b8b8f5eae))
    (pin "4" (uuid 6f9d16ea-db4b-461b-af5e-649d36349071))
  )
)
