(kicad_sch (version 20211123) (generator eeschema)

  (uuid 04b8236f-fb8d-4a35-830a-7a50e37b80a8)

  (paper "A4")

  (lib_symbols
    (symbol "Connector:Conn_ARM_JTAG_SWD_10" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -2.54 16.51 0)
        (effects (font (size 1.27 1.27)) (justify right))
      )
      (property "Value" "Conn_ARM_JTAG_SWD_10" (id 1) (at -2.54 13.97 0)
        (effects (font (size 1.27 1.27)) (justify right bottom))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf" (id 3) (at -8.89 -31.75 90)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "Cortex Debug Connector ARM SWD JTAG" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "PinHeader?2x05?P1.27mm*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Conn_ARM_JTAG_SWD_10_0_1"
        (rectangle (start -10.16 12.7) (end 10.16 -12.7)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
        (rectangle (start -2.794 -12.7) (end -2.286 -11.684)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -0.254 -12.7) (end 0.254 -11.684)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -0.254 12.7) (end 0.254 11.684)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start 9.144 2.286) (end 10.16 2.794)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start 10.16 -2.794) (end 9.144 -2.286)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start 10.16 -0.254) (end 9.144 0.254)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start 10.16 7.874) (end 9.144 7.366)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "Conn_ARM_JTAG_SWD_10_1_1"
        (rectangle (start 9.144 -5.334) (end 10.16 -4.826)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (pin power_in line (at 0 15.24 270) (length 2.54)
          (name "VTref" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin open_collector line (at 12.7 7.62 180) (length 2.54)
          (name "~{RESET}" (effects (font (size 1.27 1.27))))
          (number "10" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 0 180) (length 2.54)
          (name "SWDIO/TMS" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 0 -15.24 90) (length 2.54)
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at 12.7 2.54 180) (length 2.54)
          (name "SWDCLK/TCK" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -15.24 90) (length 2.54) hide
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 12.7 -2.54 180) (length 2.54)
          (name "SWO/TDO" (effects (font (size 1.27 1.27))))
          (number "6" (effects (font (size 1.27 1.27))))
        )
        (pin no_connect line (at -10.16 0 0) (length 2.54) hide
          (name "KEY" (effects (font (size 1.27 1.27))))
          (number "7" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at 12.7 -5.08 180) (length 2.54)
          (name "NC/TDI" (effects (font (size 1.27 1.27))))
          (number "8" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -2.54 -15.24 90) (length 2.54)
          (name "GNDDetect" (effects (font (size 1.27 1.27))))
          (number "9" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Connector_Generic:Conn_01x04" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Conn_01x04" (id 1) (at 0 -7.62 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "connector" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Conn_01x04_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start -1.27 3.81) (end 1.27 -6.35)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_2" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_3" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_4" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
      )
    )
  )

  (junction (at 118.11 59.69) (diameter 0) (color 0 0 0 0)
    (uuid 0117e167-9f59-4d45-bbfe-40a123cdbe32)
  )
  (junction (at 113.03 64.77) (diameter 0) (color 0 0 0 0)
    (uuid 2e29fa35-c85b-480e-a01c-ca05701dbdf1)
  )
  (junction (at 63.5 80.01) (diameter 0) (color 0 0 0 0)
    (uuid 34b4c5c4-f16f-4e64-b759-5193b2c4183d)
  )
  (junction (at 120.65 57.15) (diameter 0) (color 0 0 0 0)
    (uuid 792b9eb1-b8df-42de-a6f0-c84d4183d1fa)
  )
  (junction (at 115.57 62.23) (diameter 0) (color 0 0 0 0)
    (uuid 8676d3ad-2296-4530-96eb-7b6851282b01)
  )
  (junction (at 63.5 144.78) (diameter 0) (color 0 0 0 0)
    (uuid e9fc072c-612d-4235-8971-48eb082cbef4)
  )

  (no_connect (at 76.2 57.15) (uuid af1853a0-66ae-4e4d-9cb4-cfe01e312a13))

  (wire (pts (xy 113.03 64.77) (xy 113.03 86.36))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 1fa4dfec-3e8a-4d86-8c9c-f8cb79a19df7)
  )
  (wire (pts (xy 63.5 144.78) (xy 63.5 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 31de484b-c528-4a22-a66e-f9b647e59b7e)
  )
  (wire (pts (xy 113.03 86.36) (xy 123.19 86.36))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 34f13b72-6897-46e1-8dd0-358f3b550df7)
  )
  (wire (pts (xy 63.5 144.78) (xy 63.5 143.51))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 37f93dd9-fb56-4af2-b353-8b5639446c5e)
  )
  (wire (pts (xy 115.57 83.82) (xy 123.19 83.82))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 3d881d2c-0cbd-4015-9315-e1df979eb798)
  )
  (wire (pts (xy 113.03 64.77) (xy 123.19 64.77))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 45de3f58-101c-4c8d-ba6f-2a3fd2250a46)
  )
  (wire (pts (xy 93.98 59.69) (xy 118.11 59.69))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 51ccd695-606f-4f70-92ae-3c7592dfc323)
  )
  (wire (pts (xy 60.96 80.01) (xy 63.5 80.01))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 564567ef-760a-4478-8635-efd9f020dc44)
  )
  (wire (pts (xy 115.57 62.23) (xy 123.19 62.23))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 632fece3-e11f-41f1-9310-115f2b64dcad)
  )
  (wire (pts (xy 76.2 64.77) (xy 93.98 64.77))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 6379a010-ac62-4a2a-8fd7-e4f8f9c881c7)
  )
  (wire (pts (xy 96.52 69.85) (xy 96.52 62.23))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 77e4a41c-f383-449e-b4b3-3c8806f7faca)
  )
  (wire (pts (xy 63.5 110.49) (xy 63.5 113.03))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 7a159d88-d7f5-4b41-a0ff-6d7eca521a16)
  )
  (wire (pts (xy 63.5 46.99) (xy 63.5 49.53))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 7e4b75ec-9385-40f0-b172-b8279d107b3d)
  )
  (wire (pts (xy 93.98 64.77) (xy 93.98 59.69))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 8c8b301a-4b8a-453a-ae52-11815c83302d)
  )
  (wire (pts (xy 76.2 125.73) (xy 82.55 125.73))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 8dd8a249-5622-48de-97ef-c01d9b3b6f06)
  )
  (wire (pts (xy 76.2 133.35) (xy 82.55 133.35))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 9544c280-255b-4fe2-9c2f-3381f252f32a)
  )
  (wire (pts (xy 91.44 62.23) (xy 91.44 57.15))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 95a292dd-5460-4b3f-b5e2-d6db2d4f1b58)
  )
  (wire (pts (xy 118.11 59.69) (xy 123.19 59.69))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a01bbd41-52b9-43c4-a701-10d230a7a1f1)
  )
  (wire (pts (xy 91.44 57.15) (xy 120.65 57.15))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a0b129c3-e1dd-4f95-8f2d-8be4cee867df)
  )
  (wire (pts (xy 60.96 144.78) (xy 63.5 144.78))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a541b87b-fdd5-41f1-986c-d7b79eee1b92)
  )
  (wire (pts (xy 63.5 80.01) (xy 63.5 82.55))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a9d8239e-4fef-4d2c-baa3-5d84af0e7d91)
  )
  (wire (pts (xy 118.11 81.28) (xy 123.19 81.28))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid b2006e85-197d-4685-980c-0245795a5a13)
  )
  (wire (pts (xy 76.2 62.23) (xy 91.44 62.23))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid b7424066-8317-4f84-8c43-f71e7aa392c8)
  )
  (wire (pts (xy 96.52 62.23) (xy 115.57 62.23))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid b7e1b893-a515-4dc8-ae71-2dd6090aa421)
  )
  (wire (pts (xy 99.06 67.31) (xy 99.06 64.77))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid bdd91f1e-042e-4a2c-86c3-2a600dc2070c)
  )
  (wire (pts (xy 76.2 67.31) (xy 99.06 67.31))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid bf008795-0e52-4236-924f-f09baa858f54)
  )
  (wire (pts (xy 76.2 128.27) (xy 82.55 128.27))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid c47eda61-46f9-4b0d-a150-66adc375d914)
  )
  (wire (pts (xy 115.57 62.23) (xy 115.57 83.82))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ccccc6d8-2776-41fc-b0a8-0f9b9488e768)
  )
  (wire (pts (xy 76.2 130.81) (xy 82.55 130.81))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid cd047232-8e58-47fa-ae53-6f525678f0cb)
  )
  (wire (pts (xy 118.11 59.69) (xy 118.11 81.28))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid cd122421-2d9b-41a5-889f-c19f4f362d5a)
  )
  (wire (pts (xy 60.96 143.51) (xy 60.96 144.78))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid d54c99eb-8cac-4974-b3cb-aaf771006350)
  )
  (wire (pts (xy 76.2 69.85) (xy 96.52 69.85))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid d92233ca-ed6e-47af-b330-b515b9631435)
  )
  (wire (pts (xy 120.65 78.74) (xy 120.65 57.15))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid dc8e3615-61c6-4f86-b4d6-87856d3cbd51)
  )
  (wire (pts (xy 76.2 120.65) (xy 82.55 120.65))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ea7ff398-a82e-4f3c-a13e-5fa6e5b328ff)
  )
  (wire (pts (xy 120.65 57.15) (xy 123.19 57.15))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid fe91c08b-bb47-4a42-bb8d-6e5bdf3a1e71)
  )
  (wire (pts (xy 123.19 78.74) (xy 120.65 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ff2880b7-93bc-4eb7-89b9-84dfba5253bc)
  )
  (wire (pts (xy 99.06 64.77) (xy 113.03 64.77))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ff8e0256-1bde-4c6e-ae29-b58104a0822d)
  )

  (text "2.9mm from base of board to bottom (3.4mm - 1mm/2) for my ddr2 connectors\nthis roughly matches measurement"
    (at 158.75 72.39 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 087e6424-5b70-4c26-b70f-6064dc72f9b3)
  )
  (text "So pogo pins are 24.6mm away from left edge of shielding pad"
    (at 156.21 113.03 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 0899ea25-b815-4f1f-b3f5-bcdcc99ad78c)
  )
  (text "edge is 19mm from farthest metal bit on mount" (at 156.21 100.33 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 3d1ab502-2bd5-47d0-a363-9cec0e6777e3)
  )
  (text "Pogo Pins" (at 123.19 90.17 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 68218dd5-cb4c-4a24-ae09-690c6b53fe81)
  )
  (text "pogo pins are 11.4m in from the top edge" (at 156.21 115.57 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 72ce604b-3998-4f91-a7a1-fb04080ab9b1)
  )
  (text "Softcore JTAG connector" (at 50.8 102.87 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 78f15713-9aac-4cdd-a164-b94ae5cd06dd)
  )
  (text "On the dev board, the bottom of the board is ~2mm from the base board (if the pogo pins weren't mounted, i.e. pressed down)\n"
    (at 158.75 67.31 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 8891904e-1b89-4425-8fcb-42dc1e386c8b)
  )
  (text "First one is 9.4mm from edge\n" (at 157.48 95.25 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid a995a449-2a1d-4993-a88e-75e1c11457df)
  )
  (text "Pogo holes ~2mm from edge of colorlight\n" (at 154.94 91.44 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid b2c38e41-9a7c-4b2b-81de-b20fc7be1620)
  )
  (text "39.3 from edge of colorlight to back edge of plastic"
    (at 154.94 87.63 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid ba4da3ea-b8b6-4262-bc88-ae63685ac95c)
  )
  (text "These JTAG signals can be routed to arbitrary pads on\nthe FPGA."
    (at 78.74 140.97 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid bc7d7bf9-d2e1-4a6a-bfdf-a2422845eeeb)
  )
  (text "That protrusion is 21.45-13.85mm from the left edge of the DDR2 connector"
    (at 153.67 107.95 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid bca4706e-c4a8-4e38-bbf4-7e3db24ab4a3)
  )
  (text "Debug header:\nI need JTAG specifically and the\neasy options (f103, or ft2232h)\nwere out of stock, so I'll just use\nan external interface.\n\nMore flexible anyways."
    (at 57.15 38.1 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid deef9b6a-6f68-4ad6-b0d6-e7283c722a16)
  )
  (text "Extra port for if I need to break wires out." (at 106.68 49.53 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid e242c02d-bf66-48ed-92e2-a06e2b7bea4d)
  )

  (label "JTAG_TCK" (at 106.68 57.15 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 6073c16b-2217-40de-b5f7-42a39422db85)
  )
  (label "JTAG_TDI" (at 106.68 62.23 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid 699f6ad0-735a-48bb-96c1-f780c39ce3fa)
  )
  (label "JTAG_TDO" (at 106.68 64.77 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid a1538532-bbf5-4e82-9aae-91d400a626e2)
  )
  (label "JTAG_TMS" (at 106.68 59.69 0)
    (effects (font (size 1.27 1.27)) (justify left bottom))
    (uuid ecac5c2c-898c-47d2-a64e-88be2bbe4de6)
  )

  (hierarchical_label "MCU_TCK" (shape output) (at 82.55 125.73 0)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid 37ed457e-58b6-4661-8786-712397168e44)
  )
  (hierarchical_label "MCU_TMS" (shape output) (at 82.55 128.27 0)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid 5a336b05-5f98-465f-83bf-20cd908b2918)
  )
  (hierarchical_label "MCU_TDI" (shape output) (at 82.55 133.35 0)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid 6bba9b9e-a72c-4a66-92a4-9358a254b970)
  )
  (hierarchical_label "3V3" (shape input) (at 63.5 46.99 90)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid 718ea906-f469-403d-90f6-a6ac99c25672)
  )
  (hierarchical_label "3V3" (shape input) (at 63.5 110.49 90)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid 8065db69-9a66-480e-9ae5-5f34c5293774)
  )
  (hierarchical_label "MCU_TDO" (shape output) (at 82.55 130.81 0)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid 84e3283e-9135-4034-aab8-33de72dcb59e)
  )
  (hierarchical_label "GND" (shape input) (at 63.5 82.55 270)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid 8ef3dd55-4502-4b0b-a76e-e91b04d2ce03)
  )
  (hierarchical_label "MCU_NRST" (shape output) (at 82.55 120.65 0)
    (effects (font (size 1.27 1.27)) (justify left))
    (uuid a1e95bff-3bd1-46a5-9bcc-e6b84076a6b8)
  )
  (hierarchical_label "GND" (shape input) (at 63.5 147.32 270)
    (effects (font (size 1.27 1.27)) (justify right))
    (uuid f8979292-7825-4bfc-8056-13a4720e59f7)
  )

  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 128.27 62.23 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 2989b849-eb12-461f-8b71-efb6ebd31bcc)
    (property "Reference" "J701" (id 0) (at 128.27 50.8 0))
    (property "Value" "Conn_01x04" (id 1) (at 128.27 53.34 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (id 2) (at 128.27 62.23 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 128.27 62.23 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 15555486-baf7-4de1-86fe-965aa0ea14fe))
    (pin "2" (uuid fd522e67-647b-4d63-a62c-02c61b1c8213))
    (pin "3" (uuid f6941599-702b-4e75-84fd-090df8125dbe))
    (pin "4" (uuid c2a7a1ae-7bc5-4148-84a9-324d3abc325f))
  )

  (symbol (lib_id "Connector:Conn_ARM_JTAG_SWD_10") (at 63.5 64.77 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 5ce54914-beb9-4764-b31a-c87cec5510f6)
    (property "Reference" "J702" (id 0) (at 52.07 63.4999 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "Conn_ARM_JTAG_SWD_10" (id 1) (at 52.07 66.0399 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD" (id 2) (at 63.5 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf" (id 3) (at 54.61 96.52 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MPN" "FTSH-105-01-L-DV-007" (id 4) (at 63.5 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Samtec Inc." (id 5) (at 63.5 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "DPN" "SAM15641-ND" (id 6) (at 63.5 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Distributor" "DigiKey" (id 7) (at 63.5 64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid e33ad571-0ced-4ee4-a116-7acd8cb8b62c))
    (pin "10" (uuid 8a6322e5-2aa8-458e-ab8e-a40c23e996d4))
    (pin "2" (uuid 648f2be3-9a85-40fa-916d-1180f0276792))
    (pin "3" (uuid 4abd5a54-0360-4cb4-af45-b1c3252a5259))
    (pin "4" (uuid f0ef2e2d-786d-4e25-90f2-1c6f0ef44d67))
    (pin "5" (uuid 06059569-0986-4ece-93b0-c7454401b9d8))
    (pin "6" (uuid a510c4ff-6517-473e-a609-0fd0bf0271d9))
    (pin "7" (uuid 93653086-8a87-4a8c-9520-9017ddc73117))
    (pin "8" (uuid 516861a0-5dfe-4b91-838b-def8e8d591f8))
    (pin "9" (uuid 519eeafc-8f63-4057-9f2f-deb5cd7ebb1c))
  )

  (symbol (lib_id "Connector:Conn_ARM_JTAG_SWD_10") (at 63.5 128.27 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 7acb08c2-0db6-46fc-9a6c-778590288e27)
    (property "Reference" "J704" (id 0) (at 52.07 126.9999 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "Conn_ARM_JTAG_SWD_10" (id 1) (at 52.07 129.5399 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD" (id 2) (at 63.5 128.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf" (id 3) (at 54.61 160.02 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MPN" "FTSH-105-01-L-DV-007" (id 4) (at 63.5 128.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Samtec Inc." (id 5) (at 63.5 128.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "DPN" "SAM15641-ND" (id 6) (at 63.5 128.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Distributor" "DigiKey" (id 7) (at 63.5 128.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid c014cfbb-4857-4c69-bb25-f3273b5e55b5))
    (pin "10" (uuid 29faaa0b-74a5-42b7-863b-73c8ec1e7c60))
    (pin "2" (uuid 6eaed2cf-b89f-4c89-9ecf-ad4ea3785eb6))
    (pin "3" (uuid ccae10d4-016d-412a-9c47-30220802a773))
    (pin "4" (uuid afcb577b-e29e-45da-93c7-2ffed9943488))
    (pin "5" (uuid 07070cf9-cc76-42a5-8c96-80e1f4db5fd4))
    (pin "6" (uuid 18a77d56-81b9-44a0-827c-38341acf3a71))
    (pin "7" (uuid 811ebfa1-0a1c-493c-aa2c-906958ee73d5))
    (pin "8" (uuid 20bd780a-bcc8-45e6-be2f-d577eec8e0c4))
    (pin "9" (uuid 6e053fbe-59c5-4b97-ad47-78a25d2cc885))
  )

  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 128.27 83.82 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 7f8edd22-a7b9-4a63-992a-ab2da8333b82)
    (property "Reference" "J703" (id 0) (at 128.27 72.39 0))
    (property "Value" "Conn_01x04" (id 1) (at 128.27 74.93 0))
    (property "Footprint" "Sonar:PogoPin_0906-0-15-20-76-14-11-0" (id 2) (at 128.27 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Mill%20Max%20PDFs/Spring%20Loaded%20Connectors.pdf" (id 3) (at 128.27 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MPN" "0906-0-15-20-76-14-11-0" (id 4) (at 128.27 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Mill-Max Manufacturing Corp." (id 5) (at 128.27 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "DPN" "ED8180-ND" (id 6) (at 128.27 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Distributor" "DigiKey" (id 7) (at 128.27 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 4ca1ff71-0c64-4cf2-a34c-1ba6292e9918))
    (pin "2" (uuid f70a6eb3-9d93-49ba-bbb2-bd0a2a4f802e))
    (pin "3" (uuid 5f66c307-db6c-4687-b89a-f7af9b0a836a))
    (pin "4" (uuid bb1f6c43-5696-4609-8cb6-c442fdf7c6f6))
  )
)
